Steps taken to evaluate wolfSSL with the following:

Required Software for this guide:
IAR Embedded Workbench IDE - ARM v7.60.1 (or similar version)
embOS v4.16 (for Cortex-M and IAR compiler)
wolfssl (latest version)

Required items (Hardware) for this guide:
Atmel SAM V71 Xplained Ultra (Or equivelent Cortex-M Evaluation Board)
    Note: Must have J-Trace adapter (SWD or SWD + ETM)
j-Trace for ARM Cortex-M Processors
    Note: You can see here: https://www.segger.com/j-trace-for-cortex-m.html
    Note: You can also purchase other models, we used one from IAR v3.2
20 pin target ribbon cable
USB Cable with j-Trace adapter end
Micro usb cable

#--!! NOTE !!--#
For this guide "**SAMV71_DIR" will signify the directory:
C:\<path-to>\wolfssl\IDE\IAR-EWARM\embOS\SAMV71_XULT\


#----------------------------------------------------------------------------#
# Create wolfcrypt_lib.a
#----------------------------------------------------------------------------#

1. Open IAR Workbench -> Project -> Add Existing Project
    a. Browse to **SAMV71_DIR\embOS_wolfcrypt_lib
    c. Choose wolfcrypt_lib.ewp and click "Open"

2. Go to Project -> Rebuild All

3. Verify the library built, you should now have:
    **SAMV71_DIR\embOS_wolfcrypt_lib\Debug\Bin\wolfcrypt_lib.a

#----------------------------------------------------------------------------#
#----------------------------------------------------------------------------#

Thank you for using this guide and we hope this was helpful to you. If you have
any suggestions / feedback for us please contact us:
support@wolfssl.com
info@wolfssl.com

Copyright © 2016 wolfSSL Inc.  All rights reserved.