From 014b05aea0dafeee16d23444f3a7cb9889f21836 Mon Sep 17 00:00:00 2001
From: Felix Fietkau <nbd@openwrt.org>
Date: Sat, 4 Aug 2007 11:58:31 +0000
Subject: fix a few overfull hboxes, remove some redundant stuff

SVN-Revision: 8341
---
 docs/adding.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'docs/adding.tex')

diff --git a/docs/adding.tex b/docs/adding.tex
index b1712ac9d2..2b47e6a328 100644
--- a/docs/adding.tex
+++ b/docs/adding.tex
@@ -357,7 +357,7 @@ firmware image and flash is structured. You will find below a commented example
 that covers the case of the device where the bootloader can pass to the kernel its partition plan.
 
 First of all, you need to make your flash map driver be visible in the kernel 
-configuration options, this can be done by editing the file 
+configuration options, this can be done by editing the file \
 \textbf{linux/drivers/mtd/maps/Kconfig}:
 
 \begin{verbatim}
-- 
cgit v1.2.3

