From 773c31afdcd77564d10cc7b622344d0eb8884758 Mon Sep 17 00:00:00 2001
From: Florian Fainelli <florian@openwrt.org>
Date: Fri, 26 Oct 2007 16:21:03 +0000
Subject: Document the IPv6 connectivity with OpenWrt.

SVN-Revision: 9452
---
 docs/wireless.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'docs/wireless.tex')

diff --git a/docs/wireless.tex b/docs/wireless.tex
index 5734fc093b..7e96239722 100644
--- a/docs/wireless.tex
+++ b/docs/wireless.tex
@@ -7,7 +7,7 @@ Each wireless driver has its own configuration script in \texttt{/lib/wifi/drive
 driver specific options and configurations. This script is also calling driver specific binaries like wlc for
 Broadcom, or hostapd and wpa\_supplicant for atheros.
 
-The reason for using such architecture, is that it abstracts the driver configuration 
+The reason for using such architecture, is that it abstracts the driver configuration. 
 
 \paragraph{Generic Broadcom wireless config:}
 
-- 
cgit v1.2.3

