From 48acfc25685a902044f7d3d3ace86a1e0b7bc66d Mon Sep 17 00:00:00 2001
From: Felix Fietkau <nbd@openwrt.org>
Date: Sat, 4 Aug 2007 11:58:31 +0000
Subject: fix a few overfull hboxes, remove some redundant stuff

git-svn-id: svn://svn.openwrt.org/openwrt/trunk@8341 3c298f89-4303-0410-b956-a3cf2f4a3e73
---
 docs/adding.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'docs/adding.tex')

diff --git a/docs/adding.tex b/docs/adding.tex
index b1712ac9d2..2b47e6a328 100644
--- a/docs/adding.tex
+++ b/docs/adding.tex
@@ -357,7 +357,7 @@ firmware image and flash is structured. You will find below a commented example
 that covers the case of the device where the bootloader can pass to the kernel its partition plan.
 
 First of all, you need to make your flash map driver be visible in the kernel 
-configuration options, this can be done by editing the file 
+configuration options, this can be done by editing the file \
 \textbf{linux/drivers/mtd/maps/Kconfig}:
 
 \begin{verbatim}
-- 
cgit v1.2.3

