='generator' content='cgit v1.2.3'/>
<meta name='robots' content='index, nofollow'/>
<link rel='stylesheet' type='text/css' href='/cgit.css'/>
<link rel='shortcut icon' href='/favicon.ico'/>
<link rel='alternate' title='Atom feed' href='https://openwrt.panaceas.org/cgit/xen/xen/atom/xen/drivers/net/e1000/e1000_hw.c?h=master' type='application/atom+xml'/>
<link rel='vcs-git' href='git://git.panaceas.org/xen/xen' title='xen/xen Git repository'/>
<link rel='vcs-git' href='ssh://git@git.panaceas.org/git/xen/xen' title='xen/xen Git repository'/>
</head>
<body>
<div id='cgit'><table id='header'>
<tr>
<td class='logo' rowspan='2'><a href='/cgit/'><img src='/cgit.png' alt='cgit logo'/></a></td>
<td class='main'><a href='/cgit/'>index</a> : <a title='xen/xen' href='/cgit/xen/xen/'>xen/xen</a></td><td class='form'><form method='get'>
<input type='hidden' name='id' value='2c6f432e14345aacd41430870a7fc7fc68f8f8a2'/><select name='h' onchange='this.form.submit();'>
<option value='master' selected='selected'>master</option>
<option value='stable-4.0'>stable-4.0</option>
<option value='stable-4.1'>stable-4.1</option>
<option value='stable-4.2'>stable-4.2</option>
<option value='stable-4.3'>stable-4.3</option>
<option value='staging'>staging</option>
<option value='staging-4.0'>staging-4.0</option>
<option value='staging-4.1'>staging-4.1</option>
<option value='staging-4.2'>staging-4.2</option>
<option value='staging-4.3'>staging-4.3</option>
</select> <input type='submit' value='switch'/></form></td></tr>
<tr><td class='sub'>xen</td><td class='sub right'>James</td></tr></table>
<table class='tabs'><tr><td>
<a href='/cgit/xen/xen/about/'>about</a><a href='/cgit/xen/xen/'>summary</a><a href='/cgit/xen/xen/refs/?id=2c6f432e14345aacd41430870a7fc7fc68f8f8a2'>refs</a><a href='/cgit/xen/xen/log/xen/drivers/net/e1000/e1000_hw.c'>log</a><a class='active' href='/cgit/xen/xen/tree/xen/drivers/net/e1000/e1000_hw.c?id=2c6f432e14345aacd41430870a7fc7fc68f8f8a2'>tree</a><a href='/cgit/xen/xen/commit/xen/drivers/net/e1000/e1000_hw.c?id=2c6f432e14345aacd41430870a7fc7fc68f8f8a2'>commit</a><a href='/cgit/xen/xen/diff/xen/drivers/net/e1000/e1000_hw.c?id=2c6f432e14345aacd41430870a7fc7fc68f8f8a2'>diff</a><a href='/cgit/xen/xen/stats/xen/drivers/net/e1000/e1000_hw.c'>stats</a></td><td class='form'><form class='right' method='get' action='/cgit/xen/xen/log/xen/drivers/net/e1000/e1000_hw.c'>
<input type='hidden' name='id' value='2c6f432e14345aacd41430870a7fc7fc68f8f8a2'/><select name='qt'>
<option value='grep'>log msg</option>
<option value='author'>author</option>
<option value='committer'>committer</option>
<option value='range'>range</option>
</select>
<input class='txt' type='search' size='10' name='q' value=''/>
<input type='submit' value='search'/>
</form>
</td></tr></table>
<div class='path'>path: <a href='/cgit/xen/xen/tree/?id=2c6f432e14345aacd41430870a7fc7fc68f8f8a2'>root</a>/<a href='/cgit/xen/xen/tree/xen?id=2c6f432e14345aacd41430870a7fc7fc68f8f8a2'>xen</a>/<a href='/cgit/xen/xen/tree/xen/drivers?id=2c6f432e14345aacd41430870a7fc7fc68f8f8a2'>drivers</a>/<a href='/cgit/xen/xen/tree/xen/drivers/net?id=2c6f432e14345aacd41430870a7fc7fc68f8f8a2'>net</a>/<a href='/cgit/xen/xen/tree/xen/drivers/net/e1000?id=2c6f432e14345aacd41430870a7fc7fc68f8f8a2'>e1000</a>/<a href='/cgit/xen/xen/tree/xen/drivers/net/e1000/e1000_hw.c?id=2c6f432e14345aacd41430870a7fc7fc68f8f8a2'>e1000_hw.c</a></div><div class='content'>blob: 1d70dab9371dc6d0a23d7c67a6332ca7d205f9fb (<a href='/cgit/xen/xen/plain/xen/drivers/net/e1000/e1000_hw.c?id=2c6f432e14345aacd41430870a7fc7fc68f8f8a2'>plain</a>)
<table summary='blob content' class='blob'>
<tr><td class='linenumbers'><pre><a id='n1' href='#n1'>1</a>
<a id='n2' href='#n2'>2</a>
<a id='n3' href='#n3'>3</a>
<a id='n4' href='#n4'>4</a>
<a id='n5' href='#n5'>5</a>
<a id='n6' href='#n6'>6</a>
<a id='n7' href='#n7'>7</a>
<a id='n8' href='#n8'>8</a>
<a id='n9' href='#n9'>9</a>
<a id='n10' href='#n10'>10</a>
<a id='n11' href='#n11'>11</a>
<a id='n12' href='#n12'>12</a>
<a id='n13' href='#n13'>13</a>
<a id='n14' href='#n14'>14</a>
<a id='n15' href='#n15'>15</a>
<a id='n16' href='#n16'>16</a>
<a id='n17' href='#n17'>17</a>
<a id='n18' href='#n18'>18</a>
<a id='n19' href='#n19'>19</a>
<a id='n20' href='#n20'>20</a>
<a id='n21' href='#n21'>21</a>
<a id='n22' href='#n22'>22</a>
<a id='n23' href='#n23'>23</a>
<a id='n24' href='#n24'>24</a>
<a id='n25' href='#n25'>25</a>
<a id='n26' href='#n26'>26</a>
<a id='n27' href='#n27'>27</a>
<a id='n28' href='#n28'>28</a>
<a id='n29' href='#n29'>29</a>
<a id='n30' href='#n30'>30</a>
<a id='n31' href='#n31'>31</a>
<a id='n32' href='#n32'>32</a>
<a id='n33' href='#n33'>33</a>
<a id='n34' href='#n34'>34</a>
<a id='n35' href='#n35'>35</a>
<a id='n36' href='#n36'>36</a>
<a id='n37' href='#n37'>37</a>
<a id='n38' href='#n38'>38</a>
<a id='n39' href='#n39'>39</a>
<a id='n40' href='#n40'>40</a>
<a id='n41' href='#n41'>41</a>
<a id='n42' href='#n42'>42</a>
<a id='n43' href='#n43'>43</a>
<a id='n44' href='#n44'>44</a>
<a id='n45' href='#n45'>45</a>
<a id='n46' href='#n46'>46</a>
<a id='n47' href='#n47'>47</a>
<a id='n48' href='#n48'>48</a>
<a id='n49' href='#n49'>49</a>
<a id='n50' href='#n50'>50</a>
<a id='n51' href='#n51'>51</a>
<a id='n52' href='#n52'>52</a>
<a id='n53' href='#n53'>53</a>
<a id='n54' href='#n54'>54</a>
<a id='n55' href='#n55'>55</a>
<a id='n56' href='#n56'>56</a>
<a id='n57' href='#n57'>57</a>
<a id='n58' href='#n58'>58</a>
<a id='n59' href='#n59'>59</a>
<a id='n60' href='#n60'>60</a>
<a id='n61' href='#n61'>61</a>
<a id='n62' href='#n62'>62</a>
<a id='n63' href='#n63'>63</a>
<a id='n64' href='#n64'>64</a>
<a id='n65' href='#n65'>65</a>
<a id='n66' href='#n66'>66</a>
<a id='n67' href='#n67'>67</a>
<a id='n68' href='#n68'>68</a>
<a id='n69' href='#n69'>69</a>
<a id='n70' href='#n70'>70</a>
<a id='n71' href='#n71'>71</a>
<a id='n72' href='#n72'>72</a>
<a id='n73' href='#n73'>73</a>
<a id='n74' href='#n74'>74</a>
<a id='n75' href='#n75'>75</a>
<a id='n76' href='#n76'>76</a>
<a id='n77' href='#n77'>77</a>
<a id='n78' href='#n78'>78</a>
<a id='n79' href='#n79'>79</a>
<a id='n80' href='#n80'>80</a>
<a id='n81' href='#n81'>81</a>
<a id='n82' href='#n82'>82</a>
<a id='n83' href='#n83'>83</a>
<a id='n84' href='#n84'>84</a>
<a id='n85' href='#n85'>85</a>
<a id='n86' href='#n86'>86</a>
<a id='n87' href='#n87'>87</a>
<a id='n88' href='#n88'>88</a>
<a id='n89' href='#n89'>89</a>
<a id='n90' href='#n90'>90</a>
<a id='n91' href='#n91'>91</a>
<a id='n92' href='#n92'>92</a>
<a id='n93' href='#n93'>93</a>
<a id='n94' href='#n94'>94</a>
<a id='n95' href='#n95'>95</a>
<a id='n96' href='#n96'>96</a>
<a id='n97' href='#n97'>97</a>
<a id='n98' href='#n98'>98</a>
<a id='n99' href='#n99'>99</a>
<a id='n100' href='#n100'>100</a>
<a id='n101' href='#n101'>101</a>
<a id='n102' href='#n102'>102</a>
<a id='n103' href='#n103'>103</a>
<a id='n104' href='#n104'>104</a>
<a id='n105' href='#n105'>105</a>
<a id='n106' href='#n106'>106</a>
<a id='n107' href='#n107'>107</a>
<a id='n108' href='#n108'>108</a>
<a id='n109' href='#n109'>109</a>
<a id='n110' href='#n110'>110</a>
<a id='n111' href='#n111'>111</a>
<a id='n112' href='#n112'>112</a>
<a id='n113' href='#n113'>113</a>
<a id='n114' href='#n114'>114</a>
<a id='n115' href='#n115'>115</a>
<a id='n116' href='#n116'>116</a>
<a id='n117' href='#n117'>117</a>
<a id='n118' href='#n118'>118</a>
<a id='n119' href='#n119'>119</a>
<a id='n120' href='#n120'>120</a>
<a id='n121' href='#n121'>121</a>
<a id='n122' href='#n122'>122</a>
<a id='n123' href='#n123'>123</a>
<a id='n124' href='#n124'>124</a>
<a id='n125' href='#n125'>125</a>
<a id='n126' href='#n126'>126</a>
<a id='n127' href='#n127'>127</a>
<a id='n128' href='#n128'>128</a>
<a id='n129' href='#n129'>129</a>
<a id='n130' href='#n130'>130</a>
<a id='n131' href='#n131'>131</a>
<a id='n132' href='#n132'>132</a>
<a id='n133' href='#n133'>133</a>
<a id='n134' href='#n134'>134</a>
<a id='n135' href='#n135'>135</a>
<a id='n136' href='#n136'>136</a>
<a id='n137' href='#n137'>137</a>
<a id='n138' href='#n138'>138</a>
<a id='n139' href='#n139'>139</a>
<a id='n140' href='#n140'>140</a>
<a id='n141' href='#n141'>141</a>
<a id='n142' href='#n142'>142</a>
<a id='n143' href='#n143'>143</a>
<a id='n144' href='#n144'>144</a>
<a id='n145' href='#n145'>145</a>
<a id='n146' href='#n146'>146</a>
<a id='n147' href='#n147'>147</a>
<a id='n148' href='#n148'>148</a>
<a id='n149' href='#n149'>149</a>
<a id='n150' href='#n150'>150</a>
<a id='n151' href='#n151'>151</a>
<a id='n152' href='#n152'>152</a>
<a id='n153' href='#n153'>153</a>
<a id='n154' href='#n154'>154</a>
<a id='n155' href='#n155'>155</a>
<a id='n156' href='#n156'>156</a>
<a id='n157' href='#n157'>157</a>
<a id='n158' href='#n158'>158</a>
<a id='n159' href='#n159'>159</a>
<a id='n160' href='#n160'>160</a>
<a id='n161' href='#n161'>161</a>
<a id='n162' href='#n162'>162</a>
<a id='n163' href='#n163'>163</a>
<a id='n164' href='#n164'>164</a>
<a id='n165' href='#n165'>165</a>
<a id='n166' href='#n166'>166</a>
<a id='n167' href='#n167'>167</a>
<a id='n168' href='#n168'>168</a>
<a id='n169' href='#n169'>169</a>
<a id='n170' href='#n170'>170</a>
<a id='n171' href='#n171'>171</a>
<a id='n172' href='#n172'>172</a>
<a id='n173' href='#n173'>173</a>
<a id='n174' href='#n174'>174</a>
<a id='n175' href='#n175'>175</a>
<a id='n176' href='#n176'>176</a>
<a id='n177' href='#n177'>177</a>
<a id='n178' href='#n178'>178</a>
<a id='n179' href='#n179'>179</a>
<a id='n180' href='#n180'>180</a>
<a id='n181' href='#n181'>181</a>
<a id='n182' href='#n182'>182</a>
<a id='n183' href='#n183'>183</a>
<a id='n184' href='#n184'>184</a>
<a id='n185' href='#n185'>185</a>
<a id='n186' href='#n186'>186</a>
<a id='n187' href='#n187'>187</a>
<a id='n188' href='#n188'>188</a>
<a id='n189' href='#n189'>189</a>
<a id='n190' href='#n190'>190</a>
<a id='n191' href='#n191'>191</a>
<a id='n192' href='#n192'>192</a>
<a id='n193' href='#n193'>193</a>
<a id='n194' href='#n194'>194</a>
<a id='n195' href='#n195'>195</a>
<a id='n196' href='#n196'>196</a>
<a id='n197' href='#n197'>197</a>
<a id='n198' href='#n198'>198</a>
<a id='n199' href='#n199'>199</a>
<a id='n200' href='#n200'>200</a>
<a id='n201' href='#n201'>201</a>
<a id='n202' href='#n202'>202</a>
<a id='n203' href='#n203'>203</a>
<a id='n204' href='#n204'>204</a>
<a id='n205' href='#n205'>205</a>
<a id='n206' href='#n206'>206</a>
<a id='n207' href='#n207'>207</a>
<a id='n208' href='#n208'>208</a>
<a id='n209' href='#n209'>209</a>
<a id='n210' href='#n210'>210</a>
<a id='n211' href='#n211'>211</a>
<a id='n212' href='#n212'>212</a>
<a id='n213' href='#n213'>213</a>
<a id='n214' href='#n214'>214</a>
<a id='n215' href='#n215'>215</a>
<a id='n216' href='#n216'>216</a>
<a id='n217' href='#n217'>217</a>
<a id='n218' href='#n218'>218</a>
<a id='n219' href='#n219'>219</a>
<a id='n220' href='#n220'>220</a>
<a id='n221' href='#n221'>221</a>
<a id='n222' href='#n222'>222</a>
<a id='n223' href='#n223'>223</a>
<a id='n224' href='#n224'>224</a>
<a id='n225' href='#n225'>225</a>
<a id='n226' href='#n226'>226</a>
<a id='n227' href='#n227'>227</a>
<a id='n228' href='#n228'>228</a>
<a id='n229' href='#n229'>229</a>
<a id='n230' href='#n230'>230</a>
<a id='n231' href='#n231'>231</a>
<a id='n232' href='#n232'>232</a>
<a id='n233' href='#n233'>233</a>
<a id='n234' href='#n234'>234</a>
<a id='n235' href='#n235'>235</a>
<a id='n236' href='#n236'>236</a>
<a id='n237' href='#n237'>237</a>
<a id='n238' href='#n238'>238</a>
<a id='n239' href='#n239'>239</a>
<a id='n240' href='#n240'>240</a>
<a id='n241' href='#n241'>241</a>
<a id='n242' href='#n242'>242</a>
<a id='n243' href='#n243'>243</a>
<a id='n244' href='#n244'>244</a>
<a id='n245' href='#n245'>245</a>
<a id='n246' href='#n246'>246</a>
<a id='n247' href='#n247'>247</a>
<a id='n248' href='#n248'>248</a>
<a id='n249' href='#n249'>249</a>
<a id='n250' href='#n250'>250</a>
<a id='n251' href='#n251'>251</a>
<a id='n252' href='#n252'>252</a>
<a id='n253' href='#n253'>253</a>
<a id='n254' href='#n254'>254</a>
<a id='n255' href='#n255'>255</a>
<a id='n256' href='#n256'>256</a>
<a id='n257' href='#n257'>257</a>
<a id='n258' href='#n258'>258</a>
<a id='n259' href='#n259'>259</a>
<a id='n260' href='#n260'>260</a>
<a id='n261' href='#n261'>261</a>
<a id='n262' href='#n262'>262</a>
<a id='n263' href='#n263'>263</a>
<a id='n264' href='#n264'>264</a>
<a id='n265' href='#n265'>265</a>
<a id='n266' href='#n266'>266</a>
<a id='n267' href='#n267'>267</a>
<a id='n268' href='#n268'>268</a>
<a id='n269' href='#n269'>269</a>
<a id='n270' href='#n270'>270</a>
<a id='n271' href='#n271'>271</a>
<a id='n272' href='#n272'>272</a>
<a id='n273' href='#n273'>273</a>
<a id='n274' href='#n274'>274</a>
<a id='n275' href='#n275'>275</a>
<a id='n276' href='#n276'>276</a>
<a id='n277' href='#n277'>277</a>
<a id='n278' href='#n278'>278</a>
<a id='n279' href='#n279'>279</a>
<a id='n280' href='#n280'>280</a>
<a id='n281' href='#n281'>281</a>
<a id='n282' href='#n282'>282</a>
<a id='n283' href='#n283'>283</a>
<a id='n284' href='#n284'>284</a>
<a id='n285' href='#n285'>285</a>
<a id='n286' href='#n286'>286</a>
<a id='n287' href='#n287'>287</a>
<a id='n288' href='#n288'>288</a>
<a id='n289' href='#n289'>289</a>
<a id='n290' href='#n290'>290</a>
<a id='n291' href='#n291'>291</a>
<a id='n292' href='#n292'>292</a>
<a id='n293' href='#n293'>293</a>
<a id='n294' href='#n294'>294</a>
<a id='n295' href='#n295'>295</a>
<a id='n296' href='#n296'>296</a>
<a id='n297' href='#n297'>297</a>
<a id='n298' href='#n298'>298</a>
<a id='n299' href='#n299'>299</a>
<a id='n300' href='#n300'>300</a>
<a id='n301' href='#n301'>301</a>
<a id='n302' href='#n302'>302</a>
<a id='n303' href='#n303'>303</a>
<a id='n304' href='#n304'>304</a>
<a id='n305' href='#n305'>305</a>
<a id='n306' href='#n306'>306</a>
<a id='n307' href='#n307'>307</a>
<a id='n308' href='#n308'>308</a>
<a id='n309' href='#n309'>309</a>
<a id='n310' href='#n310'>310</a>
<a id='n311' href='#n311'>311</a>
<a id='n312' href='#n312'>312</a>
<a id='n313' href='#n313'>313</a>
<a id='n314' href='#n314'>314</a>
<a id='n315' href='#n315'>315</a>
<a id='n316' href='#n316'>316</a>
<a id='n317' href='#n317'>317</a>
<a id='n318' href='#n318'>318</a>
<a id='n319' href='#n319'>319</a>
<a id='n320' href='#n320'>320</a>
<a id='n321' href='#n321'>321</a>
<a id='n322' href='#n322'>322</a>
<a id='n323' href='#n323'>323</a>
<a id='n324' href='#n324'>324</a>
<a id='n325' href='#n325'>325</a>
<a id='n326' href='#n326'>326</a>
<a id='n327' href='#n327'>327</a>
<a id='n328' href='#n328'>328</a>
<a id='n329' href='#n329'>329</a>
<a id='n330' href='#n330'>330</a>
<a id='n331' href='#n331'>331</a>
<a id='n332' href='#n332'>332</a>
<a id='n333' href='#n333'>333</a>
<a id='n334' href='#n334'>334</a>
<a id='n335' href='#n335'>335</a>
<a id='n336' href='#n336'>336</a>
<a id='n337' href='#n337'>337</a>
<a id='n338' href='#n338'>338</a>
<a id='n339' href='#n339'>339</a>
<a id='n340' href='#n340'>340</a>
<a id='n341' href='#n341'>341</a>
<a id='n342' href='#n342'>342</a>
<a id='n343' href='#n343'>343</a>
<a id='n344' href='#n344'>344</a>
<a id='n345' href='#n345'>345</a>
<a id='n346' href='#n346'>346</a>
<a id='n347' href='#n347'>347</a>
<a id='n348' href='#n348'>348</a>
<a id='n349' href='#n349'>349</a>
<a id='n350' href='#n350'>350</a>
<a id='n351' href='#n351'>351</a>
<a id='n352' href='#n352'>352</a>
<a id='n353' href='#n353'>353</a>
<a id='n354' href='#n354'>354</a>
<a id='n355' href='#n355'>355</a>
<a id='n356' href='#n356'>356</a>
<a id='n357' href='#n357'>357</a>
<a id='n358' href='#n358'>358</a>
<a id='n359' href='#n359'>359</a>
<a id='n360' href='#n360'>360</a>
<a id='n361' href='#n361'>361</a>
<a id='n362' href='#n362'>362</a>
<a id='n363' href='#n363'>363</a>
<a id='n364' href='#n364'>364</a>
<a id='n365' href='#n365'>365</a>
<a id='n366' href='#n366'>366</a>
<a id='n367' href='#n367'>367</a>
<a id='n368' href='#n368'>368</a>
<a id='n369' href='#n369'>369</a>
<a id='n370' href='#n370'>370</a>
<a id='n371' href='#n371'>371</a>
<a id='n372' href='#n372'>372</a>
<a id='n373' href='#n373'>373</a>
<a id='n374' href='#n374'>374</a>
<a id='n375' href='#n375'>375</a>
<a id='n376' href='#n376'>376</a>
<a id='n377' href='#n377'>377</a>
<a id='n378' href='#n378'>378</a>
<a id='n379' href='#n379'>379</a>
<a id='n380' href='#n380'>380</a>
<a id='n381' href='#n381'>381</a>
<a id='n382' href='#n382'>382</a>
<a id='n383' href='#n383'>383</a>
<a id='n384' href='#n384'>384</a>
<a id='n385' href='#n385'>385</a>
<a id='n386' href='#n386'>386</a>
<a id='n387' href='#n387'>387</a>
<a id='n388' href='#n388'>388</a>
<a id='n389' href='#n389'>389</a>
<a id='n390' href='#n390'>390</a>
<a id='n391' href='#n391'>391</a>
<a id='n392' href='#n392'>392</a>
<a id='n393' href='#n393'>393</a>
<a id='n394' href='#n394'>394</a>
<a id='n395' href='#n395'>395</a>
<a id='n396' href='#n396'>396</a>
<a id='n397' href='#n397'>397</a>
<a id='n398' href='#n398'>398</a>
<a id='n399' href='#n399'>399</a>
<a id='n400' href='#n400'>400</a>
<a id='n401' href='#n401'>401</a>
<a id='n402' href='#n402'>402</a>
<a id='n403' href='#n403'>403</a>
<a id='n404' href='#n404'>404</a>
<a id='n405' href='#n405'>405</a>
<a id='n406' href='#n406'>406</a>
<a id='n407' href='#n407'>407</a>
<a id='n408' href='#n408'>408</a>
<a id='n409' href='#n409'>409</a>
<a id='n410' href='#n410'>410</a>
<a id='n411' href='#n411'>411</a>
<a id='n412' href='#n412'>412</a>
<a id='n413' href='#n413'>413</a>
<a id='n414' href='#n414'>414</a>
<a id='n415' href='#n415'>415</a>
<a id='n416' href='#n416'>416</a>
<a id='n417' href='#n417'>417</a>
<a id='n418' href='#n418'>418</a>
<a id='n419' href='#n419'>419</a>
<a id='n420' href='#n420'>420</a>
<a id='n421' href='#n421'>421</a>
<a id='n422' href='#n422'>422</a>
<a id='n423' href='#n423'>423</a>
<a id='n424' href='#n424'>424</a>
<a id='n425' href='#n425'>425</a>
<a id='n426' href='#n426'>426</a>
<a id='n427' href='#n427'>427</a>
<a id='n428' href='#n428'>428</a>
<a id='n429' href='#n429'>429</a>
<a id='n430' href='#n430'>430</a>
<a id='n431' href='#n431'>431</a>
<a id='n432' href='#n432'>432</a>
<a id='n433' href='#n433'>433</a>
<a id='n434' href='#n434'>434</a>
<a id='n435' href='#n435'>435</a>
<a id='n436' href='#n436'>436</a>
<a id='n437' href='#n437'>437</a>
<a id='n438' href='#n438'>438</a>
<a id='n439' href='#n439'>439</a>
<a id='n440' href='#n440'>440</a>
<a id='n441' href='#n441'>441</a>
<a id='n442' href='#n442'>442</a>
<a id='n443' href='#n443'>443</a>
<a id='n444' href='#n444'>444</a>
<a id='n445' href='#n445'>445</a>
<a id='n446' href='#n446'>446</a>
<a id='n447' href='#n447'>447</a>
<a id='n448' href='#n448'>448</a>
<a id='n449' href='#n449'>449</a>
<a id='n450' href='#n450'>450</a>
<a id='n451' href='#n451'>451</a>
<a id='n452' href='#n452'>452</a>
<a id='n453' href='#n453'>453</a>
<a id='n454' href='#n454'>454</a>
<a id='n455' href='#n455'>455</a>
<a id='n456' href='#n456'>456</a>
<a id='n457' href='#n457'>457</a>
<a id='n458' href='#n458'>458</a>
<a id='n459' href='#n459'>459</a>
<a id='n460' href='#n460'>460</a>
<a id='n461' href='#n461'>461</a>
<a id='n462' href='#n462'>462</a>
<a id='n463' href='#n463'>463</a>
<a id='n464' href='#n464'>464</a>
<a id='n465' href='#n465'>465</a>
<a id='n466' href='#n466'>466</a>
<a id='n467' href='#n467'>467</a>
<a id='n468' href='#n468'>468</a>
<a id='n469' href='#n469'>469</a>
<a id='n470' href='#n470'>470</a>
<a id='n471' href='#n471'>471</a>
<a id='n472' href='#n472'>472</a>
<a id='n473' href='#n473'>473</a>
<a id='n474' href='#n474'>474</a>
<a id='n475' href='#n475'>475</a>
<a id='n476' href='#n476'>476</a>
<a id='n477' href='#n477'>477</a>
<a id='n478' href='#n478'>478</a>
<a id='n479' href='#n479'>479</a>
<a id='n480' href='#n480'>480</a>
<a id='n481' href='#n481'>481</a>
<a id='n482' href='#n482'>482</a>
<a id='n483' href='#n483'>483</a>
<a id='n484' href='#n484'>484</a>
<a id='n485' href='#n485'>485</a>
<a id='n486' href='#n486'>486</a>
<a id='n487' href='#n487'>487</a>
<a id='n488' href='#n488'>488</a>
<a id='n489' href='#n489'>489</a>
<a id='n490' href='#n490'>490</a>
<a id='n491' href='#n491'>491</a>
<a id='n492' href='#n492'>492</a>
<a id='n493' href='#n493'>493</a>
<a id='n494' href='#n494'>494</a>
<a id='n495' href='#n495'>495</a>
<a id='n496' href='#n496'>496</a>
<a id='n497' href='#n497'>497</a>
<a id='n498' href='#n498'>498</a>
<a id='n499' href='#n499'>499</a>
<a id='n500' href='#n500'>500</a>
<a id='n501' href='#n501'>501</a>
<a id='n502' href='#n502'>502</a>
<a id='n503' href='#n503'>503</a>
<a id='n504' href='#n504'>504</a>
<a id='n505' href='#n505'>505</a>
<a id='n506' href='#n506'>506</a>
<a id='n507' href='#n507'>507</a>
<a id='n508' href='#n508'>508</a>
<a id='n509' href='#n509'>509</a>
<a id='n510' href='#n510'>510</a>
<a id='n511' href='#n511'>511</a>
<a id='n512' href='#n512'>512</a>
<a id='n513' href='#n513'>513</a>
<a id='n514' href='#n514'>514</a>
<a id='n515' href='#n515'>515</a>
<a id='n516' href='#n516'>516</a>
<a id='n517' href='#n517'>517</a>
<a id='n518' href='#n518'>518</a>
<a id='n519' href='#n519'>519</a>
<a id='n520' href='#n520'>520</a>
<a id='n521' href='#n521'>521</a>
<a id='n522' href='#n522'>522</a>
<a id='n523' href='#n523'>523</a>
<a id='n524' href='#n524'>524</a>
<a id='n525' href='#n525'>525</a>
<a id='n526' href='#n526'>526</a>
<a id='n527' href='#n527'>527</a>
<a id='n528' href='#n528'>528</a>
<a id='n529' href='#n529'>529</a>
<a id='n530' href='#n530'>530</a>
<a id='n531' href='#n531'>531</a>
<a id='n532' href='#n532'>532</a>
<a id='n533' href='#n533'>533</a>
<a id='n534' href='#n534'>534</a>
<a id='n535' href='#n535'>535</a>
<a id='n536' href='#n536'>536</a>
<a id='n537' href='#n537'>537</a>
<a id='n538' href='#n538'>538</a>
<a id='n539' href='#n539'>539</a>
<a id='n540' href='#n540'>540</a>
<a id='n541' href='#n541'>541</a>
<a id='n542' href='#n542'>542</a>
<a id='n543' href='#n543'>543</a>
<a id='n544' href='#n544'>544</a>
<a id='n545' href='#n545'>545</a>
<a id='n546' href='#n546'>546</a>
<a id='n547' href='#n547'>547</a>
<a id='n548' href='#n548'>548</a>
<a id='n549' href='#n549'>549</a>
<a id='n550' href='#n550'>550</a>
<a id='n551' href='#n551'>551</a>
<a id='n552' href='#n552'>552</a>
<a id='n553' href='#n553'>553</a>
<a id='n554' href='#n554'>554</a>
<a id='n555' href='#n555'>555</a>
<a id='n556' href='#n556'>556</a>
<a id='n557' href='#n557'>557</a>
<a id='n558' href='#n558'>558</a>
<a id='n559' href='#n559'>559</a>
<a id='n560' href='#n560'>560</a>
<a id='n561' href='#n561'>561</a>
<a id='n562' href='#n562'>562</a>
<a id='n563' href='#n563'>563</a>
<a id='n564' href='#n564'>564</a>
<a id='n565' href='#n565'>565</a>
<a id='n566' href='#n566'>566</a>
<a id='n567' href='#n567'>567</a>
<a id='n568' href='#n568'>568</a>
<a id='n569' href='#n569'>569</a>
<a id='n570' href='#n570'>570</a>
<a id='n571' href='#n571'>571</a>
<a id='n572' href='#n572'>572</a>
<a id='n573' href='#n573'>573</a>
<a id='n574' href='#n574'>574</a>
<a id='n575' href='#n575'>575</a>
<a id='n576' href='#n576'>576</a>
<a id='n577' href='#n577'>577</a>
<a id='n578' href='#n578'>578</a>
<a id='n579' href='#n579'>579</a>
<a id='n580' href='#n580'>580</a>
<a id='n581' href='#n581'>581</a>
<a id='n582' href='#n582'>582</a>
<a id='n583' href='#n583'>583</a>
<a id='n584' href='#n584'>584</a>
<a id='n585' href='#n585'>585</a>
<a id='n586' href='#n586'>586</a>
<a id='n587' href='#n587'>587</a>
<a id='n588' href='#n588'>588</a>
<a id='n589' href='#n589'>589</a>
<a id='n590' href='#n590'>590</a>
<a id='n591' href='#n591'>591</a>
<a id='n592' href='#n592'>592</a>
<a id='n593' href='#n593'>593</a>
<a id='n594' href='#n594'>594</a>
<a id='n595' href='#n595'>595</a>
<a id='n596' href='#n596'>596</a>
<a id='n597' href='#n597'>597</a>
<a id='n598' href='#n598'>598</a>
<a id='n599' href='#n599'>599</a>
<a id='n600' href='#n600'>600</a>
<a id='n601' href='#n601'>601</a>
<a id='n602' href='#n602'>602</a>
<a id='n603' href='#n603'>603</a>
<a id='n604' href='#n604'>604</a>
<a id='n605' href='#n605'>605</a>
<a id='n606' href='#n606'>606</a>
<a id='n607' href='#n607'>607</a>
<a id='n608' href='#n608'>608</a>
<a id='n609' href='#n609'>609</a>
<a id='n610' href='#n610'>610</a>
<a id='n611' href='#n611'>611</a>
<a id='n612' href='#n612'>612</a>
<a id='n613' href='#n613'>613</a>
<a id='n614' href='#n614'>614</a>
<a id='n615' href='#n615'>615</a>
<a id='n616' href='#n616'>616</a>
<a id='n617' href='#n617'>617</a>
<a id='n618' href='#n618'>618</a>
<a id='n619' href='#n619'>619</a>
<a id='n620' href='#n620'>620</a>
<a id='n621' href='#n621'>621</a>
<a id='n622' href='#n622'>622</a>
<a id='n623' href='#n623'>623</a>
<a id='n624' href='#n624'>624</a>
<a id='n625' href='#n625'>625</a>
<a id='n626' href='#n626'>626</a>
<a id='n627' href='#n627'>627</a>
<a id='n628' href='#n628'>628</a>
<a id='n629' href='#n629'>629</a>
<a id='n630' href='#n630'>630</a>
<a id='n631' href='#n631'>631</a>
<a id='n632' href='#n632'>632</a>
<a id='n633' href='#n633'>633</a>
<a id='n634' href='#n634'>634</a>
<a id='n635' href='#n635'>635</a>
<a id='n636' href='#n636'>636</a>
<a id='n637' href='#n637'>637</a>
<a id='n638' href='#n638'>638</a>
<a id='n639' href='#n639'>639</a>
<a id='n640' href='#n640'>640</a>
<a id='n641' href='#n641'>641</a>
<a id='n642' href='#n642'>642</a>
<a id='n643' href='#n643'>643</a>
<a id='n644' href='#n644'>644</a>
<a id='n645' href='#n645'>645</a>
<a id='n646' href='#n646'>646</a>
<a id='n647' href='#n647'>647</a>
<a id='n648' href='#n648'>648</a>
<a id='n649' href='#n649'>649</a>
<a id='n650' href='#n650'>650</a>
<a id='n651' href='#n651'>651</a>
<a id='n652' href='#n652'>652</a>
<a id='n653' href='#n653'>653</a>
<a id='n654' href='#n654'>654</a>
<a id='n655' href='#n655'>655</a>
<a id='n656' href='#n656'>656</a>
<a id='n657' href='#n657'>657</a>
<a id='n658' href='#n658'>658</a>
<a id='n659' href='#n659'>659</a>
<a id='n660' href='#n660'>660</a>
<a id='n661' href='#n661'>661</a>
<a id='n662' href='#n662'>662</a>
<a id='n663' href='#n663'>663</a>
<a id='n664' href='#n664'>664</a>
<a id='n665' href='#n665'>665</a>
<a id='n666' href='#n666'>666</a>
<a id='n667' href='#n667'>667</a>
<a id='n668' href='#n668'>668</a>
<a id='n669' href='#n669'>669</a>
<a id='n670' href='#n670'>670</a>
<a id='n671' href='#n671'>671</a>
<a id='n672' href='#n672'>672</a>
<a id='n673' href='#n673'>673</a>
<a id='n674' href='#n674'>674</a>
<a id='n675' href='#n675'>675</a>
<a id='n676' href='#n676'>676</a>
<a id='n677' href='#n677'>677</a>
<a id='n678' href='#n678'>678</a>
<a id='n679' href='#n679'>679</a>
<a id='n680' href='#n680'>680</a>
<a id='n681' href='#n681'>681</a>
<a id='n682' href='#n682'>682</a>
<a id='n683' href='#n683'>683</a>
<a id='n684' href='#n684'>684</a>
<a id='n685' href='#n685'>685</a>
<a id='n686' href='#n686'>686</a>
<a id='n687' href='#n687'>687</a>
<a id='n688' href='#n688'>688</a>
<a id='n689' href='#n689'>689</a>
<a id='n690' href='#n690'>690</a>
<a id='n691' href='#n691'>691</a>
<a id='n692' href='#n692'>692</a>
<a id='n693' href='#n693'>693</a>
<a id='n694' href='#n694'>694</a>
<a id='n695' href='#n695'>695</a>
<a id='n696' href='#n696'>696</a>
<a id='n697' href='#n697'>697</a>
<a id='n698' href='#n698'>698</a>
<a id='n699' href='#n699'>699</a>
<a id='n700' href='#n700'>700</a>
<a id='n701' href='#n701'>701</a>
<a id='n702' href='#n702'>702</a>
<a id='n703' href='#n703'>703</a>
<a id='n704' href='#n704'>704</a>
<a id='n705' href='#n705'>705</a>
<a id='n706' href='#n706'>706</a>
<a id='n707' href='#n707'>707</a>
<a id='n708' href='#n708'>708</a>
<a id='n709' href='#n709'>709</a>
<a id='n710' href='#n710'>710</a>
<a id='n711' href='#n711'>711</a>
<a id='n712' href='#n712'>712</a>
<a id='n713' href='#n713'>713</a>
<a id='n714' href='#n714'>714</a>
<a id='n715' href='#n715'>715</a>
<a id='n716' href='#n716'>716</a>
<a id='n717' href='#n717'>717</a>
<a id='n718' href='#n718'>718</a>
<a id='n719' href='#n719'>719</a>
<a id='n720' href='#n720'>720</a>
<a id='n721' href='#n721'>721</a>
<a id='n722' href='#n722'>722</a>
<a id='n723' href='#n723'>723</a>
<a id='n724' href='#n724'>724</a>
<a id='n725' href='#n725'>725</a>
<a id='n726' href='#n726'>726</a>
<a id='n727' href='#n727'>727</a>
<a id='n728' href='#n728'>728</a>
<a id='n729' href='#n729'>729</a>
<a id='n730' href='#n730'>730</a>
<a id='n731' href='#n731'>731</a>
<a id='n732' href='#n732'>732</a>
<a id='n733' href='#n733'>733</a>
<a id='n734' href='#n734'>734</a>
<a id='n735' href='#n735'>735</a>
<a id='n736' href='#n736'>736</a>
<a id='n737' href='#n737'>737</a>
<a id='n738' href='#n738'>738</a>
<a id='n739' href='#n739'>739</a>
<a id='n740' href='#n740'>740</a>
<a id='n741' href='#n741'>741</a>
<a id='n742' href='#n742'>742</a>
<a id='n743' href='#n743'>743</a>
<a id='n744' href='#n744'>744</a>
<a id='n745' href='#n745'>745</a>
<a id='n746' href='#n746'>746</a>
<a id='n747' href='#n747'>747</a>
<a id='n748' href='#n748'>748</a>
<a id='n749' href='#n749'>749</a>
<a id='n750' href='#n750'>750</a>
<a id='n751' href='#n751'>751</a>
<a id='n752' href='#n752'>752</a>
<a id='n753' href='#n753'>753</a>
<a id='n754' href='#n754'>754</a>
<a id='n755' href='#n755'>755</a>
<a id='n756' href='#n756'>756</a>
<a id='n757' href='#n757'>757</a>
<a id='n758' href='#n758'>758</a>
<a id='n759' href='#n759'>759</a>
<a id='n760' href='#n760'>760</a>
<a id='n761' href='#n761'>761</a>
<a id='n762' href='#n762'>762</a>
<a id='n763' href='#n763'>763</a>
<a id='n764' href='#n764'>764</a>
<a id='n765' href='#n765'>765</a>
<a id='n766' href='#n766'>766</a>
<a id='n767' href='#n767'>767</a>
<a id='n768' href='#n768'>768</a>
<a id='n769' href='#n769'>769</a>
<a id='n770' href='#n770'>770</a>
<a id='n771' href='#n771'>771</a>
<a id='n772' href='#n772'>772</a>
<a id='n773' href='#n773'>773</a>
<a id='n774' href='#n774'>774</a>
<a id='n775' href='#n775'>775</a>
<a id='n776' href='#n776'>776</a>
<a id='n777' href='#n777'>777</a>
<a id='n778' href='#n778'>778</a>
<a id='n779' href='#n779'>779</a>
<a id='n780' href='#n780'>780</a>
<a id='n781' href='#n781'>781</a>
<a id='n782' href='#n782'>782</a>
<a id='n783' href='#n783'>783</a>
<a id='n784' href='#n784'>784</a>
<a id='n785' href='#n785'>785</a>
<a id='n786' href='#n786'>786</a>
<a id='n787' href='#n787'>787</a>
<a id='n788' href='#n788'>788</a>
<a id='n789' href='#n789'>789</a>
<a id='n790' href='#n790'>790</a>
<a id='n791' href='#n791'>791</a>
<a id='n792' href='#n792'>792</a>
<a id='n793' href='#n793'>793</a>
<a id='n794' href='#n794'>794</a>
<a id='n795' href='#n795'>795</a>
<a id='n796' href='#n796'>796</a>
<a id='n797' href='#n797'>797</a>
<a id='n798' href='#n798'>798</a>
<a id='n799' href='#n799'>799</a>
<a id='n800' href='#n800'>800</a>
<a id='n801' href='#n801'>801</a>
<a id='n802' href='#n802'>802</a>
<a id='n803' href='#n803'>803</a>
<a id='n804' href='#n804'>804</a>
<a id='n805' href='#n805'>805</a>
<a id='n806' href='#n806'>806</a>
<a id='n807' href='#n807'>807</a>
<a id='n808' href='#n808'>808</a>
<a id='n809' href='#n809'>809</a>
<a id='n810' href='#n810'>810</a>
<a id='n811' href='#n811'>811</a>
<a id='n812' href='#n812'>812</a>
<a id='n813' href='#n813'>813</a>
<a id='n814' href='#n814'>814</a>
<a id='n815' href='#n815'>815</a>
<a id='n816' href='#n816'>816</a>
<a id='n817' href='#n817'>817</a>
<a id='n818' href='#n818'>818</a>
<a id='n819' href='#n819'>819</a>
<a id='n820' href='#n820'>820</a>
<a id='n821' href='#n821'>821</a>
<a id='n822' href='#n822'>822</a>
<a id='n823' href='#n823'>823</a>
<a id='n824' href='#n824'>824</a>
<a id='n825' href='#n825'>825</a>
<a id='n826' href='#n826'>826</a>
<a id='n827' href='#n827'>827</a>
<a id='n828' href='#n828'>828</a>
<a id='n829' href='#n829'>829</a>
<a id='n830' href='#n830'>830</a>
<a id='n831' href='#n831'>831</a>
<a id='n832' href='#n832'>832</a>
<a id='n833' href='#n833'>833</a>
<a id='n834' href='#n834'>834</a>
<a id='n835' href='#n835'>835</a>
<a id='n836' href='#n836'>836</a>
<a id='n837' href='#n837'>837</a>
<a id='n838' href='#n838'>838</a>
<a id='n839' href='#n839'>839</a>
<a id='n840' href='#n840'>840</a>
<a id='n841' href='#n841'>841</a>
<a id='n842' href='#n842'>842</a>
<a id='n843' href='#n843'>843</a>
<a id='n844' href='#n844'>844</a>
<a id='n845' href='#n845'>845</a>
<a id='n846' href='#n846'>846</a>
<a id='n847' href='#n847'>847</a>
<a id='n848' href='#n848'>848</a>
<a id='n849' href='#n849'>849</a>
<a id='n850' href='#n850'>850</a>
<a id='n851' href='#n851'>851</a>
<a id='n852' href='#n852'>852</a>
<a id='n853' href='#n853'>853</a>
<a id='n854' href='#n854'>854</a>
<a id='n855' href='#n855'>855</a>
<a id='n856' href='#n856'>856</a>
<a id='n857' href='#n857'>857</a>
<a id='n858' href='#n858'>858</a>
<a id='n859' href='#n859'>859</a>
<a id='n860' href='#n860'>860</a>
<a id='n861' href='#n861'>861</a>
<a id='n862' href='#n862'>862</a>
<a id='n863' href='#n863'>863</a>
<a id='n864' href='#n864'>864</a>
<a id='n865' href='#n865'>865</a>
<a id='n866' href='#n866'>866</a>
<a id='n867' href='#n867'>867</a>
<a id='n868' href='#n868'>868</a>
<a id='n869' href='#n869'>869</a>
<a id='n870' href='#n870'>870</a>
<a id='n871' href='#n871'>871</a>
<a id='n872' href='#n872'>872</a>
<a id='n873' href='#n873'>873</a>
<a id='n874' href='#n874'>874</a>
<a id='n875' href='#n875'>875</a>
<a id='n876' href='#n876'>876</a>
<a id='n877' href='#n877'>877</a>
<a id='n878' href='#n878'>878</a>
<a id='n879' href='#n879'>879</a>
<a id='n880' href='#n880'>880</a>
<a id='n881' href='#n881'>881</a>
<a id='n882' href='#n882'>882</a>
<a id='n883' href='#n883'>883</a>
<a id='n884' href='#n884'>884</a>
<a id='n885' href='#n885'>885</a>
<a id='n886' href='#n886'>886</a>
<a id='n887' href='#n887'>887</a>
<a id='n888' href='#n888'>888</a>
<a id='n889' href='#n889'>889</a>
<a id='n890' href='#n890'>890</a>
<a id='n891' href='#n891'>891</a>
<a id='n892' href='#n892'>892</a>
<a id='n893' href='#n893'>893</a>
<a id='n894' href='#n894'>894</a>
<a id='n895' href='#n895'>895</a>
<a id='n896' href='#n896'>896</a>
<a id='n897' href='#n897'>897</a>
<a id='n898' href='#n898'>898</a>
<a id='n899' href='#n899'>899</a>
<a id='n900' href='#n900'>900</a>
<a id='n901' href='#n901'>901</a>
<a id='n902' href='#n902'>902</a>
<a id='n903' href='#n903'>903</a>
<a id='n904' href='#n904'>904</a>
<a id='n905' href='#n905'>905</a>
<a id='n906' href='#n906'>906</a>
<a id='n907' href='#n907'>907</a>
<a id='n908' href='#n908'>908</a>
<a id='n909' href='#n909'>909</a>
<a id='n910' href='#n910'>910</a>
<a id='n911' href='#n911'>911</a>
<a id='n912' href='#n912'>912</a>
<a id='n913' href='#n913'>913</a>
<a id='n914' href='#n914'>914</a>
<a id='n915' href='#n915'>915</a>
<a id='n916' href='#n916'>916</a>
<a id='n917' href='#n917'>917</a>
<a id='n918' href='#n918'>918</a>
<a id='n919' href='#n919'>919</a>
<a id='n920' href='#n920'>920</a>
<a id='n921' href='#n921'>921</a>
<a id='n922' href='#n922'>922</a>
<a id='n923' href='#n923'>923</a>
<a id='n924' href='#n924'>924</a>
<a id='n925' href='#n925'>925</a>
<a id='n926' href='#n926'>926</a>
<a id='n927' href='#n927'>927</a>
<a id='n928' href='#n928'>928</a>
<a id='n929' href='#n929'>929</a>
<a id='n930' href='#n930'>930</a>
<a id='n931' href='#n931'>931</a>
<a id='n932' href='#n932'>932</a>
<a id='n933' href='#n933'>933</a>
<a id='n934' href='#n934'>934</a>
<a id='n935' href='#n935'>935</a>
<a id='n936' href='#n936'>936</a>
<a id='n937' href='#n937'>937</a>
<a id='n938' href='#n938'>938</a>
<a id='n939' href='#n939'>939</a>
<a id='n940' href='#n940'>940</a>
<a id='n941' href='#n941'>941</a>
<a id='n942' href='#n942'>942</a>
<a id='n943' href='#n943'>943</a>
<a id='n944' href='#n944'>944</a>
<a id='n945' href='#n945'>945</a>
<a id='n946' href='#n946'>946</a>
<a id='n947' href='#n947'>947</a>
<a id='n948' href='#n948'>948</a>
<a id='n949' href='#n949'>949</a>
<a id='n950' href='#n950'>950</a>
<a id='n951' href='#n951'>951</a>
<a id='n952' href='#n952'>952</a>
<a id='n953' href='#n953'>953</a>
<a id='n954' href='#n954'>954</a>
<a id='n955' href='#n955'>955</a>
<a id='n956' href='#n956'>956</a>
<a id='n957' href='#n957'>957</a>
<a id='n958' href='#n958'>958</a>
<a id='n959' href='#n959'>959</a>
<a id='n960' href='#n960'>960</a>
<a id='n961' href='#n961'>961</a>
<a id='n962' href='#n962'>962</a>
<a id='n963' href='#n963'>963</a>
<a id='n964' href='#n964'>964</a>
<a id='n965' href='#n965'>965</a>
<a id='n966' href='#n966'>966</a>
<a id='n967' href='#n967'>967</a>
<a id='n968' href='#n968'>968</a>
<a id='n969' href='#n969'>969</a>
<a id='n970' href='#n970'>970</a>
<a id='n971' href='#n971'>971</a>
<a id='n972' href='#n972'>972</a>
<a id='n973' href='#n973'>973</a>
<a id='n974' href='#n974'>974</a>
<a id='n975' href='#n975'>975</a>
<a id='n976' href='#n976'>976</a>
<a id='n977' href='#n977'>977</a>
<a id='n978' href='#n978'>978</a>
<a id='n979' href='#n979'>979</a>
<a id='n980' href='#n980'>980</a>
<a id='n981' href='#n981'>981</a>
<a id='n982' href='#n982'>982</a>
<a id='n983' href='#n983'>983</a>
<a id='n984' href='#n984'>984</a>
<a id='n985' href='#n985'>985</a>
<a id='n986' href='#n986'>986</a>
<a id='n987' href='#n987'>987</a>
<a id='n988' href='#n988'>988</a>
<a id='n989' href='#n989'>989</a>
<a id='n990' href='#n990'>990</a>
<a id='n991' href='#n991'>991</a>
<a id='n992' href='#n992'>992</a>
<a id='n993' href='#n993'>993</a>
<a id='n994' href='#n994'>994</a>
<a id='n995' href='#n995'>995</a>
<a id='n996' href='#n996'>996</a>
<a id='n997' href='#n997'>997</a>
<a id='n998' href='#n998'>998</a>
<a id='n999' href='#n999'>999</a>
<a id='n1000' href='#n1000'>1000</a>
<a id='n1001' href='#n1001'>1001</a>
<a id='n1002' href='#n1002'>1002</a>
<a id='n1003' href='#n1003'>1003</a>
<a id='n1004' href='#n1004'>1004</a>
<a id='n1005' href='#n1005'>1005</a>
<a id='n1006' href='#n1006'>1006</a>
<a id='n1007' href='#n1007'>1007</a>
<a id='n1008' href='#n1008'>1008</a>
<a id='n1009' href='#n1009'>1009</a>
<a id='n1010' href='#n1010'>1010</a>
<a id='n1011' href='#n1011'>1011</a>
<a id='n1012' href='#n1012'>1012</a>
<a id='n1013' href='#n1013'>1013</a>
<a id='n1014' href='#n1014'>1014</a>
<a id='n1015' href='#n1015'>1015</a>
<a id='n1016' href='#n1016'>1016</a>
<a id='n1017' href='#n1017'>1017</a>
<a id='n1018' href='#n1018'>1018</a>
<a id='n1019' href='#n1019'>1019</a>
<a id='n1020' href='#n1020'>1020</a>
<a id='n1021' href='#n1021'>1021</a>
<a id='n1022' href='#n1022'>1022</a>
<a id='n1023' href='#n1023'>1023</a>
<a id='n1024' href='#n1024'>1024</a>
<a id='n1025' href='#n1025'>1025</a>
<a id='n1026' href='#n1026'>1026</a>
<a id='n1027' href='#n1027'>1027</a>
<a id='n1028' href='#n1028'>1028</a>
<a id='n1029' href='#n1029'>1029</a>
<a id='n1030' href='#n1030'>1030</a>
<a id='n1031' href='#n1031'>1031</a>
<a id='n1032' href='#n1032'>1032</a>
<a id='n1033' href='#n1033'>1033</a>
<a id='n1034' href='#n1034'>1034</a>
<a id='n1035' href='#n1035'>1035</a>
<a id='n1036' href='#n1036'>1036</a>
<a id='n1037' href='#n1037'>1037</a>
<a id='n1038' href='#n1038'>1038</a>
<a id='n1039' href='#n1039'>1039</a>
<a id='n1040' href='#n1040'>1040</a>
<a id='n1041' href='#n1041'>1041</a>
<a id='n1042' href='#n1042'>1042</a>
<a id='n1043' href='#n1043'>1043</a>
<a id='n1044' href='#n1044'>1044</a>
<a id='n1045' href='#n1045'>1045</a>
<a id='n1046' href='#n1046'>1046</a>
<a id='n1047' href='#n1047'>1047</a>
<a id='n1048' href='#n1048'>1048</a>
<a id='n1049' href='#n1049'>1049</a>
<a id='n1050' href='#n1050'>1050</a>
<a id='n1051' href='#n1051'>1051</a>
<a id='n1052' href='#n1052'>1052</a>
<a id='n1053' href='#n1053'>1053</a>
<a id='n1054' href='#n1054'>1054</a>
<a id='n1055' href='#n1055'>1055</a>
<a id='n1056' href='#n1056'>1056</a>
<a id='n1057' href='#n1057'>1057</a>
<a id='n1058' href='#n1058'>1058</a>
<a id='n1059' href='#n1059'>1059</a>
<a id='n1060' href='#n1060'>1060</a>
<a id='n1061' href='#n1061'>1061</a>
<a id='n1062' href='#n1062'>1062</a>
<a id='n1063' href='#n1063'>1063</a>
<a id='n1064' href='#n1064'>1064</a>
<a id='n1065' href='#n1065'>1065</a>
<a id='n1066' href='#n1066'>1066</a>
<a id='n1067' href='#n1067'>1067</a>
<a id='n1068' href='#n1068'>1068</a>
<a id='n1069' href='#n1069'>1069</a>
<a id='n1070' href='#n1070'>1070</a>
<a id='n1071' href='#n1071'>1071</a>
<a id='n1072' href='#n1072'>1072</a>
<a id='n1073' href='#n1073'>1073</a>
<a id='n1074' href='#n1074'>1074</a>
<a id='n1075' href='#n1075'>1075</a>
<a id='n1076' href='#n1076'>1076</a>
<a id='n1077' href='#n1077'>1077</a>
<a id='n1078' href='#n1078'>1078</a>
<a id='n1079' href='#n1079'>1079</a>
<a id='n1080' href='#n1080'>1080</a>
<a id='n1081' href='#n1081'>1081</a>
<a id='n1082' href='#n1082'>1082</a>
<a id='n1083' href='#n1083'>1083</a>
<a id='n1084' href='#n1084'>1084</a>
<a id='n1085' href='#n1085'>1085</a>
<a id='n1086' href='#n1086'>1086</a>
<a id='n1087' href='#n1087'>1087</a>
<a id='n1088' href='#n1088'>1088</a>
<a id='n1089' href='#n1089'>1089</a>
<a id='n1090' href='#n1090'>1090</a>
<a id='n1091' href='#n1091'>1091</a>
<a id='n1092' href='#n1092'>1092</a>
<a id='n1093' href='#n1093'>1093</a>
<a id='n1094' href='#n1094'>1094</a>
<a id='n1095' href='#n1095'>1095</a>
<a id='n1096' href='#n1096'>1096</a>
<a id='n1097' href='#n1097'>1097</a>
<a id='n1098' href='#n1098'>1098</a>
<a id='n1099' href='#n1099'>1099</a>
<a id='n1100' href='#n1100'>1100</a>
<a id='n1101' href='#n1101'>1101</a>
<a id='n1102' href='#n1102'>1102</a>
<a id='n1103' href='#n1103'>1103</a>
<a id='n1104' href='#n1104'>1104</a>
<a id='n1105' href='#n1105'>1105</a>
<a id='n1106' href='#n1106'>1106</a>
<a id='n1107' href='#n1107'>1107</a>
<a id='n1108' href='#n1108'>1108</a>
<a id='n1109' href='#n1109'>1109</a>
<a id='n1110' href='#n1110'>1110</a>
<a id='n1111' href='#n1111'>1111</a>
<a id='n1112' href='#n1112'>1112</a>
<a id='n1113' href='#n1113'>1113</a>
<a id='n1114' href='#n1114'>1114</a>
<a id='n1115' href='#n1115'>1115</a>
<a id='n1116' href='#n1116'>1116</a>
<a id='n1117' href='#n1117'>1117</a>
<a id='n1118' href='#n1118'>1118</a>
<a id='n1119' href='#n1119'>1119</a>
<a id='n1120' href='#n1120'>1120</a>
<a id='n1121' href='#n1121'>1121</a>
<a id='n1122' href='#n1122'>1122</a>
<a id='n1123' href='#n1123'>1123</a>
<a id='n1124' href='#n1124'>1124</a>
<a id='n1125' href='#n1125'>1125</a>
<a id='n1126' href='#n1126'>1126</a>
<a id='n1127' href='#n1127'>1127</a>
<a id='n1128' href='#n1128'>1128</a>
<a id='n1129' href='#n1129'>1129</a>
<a id='n1130' href='#n1130'>1130</a>
<a id='n1131' href='#n1131'>1131</a>
<a id='n1132' href='#n1132'>1132</a>
<a id='n1133' href='#n1133'>1133</a>
<a id='n1134' href='#n1134'>1134</a>
<a id='n1135' href='#n1135'>1135</a>
<a id='n1136' href='#n1136'>1136</a>
<a id='n1137' href='#n1137'>1137</a>
<a id='n1138' href='#n1138'>1138</a>
<a id='n1139' href='#n1139'>1139</a>
<a id='n1140' href='#n1140'>1140</a>
<a id='n1141' href='#n1141'>1141</a>
<a id='n1142' href='#n1142'>1142</a>
<a id='n1143' href='#n1143'>1143</a>
<a id='n1144' href='#n1144'>1144</a>
<a id='n1145' href='#n1145'>1145</a>
<a id='n1146' href='#n1146'>1146</a>
<a id='n1147' href='#n1147'>1147</a>
<a id='n1148' href='#n1148'>1148</a>
<a id='n1149' href='#n1149'>1149</a>
<a id='n1150' href='#n1150'>1150</a>
<a id='n1151' href='#n1151'>1151</a>
<a id='n1152' href='#n1152'>1152</a>
<a id='n1153' href='#n1153'>1153</a>
<a id='n1154' href='#n1154'>1154</a>
<a id='n1155' href='#n1155'>1155</a>
<a id='n1156' href='#n1156'>1156</a>
<a id='n1157' href='#n1157'>1157</a>
<a id='n1158' href='#n1158'>1158</a>
<a id='n1159' href='#n1159'>1159</a>
<a id='n1160' href='#n1160'>1160</a>
<a id='n1161' href='#n1161'>1161</a>
<a id='n1162' href='#n1162'>1162</a>
<a id='n1163' href='#n1163'>1163</a>
<a id='n1164' href='#n1164'>1164</a>
<a id='n1165' href='#n1165'>1165</a>
<a id='n1166' href='#n1166'>1166</a>
<a id='n1167' href='#n1167'>1167</a>
<a id='n1168' href='#n1168'>1168</a>
<a id='n1169' href='#n1169'>1169</a>
<a id='n1170' href='#n1170'>1170</a>
<a id='n1171' href='#n1171'>1171</a>
<a id='n1172' href='#n1172'>1172</a>
<a id='n1173' href='#n1173'>1173</a>
<a id='n1174' href='#n1174'>1174</a>
<a id='n1175' href='#n1175'>1175</a>
<a id='n1176' href='#n1176'>1176</a>
<a id='n1177' href='#n1177'>1177</a>
<a id='n1178' href='#n1178'>1178</a>
<a id='n1179' href='#n1179'>1179</a>
<a id='n1180' href='#n1180'>1180</a>
<a id='n1181' href='#n1181'>1181</a>
<a id='n1182' href='#n1182'>1182</a>
<a id='n1183' href='#n1183'>1183</a>
<a id='n1184' href='#n1184'>1184</a>
<a id='n1185' href='#n1185'>1185</a>
<a id='n1186' href='#n1186'>1186</a>
<a id='n1187' href='#n1187'>1187</a>
<a id='n1188' href='#n1188'>1188</a>
<a id='n1189' href='#n1189'>1189</a>
<a id='n1190' href='#n1190'>1190</a>
<a id='n1191' href='#n1191'>1191</a>
<a id='n1192' href='#n1192'>1192</a>
<a id='n1193' href='#n1193'>1193</a>
<a id='n1194' href='#n1194'>1194</a>
<a id='n1195' href='#n1195'>1195</a>
<a id='n1196' href='#n1196'>1196</a>
<a id='n1197' href='#n1197'>1197</a>
<a id='n1198' href='#n1198'>1198</a>
<a id='n1199' href='#n1199'>1199</a>
<a id='n1200' href='#n1200'>1200</a>
<a id='n1201' href='#n1201'>1201</a>
<a id='n1202' href='#n1202'>1202</a>
<a id='n1203' href='#n1203'>1203</a>
<a id='n1204' href='#n1204'>1204</a>
<a id='n1205' href='#n1205'>1205</a>
<a id='n1206' href='#n1206'>1206</a>
<a id='n1207' href='#n1207'>1207</a>
<a id='n1208' href='#n1208'>1208</a>
<a id='n1209' href='#n1209'>1209</a>
<a id='n1210' href='#n1210'>1210</a>
<a id='n1211' href='#n1211'>1211</a>
<a id='n1212' href='#n1212'>1212</a>
<a id='n1213' href='#n1213'>1213</a>
<a id='n1214' href='#n1214'>1214</a>
<a id='n1215' href='#n1215'>1215</a>
<a id='n1216' href='#n1216'>1216</a>
<a id='n1217' href='#n1217'>1217</a>
<a id='n1218' href='#n1218'>1218</a>
<a id='n1219' href='#n1219'>1219</a>
<a id='n1220' href='#n1220'>1220</a>
<a id='n1221' href='#n1221'>1221</a>
<a id='n1222' href='#n1222'>1222</a>
<a id='n1223' href='#n1223'>1223</a>
<a id='n1224' href='#n1224'>1224</a>
<a id='n1225' href='#n1225'>1225</a>
<a id='n1226' href='#n1226'>1226</a>
<a id='n1227' href='#n1227'>1227</a>
<a id='n1228' href='#n1228'>1228</a>
<a id='n1229' href='#n1229'>1229</a>
<a id='n1230' href='#n1230'>1230</a>
<a id='n1231' href='#n1231'>1231</a>
<a id='n1232' href='#n1232'>1232</a>
<a id='n1233' href='#n1233'>1233</a>
<a id='n1234' href='#n1234'>1234</a>
<a id='n1235' href='#n1235'>1235</a>
<a id='n1236' href='#n1236'>1236</a>
<a id='n1237' href='#n1237'>1237</a>
<a id='n1238' href='#n1238'>1238</a>
<a id='n1239' href='#n1239'>1239</a>
<a id='n1240' href='#n1240'>1240</a>
<a id='n1241' href='#n1241'>1241</a>
<a id='n1242' href='#n1242'>1242</a>
<a id='n1243' href='#n1243'>1243</a>
<a id='n1244' href='#n1244'>1244</a>
<a id='n1245' href='#n1245'>1245</a>
<a id='n1246' href='#n1246'>1246</a>
<a id='n1247' href='#n1247'>1247</a>
<a id='n1248' href='#n1248'>1248</a>
<a id='n1249' href='#n1249'>1249</a>
<a id='n1250' href='#n1250'>1250</a>
<a id='n1251' href='#n1251'>1251</a>
<a id='n1252' href='#n1252'>1252</a>
<a id='n1253' href='#n1253'>1253</a>
<a id='n1254' href='#n1254'>1254</a>
<a id='n1255' href='#n1255'>1255</a>
<a id='n1256' href='#n1256'>1256</a>
<a id='n1257' href='#n1257'>1257</a>
<a id='n1258' href='#n1258'>1258</a>
<a id='n1259' href='#n1259'>1259</a>
<a id='n1260' href='#n1260'>1260</a>
<a id='n1261' href='#n1261'>1261</a>
<a id='n1262' href='#n1262'>1262</a>
<a id='n1263' href='#n1263'>1263</a>
<a id='n1264' href='#n1264'>1264</a>
<a id='n1265' href='#n1265'>1265</a>
<a id='n1266' href='#n1266'>1266</a>
<a id='n1267' href='#n1267'>1267</a>
<a id='n1268' href='#n1268'>1268</a>
<a id='n1269' href='#n1269'>1269</a>
<a id='n1270' href='#n1270'>1270</a>
<a id='n1271' href='#n1271'>1271</a>
<a id='n1272' href='#n1272'>1272</a>
<a id='n1273' href='#n1273'>1273</a>
<a id='n1274' href='#n1274'>1274</a>
<a id='n1275' href='#n1275'>1275</a>
<a id='n1276' href='#n1276'>1276</a>
<a id='n1277' href='#n1277'>1277</a>
<a id='n1278' href='#n1278'>1278</a>
<a id='n1279' href='#n1279'>1279</a>
<a id='n1280' href='#n1280'>1280</a>
<a id='n1281' href='#n1281'>1281</a>
<a id='n1282' href='#n1282'>1282</a>
<a id='n1283' href='#n1283'>1283</a>
<a id='n1284' href='#n1284'>1284</a>
<a id='n1285' href='#n1285'>1285</a>
<a id='n1286' href='#n1286'>1286</a>
<a id='n1287' href='#n1287'>1287</a>
<a id='n1288' href='#n1288'>1288</a>
<a id='n1289' href='#n1289'>1289</a>
<a id='n1290' href='#n1290'>1290</a>
<a id='n1291' href='#n1291'>1291</a>
<a id='n1292' href='#n1292'>1292</a>
<a id='n1293' href='#n1293'>1293</a>
<a id='n1294' href='#n1294'>1294</a>
<a id='n1295' href='#n1295'>1295</a>
<a id='n1296' href='#n1296'>1296</a>
<a id='n1297' href='#n1297'>1297</a>
<a id='n1298' href='#n1298'>1298</a>
<a id='n1299' href='#n1299'>1299</a>
<a id='n1300' href='#n1300'>1300</a>
<a id='n1301' href='#n1301'>1301</a>
<a id='n1302' href='#n1302'>1302</a>
<a id='n1303' href='#n1303'>1303</a>
<a id='n1304' href='#n1304'>1304</a>
<a id='n1305' href='#n1305'>1305</a>
<a id='n1306' href='#n1306'>1306</a>
<a id='n1307' href='#n1307'>1307</a>
<a id='n1308' href='#n1308'>1308</a>
<a id='n1309' href='#n1309'>1309</a>
<a id='n1310' href='#n1310'>1310</a>
<a id='n1311' href='#n1311'>1311</a>
<a id='n1312' href='#n1312'>1312</a>
<a id='n1313' href='#n1313'>1313</a>
<a id='n1314' href='#n1314'>1314</a>
<a id='n1315' href='#n1315'>1315</a>
<a id='n1316' href='#n1316'>1316</a>
<a id='n1317' href='#n1317'>1317</a>
<a id='n1318' href='#n1318'>1318</a>
<a id='n1319' href='#n1319'>1319</a>
<a id='n1320' href='#n1320'>1320</a>
<a id='n1321' href='#n1321'>1321</a>
<a id='n1322' href='#n1322'>1322</a>
<a id='n1323' href='#n1323'>1323</a>
<a id='n1324' href='#n1324'>1324</a>
<a id='n1325' href='#n1325'>1325</a>
<a id='n1326' href='#n1326'>1326</a>
<a id='n1327' href='#n1327'>1327</a>
<a id='n1328' href='#n1328'>1328</a>
<a id='n1329' href='#n1329'>1329</a>
<a id='n1330' href='#n1330'>1330</a>
<a id='n1331' href='#n1331'>1331</a>
<a id='n1332' href='#n1332'>1332</a>
<a id='n1333' href='#n1333'>1333</a>
<a id='n1334' href='#n1334'>1334</a>
<a id='n1335' href='#n1335'>1335</a>
<a id='n1336' href='#n1336'>1336</a>
<a id='n1337' href='#n1337'>1337</a>
<a id='n1338' href='#n1338'>1338</a>
<a id='n1339' href='#n1339'>1339</a>
<a id='n1340' href='#n1340'>1340</a>
<a id='n1341' href='#n1341'>1341</a>
<a id='n1342' href='#n1342'>1342</a>
<a id='n1343' href='#n1343'>1343</a>
<a id='n1344' href='#n1344'>1344</a>
<a id='n1345' href='#n1345'>1345</a>
<a id='n1346' href='#n1346'>1346</a>
<a id='n1347' href='#n1347'>1347</a>
<a id='n1348' href='#n1348'>1348</a>
<a id='n1349' href='#n1349'>1349</a>
<a id='n1350' href='#n1350'>1350</a>
<a id='n1351' href='#n1351'>1351</a>
<a id='n1352' href='#n1352'>1352</a>
<a id='n1353' href='#n1353'>1353</a>
<a id='n1354' href='#n1354'>1354</a>
<a id='n1355' href='#n1355'>1355</a>
<a id='n1356' href='#n1356'>1356</a>
<a id='n1357' href='#n1357'>1357</a>
<a id='n1358' href='#n1358'>1358</a>
<a id='n1359' href='#n1359'>1359</a>
<a id='n1360' href='#n1360'>1360</a>
<a id='n1361' href='#n1361'>1361</a>
<a id='n1362' href='#n1362'>1362</a>
<a id='n1363' href='#n1363'>1363</a>
<a id='n1364' href='#n1364'>1364</a>
<a id='n1365' href='#n1365'>1365</a>
<a id='n1366' href='#n1366'>1366</a>
<a id='n1367' href='#n1367'>1367</a>
<a id='n1368' href='#n1368'>1368</a>
<a id='n1369' href='#n1369'>1369</a>
<a id='n1370' href='#n1370'>1370</a>
<a id='n1371' href='#n1371'>1371</a>
<a id='n1372' href='#n1372'>1372</a>
<a id='n1373' href='#n1373'>1373</a>
<a id='n1374' href='#n1374'>1374</a>
<a id='n1375' href='#n1375'>1375</a>
<a id='n1376' href='#n1376'>1376</a>
<a id='n1377' href='#n1377'>1377</a>
<a id='n1378' href='#n1378'>1378</a>
<a id='n1379' href='#n1379'>1379</a>
<a id='n1380' href='#n1380'>1380</a>
<a id='n1381' href='#n1381'>1381</a>
<a id='n1382' href='#n1382'>1382</a>
<a id='n1383' href='#n1383'>1383</a>
<a id='n1384' href='#n1384'>1384</a>
<a id='n1385' href='#n1385'>1385</a>
<a id='n1386' href='#n1386'>1386</a>
<a id='n1387' href='#n1387'>1387</a>
<a id='n1388' href='#n1388'>1388</a>
<a id='n1389' href='#n1389'>1389</a>
<a id='n1390' href='#n1390'>1390</a>
<a id='n1391' href='#n1391'>1391</a>
<a id='n1392' href='#n1392'>1392</a>
<a id='n1393' href='#n1393'>1393</a>
<a id='n1394' href='#n1394'>1394</a>
<a id='n1395' href='#n1395'>1395</a>
<a id='n1396' href='#n1396'>1396</a>
<a id='n1397' href='#n1397'>1397</a>
<a id='n1398' href='#n1398'>1398</a>
<a id='n1399' href='#n1399'>1399</a>
<a id='n1400' href='#n1400'>1400</a>
<a id='n1401' href='#n1401'>1401</a>
<a id='n1402' href='#n1402'>1402</a>
<a id='n1403' href='#n1403'>1403</a>
<a id='n1404' href='#n1404'>1404</a>
<a id='n1405' href='#n1405'>1405</a>
<a id='n1406' href='#n1406'>1406</a>
<a id='n1407' href='#n1407'>1407</a>
<a id='n1408' href='#n1408'>1408</a>
<a id='n1409' href='#n1409'>1409</a>
<a id='n1410' href='#n1410'>1410</a>
<a id='n1411' href='#n1411'>1411</a>
<a id='n1412' href='#n1412'>1412</a>
<a id='n1413' href='#n1413'>1413</a>
<a id='n1414' href='#n1414'>1414</a>
<a id='n1415' href='#n1415'>1415</a>
<a id='n1416' href='#n1416'>1416</a>
<a id='n1417' href='#n1417'>1417</a>
<a id='n1418' href='#n1418'>1418</a>
<a id='n1419' href='#n1419'>1419</a>
<a id='n1420' href='#n1420'>1420</a>
<a id='n1421' href='#n1421'>1421</a>
<a id='n1422' href='#n1422'>1422</a>
<a id='n1423' href='#n1423'>1423</a>
<a id='n1424' href='#n1424'>1424</a>
<a id='n1425' href='#n1425'>1425</a>
<a id='n1426' href='#n1426'>1426</a>
<a id='n1427' href='#n1427'>1427</a>
<a id='n1428' href='#n1428'>1428</a>
<a id='n1429' href='#n1429'>1429</a>
<a id='n1430' href='#n1430'>1430</a>
<a id='n1431' href='#n1431'>1431</a>
<a id='n1432' href='#n1432'>1432</a>
<a id='n1433' href='#n1433'>1433</a>
<a id='n1434' href='#n1434'>1434</a>
<a id='n1435' href='#n1435'>1435</a>
<a id='n1436' href='#n1436'>1436</a>
<a id='n1437' href='#n1437'>1437</a>
<a id='n1438' href='#n1438'>1438</a>
<a id='n1439' href='#n1439'>1439</a>
<a id='n1440' href='#n1440'>1440</a>
<a id='n1441' href='#n1441'>1441</a>
<a id='n1442' href='#n1442'>1442</a>
<a id='n1443' href='#n1443'>1443</a>
<a id='n1444' href='#n1444'>1444</a>
<a id='n1445' href='#n1445'>1445</a>
<a id='n1446' href='#n1446'>1446</a>
<a id='n1447' href='#n1447'>1447</a>
<a id='n1448' href='#n1448'>1448</a>
<a id='n1449' href='#n1449'>1449</a>
<a id='n1450' href='#n1450'>1450</a>
<a id='n1451' href='#n1451'>1451</a>
<a id='n1452' href='#n1452'>1452</a>
<a id='n1453' href='#n1453'>1453</a>
<a id='n1454' href='#n1454'>1454</a>
<a id='n1455' href='#n1455'>1455</a>
<a id='n1456' href='#n1456'>1456</a>
<a id='n1457' href='#n1457'>1457</a>
<a id='n1458' href='#n1458'>1458</a>
<a id='n1459' href='#n1459'>1459</a>
<a id='n1460' href='#n1460'>1460</a>
<a id='n1461' href='#n1461'>1461</a>
<a id='n1462' href='#n1462'>1462</a>
<a id='n1463' href='#n1463'>1463</a>
<a id='n1464' href='#n1464'>1464</a>
<a id='n1465' href='#n1465'>1465</a>
<a id='n1466' href='#n1466'>1466</a>
<a id='n1467' href='#n1467'>1467</a>
<a id='n1468' href='#n1468'>1468</a>
<a id='n1469' href='#n1469'>1469</a>
<a id='n1470' href='#n1470'>1470</a>
<a id='n1471' href='#n1471'>1471</a>
<a id='n1472' href='#n1472'>1472</a>
<a id='n1473' href='#n1473'>1473</a>
<a id='n1474' href='#n1474'>1474</a>
<a id='n1475' href='#n1475'>1475</a>
<a id='n1476' href='#n1476'>1476</a>
<a id='n1477' href='#n1477'>1477</a>
<a id='n1478' href='#n1478'>1478</a>
<a id='n1479' href='#n1479'>1479</a>
<a id='n1480' href='#n1480'>1480</a>
<a id='n1481' href='#n1481'>1481</a>
<a id='n1482' href='#n1482'>1482</a>
<a id='n1483' href='#n1483'>1483</a>
<a id='n1484' href='#n1484'>1484</a>
<a id='n1485' href='#n1485'>1485</a>
<a id='n1486' href='#n1486'>1486</a>
<a id='n1487' href='#n1487'>1487</a>
<a id='n1488' href='#n1488'>1488</a>
<a id='n1489' href='#n1489'>1489</a>
<a id='n1490' href='#n1490'>1490</a>
<a id='n1491' href='#n1491'>1491</a>
<a id='n1492' href='#n1492'>1492</a>
<a id='n1493' href='#n1493'>1493</a>
<a id='n1494' href='#n1494'>1494</a>
<a id='n1495' href='#n1495'>1495</a>
<a id='n1496' href='#n1496'>1496</a>
<a id='n1497' href='#n1497'>1497</a>
<a id='n1498' href='#n1498'>1498</a>
<a id='n1499' href='#n1499'>1499</a>
<a id='n1500' href='#n1500'>1500</a>
<a id='n1501' href='#n1501'>1501</a>
<a id='n1502' href='#n1502'>1502</a>
<a id='n1503' href='#n1503'>1503</a>
<a id='n1504' href='#n1504'>1504</a>
<a id='n1505' href='#n1505'>1505</a>
<a id='n1506' href='#n1506'>1506</a>
<a id='n1507' href='#n1507'>1507</a>
<a id='n1508' href='#n1508'>1508</a>
<a id='n1509' href='#n1509'>1509</a>
<a id='n1510' href='#n1510'>1510</a>
<a id='n1511' href='#n1511'>1511</a>
<a id='n1512' href='#n1512'>1512</a>
<a id='n1513' href='#n1513'>1513</a>
<a id='n1514' href='#n1514'>1514</a>
<a id='n1515' href='#n1515'>1515</a>
<a id='n1516' href='#n1516'>1516</a>
<a id='n1517' href='#n1517'>1517</a>
<a id='n1518' href='#n1518'>1518</a>
<a id='n1519' href='#n1519'>1519</a>
<a id='n1520' href='#n1520'>1520</a>
<a id='n1521' href='#n1521'>1521</a>
<a id='n1522' href='#n1522'>1522</a>
<a id='n1523' href='#n1523'>1523</a>
<a id='n1524' href='#n1524'>1524</a>
<a id='n1525' href='#n1525'>1525</a>
<a id='n1526' href='#n1526'>1526</a>
<a id='n1527' href='#n1527'>1527</a>
<a id='n1528' href='#n1528'>1528</a>
<a id='n1529' href='#n1529'>1529</a>
<a id='n1530' href='#n1530'>1530</a>
<a id='n1531' href='#n1531'>1531</a>
<a id='n1532' href='#n1532'>1532</a>
<a id='n1533' href='#n1533'>1533</a>
<a id='n1534' href='#n1534'>1534</a>
<a id='n1535' href='#n1535'>1535</a>
<a id='n1536' href='#n1536'>1536</a>
<a id='n1537' href='#n1537'>1537</a>
<a id='n1538' href='#n1538'>1538</a>
<a id='n1539' href='#n1539'>1539</a>
<a id='n1540' href='#n1540'>1540</a>
<a id='n1541' href='#n1541'>1541</a>
<a id='n1542' href='#n1542'>1542</a>
<a id='n1543' href='#n1543'>1543</a>
<a id='n1544' href='#n1544'>1544</a>
<a id='n1545' href='#n1545'>1545</a>
<a id='n1546' href='#n1546'>1546</a>
<a id='n1547' href='#n1547'>1547</a>
<a id='n1548' href='#n1548'>1548</a>
<a id='n1549' href='#n1549'>1549</a>
<a id='n1550' href='#n1550'>1550</a>
<a id='n1551' href='#n1551'>1551</a>
<a id='n1552' href='#n1552'>1552</a>
<a id='n1553' href='#n1553'>1553</a>
<a id='n1554' href='#n1554'>1554</a>
<a id='n1555' href='#n1555'>1555</a>
<a id='n1556' href='#n1556'>1556</a>
<a id='n1557' href='#n1557'>1557</a>
<a id='n1558' href='#n1558'>1558</a>
<a id='n1559' href='#n1559'>1559</a>
<a id='n1560' href='#n1560'>1560</a>
<a id='n1561' href='#n1561'>1561</a>
<a id='n1562' href='#n1562'>1562</a>
<a id='n1563' href='#n1563'>1563</a>
<a id='n1564' href='#n1564'>1564</a>
<a id='n1565' href='#n1565'>1565</a>
<a id='n1566' href='#n1566'>1566</a>
<a id='n1567' href='#n1567'>1567</a>
<a id='n1568' href='#n1568'>1568</a>
<a id='n1569' href='#n1569'>1569</a>
<a id='n1570' href='#n1570'>1570</a>
<a id='n1571' href='#n1571'>1571</a>
<a id='n1572' href='#n1572'>1572</a>
<a id='n1573' href='#n1573'>1573</a>
<a id='n1574' href='#n1574'>1574</a>
<a id='n1575' href='#n1575'>1575</a>
<a id='n1576' href='#n1576'>1576</a>
<a id='n1577' href='#n1577'>1577</a>
<a id='n1578' href='#n1578'>1578</a>
<a id='n1579' href='#n1579'>1579</a>
<a id='n1580' href='#n1580'>1580</a>
<a id='n1581' href='#n1581'>1581</a>
<a id='n1582' href='#n1582'>1582</a>
<a id='n1583' href='#n1583'>1583</a>
<a id='n1584' href='#n1584'>1584</a>
<a id='n1585' href='#n1585'>1585</a>
<a id='n1586' href='#n1586'>1586</a>
<a id='n1587' href='#n1587'>1587</a>
<a id='n1588' href='#n1588'>1588</a>
<a id='n1589' href='#n1589'>1589</a>
<a id='n1590' href='#n1590'>1590</a>
<a id='n1591' href='#n1591'>1591</a>
<a id='n1592' href='#n1592'>1592</a>
<a id='n1593' href='#n1593'>1593</a>
<a id='n1594' href='#n1594'>1594</a>
<a id='n1595' href='#n1595'>1595</a>
<a id='n1596' href='#n1596'>1596</a>
<a id='n1597' href='#n1597'>1597</a>
<a id='n1598' href='#n1598'>1598</a>
<a id='n1599' href='#n1599'>1599</a>
<a id='n1600' href='#n1600'>1600</a>
<a id='n1601' href='#n1601'>1601</a>
<a id='n1602' href='#n1602'>1602</a>
<a id='n1603' href='#n1603'>1603</a>
<a id='n1604' href='#n1604'>1604</a>
<a id='n1605' href='#n1605'>1605</a>
<a id='n1606' href='#n1606'>1606</a>
<a id='n1607' href='#n1607'>1607</a>
<a id='n1608' href='#n1608'>1608</a>
<a id='n1609' href='#n1609'>1609</a>
<a id='n1610' href='#n1610'>1610</a>
<a id='n1611' href='#n1611'>1611</a>
<a id='n1612' href='#n1612'>1612</a>
<a id='n1613' href='#n1613'>1613</a>
<a id='n1614' href='#n1614'>1614</a>
<a id='n1615' href='#n1615'>1615</a>
<a id='n1616' href='#n1616'>1616</a>
<a id='n1617' href='#n1617'>1617</a>
<a id='n1618' href='#n1618'>1618</a>
<a id='n1619' href='#n1619'>1619</a>
<a id='n1620' href='#n1620'>1620</a>
<a id='n1621' href='#n1621'>1621</a>
<a id='n1622' href='#n1622'>1622</a>
<a id='n1623' href='#n1623'>1623</a>
<a id='n1624' href='#n1624'>1624</a>
<a id='n1625' href='#n1625'>1625</a>
<a id='n1626' href='#n1626'>1626</a>
<a id='n1627' href='#n1627'>1627</a>
<a id='n1628' href='#n1628'>1628</a>
<a id='n1629' href='#n1629'>1629</a>
<a id='n1630' href='#n1630'>1630</a>
<a id='n1631' href='#n1631'>1631</a>
<a id='n1632' href='#n1632'>1632</a>
<a id='n1633' href='#n1633'>1633</a>
<a id='n1634' href='#n1634'>1634</a>
<a id='n1635' href='#n1635'>1635</a>
<a id='n1636' href='#n1636'>1636</a>
<a id='n1637' href='#n1637'>1637</a>
<a id='n1638' href='#n1638'>1638</a>
<a id='n1639' href='#n1639'>1639</a>
<a id='n1640' href='#n1640'>1640</a>
<a id='n1641' href='#n1641'>1641</a>
<a id='n1642' href='#n1642'>1642</a>
<a id='n1643' href='#n1643'>1643</a>
<a id='n1644' href='#n1644'>1644</a>
<a id='n1645' href='#n1645'>1645</a>
<a id='n1646' href='#n1646'>1646</a>
<a id='n1647' href='#n1647'>1647</a>
<a id='n1648' href='#n1648'>1648</a>
<a id='n1649' href='#n1649'>1649</a>
<a id='n1650' href='#n1650'>1650</a>
<a id='n1651' href='#n1651'>1651</a>
<a id='n1652' href='#n1652'>1652</a>
<a id='n1653' href='#n1653'>1653</a>
<a id='n1654' href='#n1654'>1654</a>
<a id='n1655' href='#n1655'>1655</a>
<a id='n1656' href='#n1656'>1656</a>
<a id='n1657' href='#n1657'>1657</a>
<a id='n1658' href='#n1658'>1658</a>
<a id='n1659' href='#n1659'>1659</a>
<a id='n1660' href='#n1660'>1660</a>
<a id='n1661' href='#n1661'>1661</a>
<a id='n1662' href='#n1662'>1662</a>
<a id='n1663' href='#n1663'>1663</a>
<a id='n1664' href='#n1664'>1664</a>
<a id='n1665' href='#n1665'>1665</a>
<a id='n1666' href='#n1666'>1666</a>
<a id='n1667' href='#n1667'>1667</a>
<a id='n1668' href='#n1668'>1668</a>
<a id='n1669' href='#n1669'>1669</a>
<a id='n1670' href='#n1670'>1670</a>
<a id='n1671' href='#n1671'>1671</a>
<a id='n1672' href='#n1672'>1672</a>
<a id='n1673' href='#n1673'>1673</a>
<a id='n1674' href='#n1674'>1674</a>
<a id='n1675' href='#n1675'>1675</a>
<a id='n1676' href='#n1676'>1676</a>
<a id='n1677' href='#n1677'>1677</a>
<a id='n1678' href='#n1678'>1678</a>
<a id='n1679' href='#n1679'>1679</a>
<a id='n1680' href='#n1680'>1680</a>
<a id='n1681' href='#n1681'>1681</a>
<a id='n1682' href='#n1682'>1682</a>
<a id='n1683' href='#n1683'>1683</a>
<a id='n1684' href='#n1684'>1684</a>
<a id='n1685' href='#n1685'>1685</a>
<a id='n1686' href='#n1686'>1686</a>
<a id='n1687' href='#n1687'>1687</a>
<a id='n1688' href='#n1688'>1688</a>
<a id='n1689' href='#n1689'>1689</a>
<a id='n1690' href='#n1690'>1690</a>
<a id='n1691' href='#n1691'>1691</a>
<a id='n1692' href='#n1692'>1692</a>
<a id='n1693' href='#n1693'>1693</a>
<a id='n1694' href='#n1694'>1694</a>
<a id='n1695' href='#n1695'>1695</a>
<a id='n1696' href='#n1696'>1696</a>
<a id='n1697' href='#n1697'>1697</a>
<a id='n1698' href='#n1698'>1698</a>
<a id='n1699' href='#n1699'>1699</a>
<a id='n1700' href='#n1700'>1700</a>
<a id='n1701' href='#n1701'>1701</a>
<a id='n1702' href='#n1702'>1702</a>
<a id='n1703' href='#n1703'>1703</a>
<a id='n1704' href='#n1704'>1704</a>
<a id='n1705' href='#n1705'>1705</a>
<a id='n1706' href='#n1706'>1706</a>
<a id='n1707' href='#n1707'>1707</a>
<a id='n1708' href='#n1708'>1708</a>
<a id='n1709' href='#n1709'>1709</a>
<a id='n1710' href='#n1710'>1710</a>
<a id='n1711' href='#n1711'>1711</a>
<a id='n1712' href='#n1712'>1712</a>
<a id='n1713' href='#n1713'>1713</a>
<a id='n1714' href='#n1714'>1714</a>
<a id='n1715' href='#n1715'>1715</a>
<a id='n1716' href='#n1716'>1716</a>
<a id='n1717' href='#n1717'>1717</a>
<a id='n1718' href='#n1718'>1718</a>
<a id='n1719' href='#n1719'>1719</a>
<a id='n1720' href='#n1720'>1720</a>
<a id='n1721' href='#n1721'>1721</a>
<a id='n1722' href='#n1722'>1722</a>
<a id='n1723' href='#n1723'>1723</a>
<a id='n1724' href='#n1724'>1724</a>
<a id='n1725' href='#n1725'>1725</a>
<a id='n1726' href='#n1726'>1726</a>
<a id='n1727' href='#n1727'>1727</a>
<a id='n1728' href='#n1728'>1728</a>
<a id='n1729' href='#n1729'>1729</a>
<a id='n1730' href='#n1730'>1730</a>
<a id='n1731' href='#n1731'>1731</a>
<a id='n1732' href='#n1732'>1732</a>
<a id='n1733' href='#n1733'>1733</a>
<a id='n1734' href='#n1734'>1734</a>
<a id='n1735' href='#n1735'>1735</a>
<a id='n1736' href='#n1736'>1736</a>
<a id='n1737' href='#n1737'>1737</a>
<a id='n1738' href='#n1738'>1738</a>
<a id='n1739' href='#n1739'>1739</a>
<a id='n1740' href='#n1740'>1740</a>
<a id='n1741' href='#n1741'>1741</a>
<a id='n1742' href='#n1742'>1742</a>
<a id='n1743' href='#n1743'>1743</a>
<a id='n1744' href='#n1744'>1744</a>
<a id='n1745' href='#n1745'>1745</a>
<a id='n1746' href='#n1746'>1746</a>
<a id='n1747' href='#n1747'>1747</a>
<a id='n1748' href='#n1748'>1748</a>
<a id='n1749' href='#n1749'>1749</a>
<a id='n1750' href='#n1750'>1750</a>
<a id='n1751' href='#n1751'>1751</a>
<a id='n1752' href='#n1752'>1752</a>
<a id='n1753' href='#n1753'>1753</a>
<a id='n1754' href='#n1754'>1754</a>
<a id='n1755' href='#n1755'>1755</a>
<a id='n1756' href='#n1756'>1756</a>
<a id='n1757' href='#n1757'>1757</a>
<a id='n1758' href='#n1758'>1758</a>
<a id='n1759' href='#n1759'>1759</a>
<a id='n1760' href='#n1760'>1760</a>
<a id='n1761' href='#n1761'>1761</a>
<a id='n1762' href='#n1762'>1762</a>
<a id='n1763' href='#n1763'>1763</a>
<a id='n1764' href='#n1764'>1764</a>
<a id='n1765' href='#n1765'>1765</a>
<a id='n1766' href='#n1766'>1766</a>
<a id='n1767' href='#n1767'>1767</a>
<a id='n1768' href='#n1768'>1768</a>
<a id='n1769' href='#n1769'>1769</a>
<a id='n1770' href='#n1770'>1770</a>
<a id='n1771' href='#n1771'>1771</a>
<a id='n1772' href='#n1772'>1772</a>
<a id='n1773' href='#n1773'>1773</a>
<a id='n1774' href='#n1774'>1774</a>
<a id='n1775' href='#n1775'>1775</a>
<a id='n1776' href='#n1776'>1776</a>
<a id='n1777' href='#n1777'>1777</a>
<a id='n1778' href='#n1778'>1778</a>
<a id='n1779' href='#n1779'>1779</a>
<a id='n1780' href='#n1780'>1780</a>
<a id='n1781' href='#n1781'>1781</a>
<a id='n1782' href='#n1782'>1782</a>
<a id='n1783' href='#n1783'>1783</a>
<a id='n1784' href='#n1784'>1784</a>
<a id='n1785' href='#n1785'>1785</a>
<a id='n1786' href='#n1786'>1786</a>
<a id='n1787' href='#n1787'>1787</a>
<a id='n1788' href='#n1788'>1788</a>
<a id='n1789' href='#n1789'>1789</a>
<a id='n1790' href='#n1790'>1790</a>
<a id='n1791' href='#n1791'>1791</a>
<a id='n1792' href='#n1792'>1792</a>
<a id='n1793' href='#n1793'>1793</a>
<a id='n1794' href='#n1794'>1794</a>
<a id='n1795' href='#n1795'>1795</a>
<a id='n1796' href='#n1796'>1796</a>
<a id='n1797' href='#n1797'>1797</a>
<a id='n1798' href='#n1798'>1798</a>
<a id='n1799' href='#n1799'>1799</a>
<a id='n1800' href='#n1800'>1800</a>
<a id='n1801' href='#n1801'>1801</a>
<a id='n1802' href='#n1802'>1802</a>
<a id='n1803' href='#n1803'>1803</a>
<a id='n1804' href='#n1804'>1804</a>
<a id='n1805' href='#n1805'>1805</a>
<a id='n1806' href='#n1806'>1806</a>
<a id='n1807' href='#n1807'>1807</a>
<a id='n1808' href='#n1808'>1808</a>
<a id='n1809' href='#n1809'>1809</a>
<a id='n1810' href='#n1810'>1810</a>
<a id='n1811' href='#n1811'>1811</a>
<a id='n1812' href='#n1812'>1812</a>
<a id='n1813' href='#n1813'>1813</a>
<a id='n1814' href='#n1814'>1814</a>
<a id='n1815' href='#n1815'>1815</a>
<a id='n1816' href='#n1816'>1816</a>
<a id='n1817' href='#n1817'>1817</a>
<a id='n1818' href='#n1818'>1818</a>
<a id='n1819' href='#n1819'>1819</a>
<a id='n1820' href='#n1820'>1820</a>
<a id='n1821' href='#n1821'>1821</a>
<a id='n1822' href='#n1822'>1822</a>
<a id='n1823' href='#n1823'>1823</a>
<a id='n1824' href='#n1824'>1824</a>
<a id='n1825' href='#n1825'>1825</a>
<a id='n1826' href='#n1826'>1826</a>
<a id='n1827' href='#n1827'>1827</a>
<a id='n1828' href='#n1828'>1828</a>
<a id='n1829' href='#n1829'>1829</a>
<a id='n1830' href='#n1830'>1830</a>
<a id='n1831' href='#n1831'>1831</a>
<a id='n1832' href='#n1832'>1832</a>
<a id='n1833' href='#n1833'>1833</a>
<a id='n1834' href='#n1834'>1834</a>
<a id='n1835' href='#n1835'>1835</a>
<a id='n1836' href='#n1836'>1836</a>
<a id='n1837' href='#n1837'>1837</a>
<a id='n1838' href='#n1838'>1838</a>
<a id='n1839' href='#n1839'>1839</a>
<a id='n1840' href='#n1840'>1840</a>
<a id='n1841' href='#n1841'>1841</a>
<a id='n1842' href='#n1842'>1842</a>
<a id='n1843' href='#n1843'>1843</a>
<a id='n1844' href='#n1844'>1844</a>
<a id='n1845' href='#n1845'>1845</a>
<a id='n1846' href='#n1846'>1846</a>
<a id='n1847' href='#n1847'>1847</a>
<a id='n1848' href='#n1848'>1848</a>
<a id='n1849' href='#n1849'>1849</a>
<a id='n1850' href='#n1850'>1850</a>
<a id='n1851' href='#n1851'>1851</a>
<a id='n1852' href='#n1852'>1852</a>
<a id='n1853' href='#n1853'>1853</a>
<a id='n1854' href='#n1854'>1854</a>
<a id='n1855' href='#n1855'>1855</a>
<a id='n1856' href='#n1856'>1856</a>
<a id='n1857' href='#n1857'>1857</a>
<a id='n1858' href='#n1858'>1858</a>
<a id='n1859' href='#n1859'>1859</a>
<a id='n1860' href='#n1860'>1860</a>
<a id='n1861' href='#n1861'>1861</a>
<a id='n1862' href='#n1862'>1862</a>
<a id='n1863' href='#n1863'>1863</a>
<a id='n1864' href='#n1864'>1864</a>
<a id='n1865' href='#n1865'>1865</a>
<a id='n1866' href='#n1866'>1866</a>
<a id='n1867' href='#n1867'>1867</a>
<a id='n1868' href='#n1868'>1868</a>
<a id='n1869' href='#n1869'>1869</a>
<a id='n1870' href='#n1870'>1870</a>
<a id='n1871' href='#n1871'>1871</a>
<a id='n1872' href='#n1872'>1872</a>
<a id='n1873' href='#n1873'>1873</a>
<a id='n1874' href='#n1874'>1874</a>
<a id='n1875' href='#n1875'>1875</a>
<a id='n1876' href='#n1876'>1876</a>
<a id='n1877' href='#n1877'>1877</a>
<a id='n1878' href='#n1878'>1878</a>
<a id='n1879' href='#n1879'>1879</a>
<a id='n1880' href='#n1880'>1880</a>
<a id='n1881' href='#n1881'>1881</a>
<a id='n1882' href='#n1882'>1882</a>
<a id='n1883' href='#n1883'>1883</a>
<a id='n1884' href='#n1884'>1884</a>
<a id='n1885' href='#n1885'>1885</a>
<a id='n1886' href='#n1886'>1886</a>
<a id='n1887' href='#n1887'>1887</a>
<a id='n1888' href='#n1888'>1888</a>
<a id='n1889' href='#n1889'>1889</a>
<a id='n1890' href='#n1890'>1890</a>
<a id='n1891' href='#n1891'>1891</a>
<a id='n1892' href='#n1892'>1892</a>
<a id='n1893' href='#n1893'>1893</a>
<a id='n1894' href='#n1894'>1894</a>
<a id='n1895' href='#n1895'>1895</a>
<a id='n1896' href='#n1896'>1896</a>
<a id='n1897' href='#n1897'>1897</a>
<a id='n1898' href='#n1898'>1898</a>
<a id='n1899' href='#n1899'>1899</a>
<a id='n1900' href='#n1900'>1900</a>
<a id='n1901' href='#n1901'>1901</a>
<a id='n1902' href='#n1902'>1902</a>
<a id='n1903' href='#n1903'>1903</a>
<a id='n1904' href='#n1904'>1904</a>
<a id='n1905' href='#n1905'>1905</a>
<a id='n1906' href='#n1906'>1906</a>
<a id='n1907' href='#n1907'>1907</a>
<a id='n1908' href='#n1908'>1908</a>
<a id='n1909' href='#n1909'>1909</a>
<a id='n1910' href='#n1910'>1910</a>
<a id='n1911' href='#n1911'>1911</a>
<a id='n1912' href='#n1912'>1912</a>
<a id='n1913' href='#n1913'>1913</a>
<a id='n1914' href='#n1914'>1914</a>
<a id='n1915' href='#n1915'>1915</a>
<a id='n1916' href='#n1916'>1916</a>
<a id='n1917' href='#n1917'>1917</a>
<a id='n1918' href='#n1918'>1918</a>
<a id='n1919' href='#n1919'>1919</a>
<a id='n1920' href='#n1920'>1920</a>
<a id='n1921' href='#n1921'>1921</a>
<a id='n1922' href='#n1922'>1922</a>
<a id='n1923' href='#n1923'>1923</a>
<a id='n1924' href='#n1924'>1924</a>
<a id='n1925' href='#n1925'>1925</a>
<a id='n1926' href='#n1926'>1926</a>
<a id='n1927' href='#n1927'>1927</a>
<a id='n1928' href='#n1928'>1928</a>
<a id='n1929' href='#n1929'>1929</a>
<a id='n1930' href='#n1930'>1930</a>
<a id='n1931' href='#n1931'>1931</a>
<a id='n1932' href='#n1932'>1932</a>
<a id='n1933' href='#n1933'>1933</a>
<a id='n1934' href='#n1934'>1934</a>
<a id='n1935' href='#n1935'>1935</a>
<a id='n1936' href='#n1936'>1936</a>
<a id='n1937' href='#n1937'>1937</a>
<a id='n1938' href='#n1938'>1938</a>
<a id='n1939' href='#n1939'>1939</a>
<a id='n1940' href='#n1940'>1940</a>
<a id='n1941' href='#n1941'>1941</a>
<a id='n1942' href='#n1942'>1942</a>
<a id='n1943' href='#n1943'>1943</a>
<a id='n1944' href='#n1944'>1944</a>
<a id='n1945' href='#n1945'>1945</a>
<a id='n1946' href='#n1946'>1946</a>
<a id='n1947' href='#n1947'>1947</a>
<a id='n1948' href='#n1948'>1948</a>
<a id='n1949' href='#n1949'>1949</a>
<a id='n1950' href='#n1950'>1950</a>
<a id='n1951' href='#n1951'>1951</a>
<a id='n1952' href='#n1952'>1952</a>
<a id='n1953' href='#n1953'>1953</a>
<a id='n1954' href='#n1954'>1954</a>
<a id='n1955' href='#n1955'>1955</a>
<a id='n1956' href='#n1956'>1956</a>
<a id='n1957' href='#n1957'>1957</a>
<a id='n1958' href='#n1958'>1958</a>
<a id='n1959' href='#n1959'>1959</a>
<a id='n1960' href='#n1960'>1960</a>
<a id='n1961' href='#n1961'>1961</a>
<a id='n1962' href='#n1962'>1962</a>
<a id='n1963' href='#n1963'>1963</a>
<a id='n1964' href='#n1964'>1964</a>
<a id='n1965' href='#n1965'>1965</a>
<a id='n1966' href='#n1966'>1966</a>
<a id='n1967' href='#n1967'>1967</a>
<a id='n1968' href='#n1968'>1968</a>
<a id='n1969' href='#n1969'>1969</a>
<a id='n1970' href='#n1970'>1970</a>
<a id='n1971' href='#n1971'>1971</a>
<a id='n1972' href='#n1972'>1972</a>
<a id='n1973' href='#n1973'>1973</a>
<a id='n1974' href='#n1974'>1974</a>
<a id='n1975' href='#n1975'>1975</a>
<a id='n1976' href='#n1976'>1976</a>
<a id='n1977' href='#n1977'>1977</a>
<a id='n1978' href='#n1978'>1978</a>
<a id='n1979' href='#n1979'>1979</a>
<a id='n1980' href='#n1980'>1980</a>
<a id='n1981' href='#n1981'>1981</a>
<a id='n1982' href='#n1982'>1982</a>
<a id='n1983' href='#n1983'>1983</a>
<a id='n1984' href='#n1984'>1984</a>
<a id='n1985' href='#n1985'>1985</a>
<a id='n1986' href='#n1986'>1986</a>
<a id='n1987' href='#n1987'>1987</a>
<a id='n1988' href='#n1988'>1988</a>
<a id='n1989' href='#n1989'>1989</a>
<a id='n1990' href='#n1990'>1990</a>
<a id='n1991' href='#n1991'>1991</a>
<a id='n1992' href='#n1992'>1992</a>
<a id='n1993' href='#n1993'>1993</a>
<a id='n1994' href='#n1994'>1994</a>
<a id='n1995' href='#n1995'>1995</a>
<a id='n1996' href='#n1996'>1996</a>
<a id='n1997' href='#n1997'>1997</a>
<a id='n1998' href='#n1998'>1998</a>
<a id='n1999' href='#n1999'>1999</a>
<a id='n2000' href='#n2000'>2000</a>
<a id='n2001' href='#n2001'>2001</a>
<a id='n2002' href='#n2002'>2002</a>
<a id='n2003' href='#n2003'>2003</a>
<a id='n2004' href='#n2004'>2004</a>
<a id='n2005' href='#n2005'>2005</a>
<a id='n2006' href='#n2006'>2006</a>
<a id='n2007' href='#n2007'>2007</a>
<a id='n2008' href='#n2008'>2008</a>
<a id='n2009' href='#n2009'>2009</a>
<a id='n2010' href='#n2010'>2010</a>
<a id='n2011' href='#n2011'>2011</a>
<a id='n2012' href='#n2012'>2012</a>
<a id='n2013' href='#n2013'>2013</a>
<a id='n2014' href='#n2014'>2014</a>
<a id='n2015' href='#n2015'>2015</a>
<a id='n2016' href='#n2016'>2016</a>
<a id='n2017' href='#n2017'>2017</a>
<a id='n2018' href='#n2018'>2018</a>
<a id='n2019' href='#n2019'>2019</a>
<a id='n2020' href='#n2020'>2020</a>
<a id='n2021' href='#n2021'>2021</a>
<a id='n2022' href='#n2022'>2022</a>
<a id='n2023' href='#n2023'>2023</a>
<a id='n2024' href='#n2024'>2024</a>
<a id='n2025' href='#n2025'>2025</a>
<a id='n2026' href='#n2026'>2026</a>
<a id='n2027' href='#n2027'>2027</a>
<a id='n2028' href='#n2028'>2028</a>
<a id='n2029' href='#n2029'>2029</a>
<a id='n2030' href='#n2030'>2030</a>
<a id='n2031' href='#n2031'>2031</a>
<a id='n2032' href='#n2032'>2032</a>
<a id='n2033' href='#n2033'>2033</a>
<a id='n2034' href='#n2034'>2034</a>
<a id='n2035' href='#n2035'>2035</a>
<a id='n2036' href='#n2036'>2036</a>
<a id='n2037' href='#n2037'>2037</a>
<a id='n2038' href='#n2038'>2038</a>
<a id='n2039' href='#n2039'>2039</a>
<a id='n2040' href='#n2040'>2040</a>
<a id='n2041' href='#n2041'>2041</a>
<a id='n2042' href='#n2042'>2042</a>
<a id='n2043' href='#n2043'>2043</a>
<a id='n2044' href='#n2044'>2044</a>
<a id='n2045' href='#n2045'>2045</a>
<a id='n2046' href='#n2046'>2046</a>
<a id='n2047' href='#n2047'>2047</a>
<a id='n2048' href='#n2048'>2048</a>
<a id='n2049' href='#n2049'>2049</a>
<a id='n2050' href='#n2050'>2050</a>
<a id='n2051' href='#n2051'>2051</a>
<a id='n2052' href='#n2052'>2052</a>
<a id='n2053' href='#n2053'>2053</a>
<a id='n2054' href='#n2054'>2054</a>
<a id='n2055' href='#n2055'>2055</a>
<a id='n2056' href='#n2056'>2056</a>
<a id='n2057' href='#n2057'>2057</a>
<a id='n2058' href='#n2058'>2058</a>
<a id='n2059' href='#n2059'>2059</a>
<a id='n2060' href='#n2060'>2060</a>
<a id='n2061' href='#n2061'>2061</a>
<a id='n2062' href='#n2062'>2062</a>
<a id='n2063' href='#n2063'>2063</a>
<a id='n2064' href='#n2064'>2064</a>
<a id='n2065' href='#n2065'>2065</a>
<a id='n2066' href='#n2066'>2066</a>
<a id='n2067' href='#n2067'>2067</a>
<a id='n2068' href='#n2068'>2068</a>
<a id='n2069' href='#n2069'>2069</a>
<a id='n2070' href='#n2070'>2070</a>
<a id='n2071' href='#n2071'>2071</a>
<a id='n2072' href='#n2072'>2072</a>
<a id='n2073' href='#n2073'>2073</a>
<a id='n2074' href='#n2074'>2074</a>
<a id='n2075' href='#n2075'>2075</a>
<a id='n2076' href='#n2076'>2076</a>
<a id='n2077' href='#n2077'>2077</a>
<a id='n2078' href='#n2078'>2078</a>
<a id='n2079' href='#n2079'>2079</a>
<a id='n2080' href='#n2080'>2080</a>
<a id='n2081' href='#n2081'>2081</a>
<a id='n2082' href='#n2082'>2082</a>
<a id='n2083' href='#n2083'>2083</a>
<a id='n2084' href='#n2084'>2084</a>
<a id='n2085' href='#n2085'>2085</a>
<a id='n2086' href='#n2086'>2086</a>
<a id='n2087' href='#n2087'>2087</a>
<a id='n2088' href='#n2088'>2088</a>
<a id='n2089' href='#n2089'>2089</a>
<a id='n2090' href='#n2090'>2090</a>
<a id='n2091' href='#n2091'>2091</a>
<a id='n2092' href='#n2092'>2092</a>
<a id='n2093' href='#n2093'>2093</a>
<a id='n2094' href='#n2094'>2094</a>
<a id='n2095' href='#n2095'>2095</a>
<a id='n2096' href='#n2096'>2096</a>
<a id='n2097' href='#n2097'>2097</a>
<a id='n2098' href='#n2098'>2098</a>
<a id='n2099' href='#n2099'>2099</a>
<a id='n2100' href='#n2100'>2100</a>
<a id='n2101' href='#n2101'>2101</a>
<a id='n2102' href='#n2102'>2102</a>
<a id='n2103' href='#n2103'>2103</a>
<a id='n2104' href='#n2104'>2104</a>
<a id='n2105' href='#n2105'>2105</a>
<a id='n2106' href='#n2106'>2106</a>
<a id='n2107' href='#n2107'>2107</a>
<a id='n2108' href='#n2108'>2108</a>
<a id='n2109' href='#n2109'>2109</a>
<a id='n2110' href='#n2110'>2110</a>
<a id='n2111' href='#n2111'>2111</a>
<a id='n2112' href='#n2112'>2112</a>
<a id='n2113' href='#n2113'>2113</a>
<a id='n2114' href='#n2114'>2114</a>
<a id='n2115' href='#n2115'>2115</a>
<a id='n2116' href='#n2116'>2116</a>
<a id='n2117' href='#n2117'>2117</a>
<a id='n2118' href='#n2118'>2118</a>
<a id='n2119' href='#n2119'>2119</a>
<a id='n2120' href='#n2120'>2120</a>
<a id='n2121' href='#n2121'>2121</a>
<a id='n2122' href='#n2122'>2122</a>
<a id='n2123' href='#n2123'>2123</a>
<a id='n2124' href='#n2124'>2124</a>
<a id='n2125' href='#n2125'>2125</a>
<a id='n2126' href='#n2126'>2126</a>
<a id='n2127' href='#n2127'>2127</a>
<a id='n2128' href='#n2128'>2128</a>
<a id='n2129' href='#n2129'>2129</a>
<a id='n2130' href='#n2130'>2130</a>
<a id='n2131' href='#n2131'>2131</a>
<a id='n2132' href='#n2132'>2132</a>
<a id='n2133' href='#n2133'>2133</a>
<a id='n2134' href='#n2134'>2134</a>
<a id='n2135' href='#n2135'>2135</a>
<a id='n2136' href='#n2136'>2136</a>
<a id='n2137' href='#n2137'>2137</a>
<a id='n2138' href='#n2138'>2138</a>
<a id='n2139' href='#n2139'>2139</a>
<a id='n2140' href='#n2140'>2140</a>
<a id='n2141' href='#n2141'>2141</a>
<a id='n2142' href='#n2142'>2142</a>
<a id='n2143' href='#n2143'>2143</a>
<a id='n2144' href='#n2144'>2144</a>
<a id='n2145' href='#n2145'>2145</a>
<a id='n2146' href='#n2146'>2146</a>
<a id='n2147' href='#n2147'>2147</a>
<a id='n2148' href='#n2148'>2148</a>
<a id='n2149' href='#n2149'>2149</a>
<a id='n2150' href='#n2150'>2150</a>
<a id='n2151' href='#n2151'>2151</a>
<a id='n2152' href='#n2152'>2152</a>
<a id='n2153' href='#n2153'>2153</a>
<a id='n2154' href='#n2154'>2154</a>
<a id='n2155' href='#n2155'>2155</a>
<a id='n2156' href='#n2156'>2156</a>
<a id='n2157' href='#n2157'>2157</a>
<a id='n2158' href='#n2158'>2158</a>
<a id='n2159' href='#n2159'>2159</a>
<a id='n2160' href='#n2160'>2160</a>
<a id='n2161' href='#n2161'>2161</a>
<a id='n2162' href='#n2162'>2162</a>
<a id='n2163' href='#n2163'>2163</a>
<a id='n2164' href='#n2164'>2164</a>
<a id='n2165' href='#n2165'>2165</a>
<a id='n2166' href='#n2166'>2166</a>
<a id='n2167' href='#n2167'>2167</a>
<a id='n2168' href='#n2168'>2168</a>
<a id='n2169' href='#n2169'>2169</a>
<a id='n2170' href='#n2170'>2170</a>
<a id='n2171' href='#n2171'>2171</a>
<a id='n2172' href='#n2172'>2172</a>
<a id='n2173' href='#n2173'>2173</a>
<a id='n2174' href='#n2174'>2174</a>
<a id='n2175' href='#n2175'>2175</a>
<a id='n2176' href='#n2176'>2176</a>
<a id='n2177' href='#n2177'>2177</a>
<a id='n2178' href='#n2178'>2178</a>
<a id='n2179' href='#n2179'>2179</a>
<a id='n2180' href='#n2180'>2180</a>
<a id='n2181' href='#n2181'>2181</a>
<a id='n2182' href='#n2182'>2182</a>
<a id='n2183' href='#n2183'>2183</a>
<a id='n2184' href='#n2184'>2184</a>
<a id='n2185' href='#n2185'>2185</a>
<a id='n2186' href='#n2186'>2186</a>
<a id='n2187' href='#n2187'>2187</a>
<a id='n2188' href='#n2188'>2188</a>
<a id='n2189' href='#n2189'>2189</a>
<a id='n2190' href='#n2190'>2190</a>
<a id='n2191' href='#n2191'>2191</a>
<a id='n2192' href='#n2192'>2192</a>
<a id='n2193' href='#n2193'>2193</a>
<a id='n2194' href='#n2194'>2194</a>
<a id='n2195' href='#n2195'>2195</a>
<a id='n2196' href='#n2196'>2196</a>
<a id='n2197' href='#n2197'>2197</a>
<a id='n2198' href='#n2198'>2198</a>
<a id='n2199' href='#n2199'>2199</a>
<a id='n2200' href='#n2200'>2200</a>
<a id='n2201' href='#n2201'>2201</a>
<a id='n2202' href='#n2202'>2202</a>
<a id='n2203' href='#n2203'>2203</a>
<a id='n2204' href='#n2204'>2204</a>
<a id='n2205' href='#n2205'>2205</a>
<a id='n2206' href='#n2206'>2206</a>
<a id='n2207' href='#n2207'>2207</a>
<a id='n2208' href='#n2208'>2208</a>
<a id='n2209' href='#n2209'>2209</a>
<a id='n2210' href='#n2210'>2210</a>
<a id='n2211' href='#n2211'>2211</a>
<a id='n2212' href='#n2212'>2212</a>
<a id='n2213' href='#n2213'>2213</a>
<a id='n2214' href='#n2214'>2214</a>
<a id='n2215' href='#n2215'>2215</a>
<a id='n2216' href='#n2216'>2216</a>
<a id='n2217' href='#n2217'>2217</a>
<a id='n2218' href='#n2218'>2218</a>
<a id='n2219' href='#n2219'>2219</a>
<a id='n2220' href='#n2220'>2220</a>
<a id='n2221' href='#n2221'>2221</a>
<a id='n2222' href='#n2222'>2222</a>
<a id='n2223' href='#n2223'>2223</a>
<a id='n2224' href='#n2224'>2224</a>
<a id='n2225' href='#n2225'>2225</a>
<a id='n2226' href='#n2226'>2226</a>
<a id='n2227' href='#n2227'>2227</a>
<a id='n2228' href='#n2228'>2228</a>
<a id='n2229' href='#n2229'>2229</a>
<a id='n2230' href='#n2230'>2230</a>
<a id='n2231' href='#n2231'>2231</a>
<a id='n2232' href='#n2232'>2232</a>
<a id='n2233' href='#n2233'>2233</a>
<a id='n2234' href='#n2234'>2234</a>
<a id='n2235' href='#n2235'>2235</a>
<a id='n2236' href='#n2236'>2236</a>
<a id='n2237' href='#n2237'>2237</a>
<a id='n2238' href='#n2238'>2238</a>
<a id='n2239' href='#n2239'>2239</a>
<a id='n2240' href='#n2240'>2240</a>
<a id='n2241' href='#n2241'>2241</a>
<a id='n2242' href='#n2242'>2242</a>
<a id='n2243' href='#n2243'>2243</a>
<a id='n2244' href='#n2244'>2244</a>
<a id='n2245' href='#n2245'>2245</a>
<a id='n2246' href='#n2246'>2246</a>
<a id='n2247' href='#n2247'>2247</a>
<a id='n2248' href='#n2248'>2248</a>
<a id='n2249' href='#n2249'>2249</a>
<a id='n2250' href='#n2250'>2250</a>
<a id='n2251' href='#n2251'>2251</a>
<a id='n2252' href='#n2252'>2252</a>
<a id='n2253' href='#n2253'>2253</a>
<a id='n2254' href='#n2254'>2254</a>
<a id='n2255' href='#n2255'>2255</a>
<a id='n2256' href='#n2256'>2256</a>
<a id='n2257' href='#n2257'>2257</a>
<a id='n2258' href='#n2258'>2258</a>
<a id='n2259' href='#n2259'>2259</a>
<a id='n2260' href='#n2260'>2260</a>
<a id='n2261' href='#n2261'>2261</a>
<a id='n2262' href='#n2262'>2262</a>
<a id='n2263' href='#n2263'>2263</a>
<a id='n2264' href='#n2264'>2264</a>
<a id='n2265' href='#n2265'>2265</a>
<a id='n2266' href='#n2266'>2266</a>
<a id='n2267' href='#n2267'>2267</a>
<a id='n2268' href='#n2268'>2268</a>
<a id='n2269' href='#n2269'>2269</a>
<a id='n2270' href='#n2270'>2270</a>
<a id='n2271' href='#n2271'>2271</a>
<a id='n2272' href='#n2272'>2272</a>
<a id='n2273' href='#n2273'>2273</a>
<a id='n2274' href='#n2274'>2274</a>
<a id='n2275' href='#n2275'>2275</a>
<a id='n2276' href='#n2276'>2276</a>
<a id='n2277' href='#n2277'>2277</a>
<a id='n2278' href='#n2278'>2278</a>
<a id='n2279' href='#n2279'>2279</a>
<a id='n2280' href='#n2280'>2280</a>
<a id='n2281' href='#n2281'>2281</a>
<a id='n2282' href='#n2282'>2282</a>
<a id='n2283' href='#n2283'>2283</a>
<a id='n2284' href='#n2284'>2284</a>
<a id='n2285' href='#n2285'>2285</a>
<a id='n2286' href='#n2286'>2286</a>
<a id='n2287' href='#n2287'>2287</a>
<a id='n2288' href='#n2288'>2288</a>
<a id='n2289' href='#n2289'>2289</a>
<a id='n2290' href='#n2290'>2290</a>
<a id='n2291' href='#n2291'>2291</a>
<a id='n2292' href='#n2292'>2292</a>
<a id='n2293' href='#n2293'>2293</a>
<a id='n2294' href='#n2294'>2294</a>
<a id='n2295' href='#n2295'>2295</a>
<a id='n2296' href='#n2296'>2296</a>
<a id='n2297' href='#n2297'>2297</a>
<a id='n2298' href='#n2298'>2298</a>
<a id='n2299' href='#n2299'>2299</a>
<a id='n2300' href='#n2300'>2300</a>
<a id='n2301' href='#n2301'>2301</a>
<a id='n2302' href='#n2302'>2302</a>
<a id='n2303' href='#n2303'>2303</a>
<a id='n2304' href='#n2304'>2304</a>
<a id='n2305' href='#n2305'>2305</a>
<a id='n2306' href='#n2306'>2306</a>
<a id='n2307' href='#n2307'>2307</a>
<a id='n2308' href='#n2308'>2308</a>
<a id='n2309' href='#n2309'>2309</a>
<a id='n2310' href='#n2310'>2310</a>
<a id='n2311' href='#n2311'>2311</a>
<a id='n2312' href='#n2312'>2312</a>
<a id='n2313' href='#n2313'>2313</a>
<a id='n2314' href='#n2314'>2314</a>
<a id='n2315' href='#n2315'>2315</a>
<a id='n2316' href='#n2316'>2316</a>
<a id='n2317' href='#n2317'>2317</a>
<a id='n2318' href='#n2318'>2318</a>
<a id='n2319' href='#n2319'>2319</a>
<a id='n2320' href='#n2320'>2320</a>
<a id='n2321' href='#n2321'>2321</a>
<a id='n2322' href='#n2322'>2322</a>
<a id='n2323' href='#n2323'>2323</a>
<a id='n2324' href='#n2324'>2324</a>
<a id='n2325' href='#n2325'>2325</a>
<a id='n2326' href='#n2326'>2326</a>
<a id='n2327' href='#n2327'>2327</a>
<a id='n2328' href='#n2328'>2328</a>
<a id='n2329' href='#n2329'>2329</a>
<a id='n2330' href='#n2330'>2330</a>
<a id='n2331' href='#n2331'>2331</a>
<a id='n2332' href='#n2332'>2332</a>
<a id='n2333' href='#n2333'>2333</a>
<a id='n2334' href='#n2334'>2334</a>
<a id='n2335' href='#n2335'>2335</a>
<a id='n2336' href='#n2336'>2336</a>
<a id='n2337' href='#n2337'>2337</a>
<a id='n2338' href='#n2338'>2338</a>
<a id='n2339' href='#n2339'>2339</a>
<a id='n2340' href='#n2340'>2340</a>
<a id='n2341' href='#n2341'>2341</a>
<a id='n2342' href='#n2342'>2342</a>
<a id='n2343' href='#n2343'>2343</a>
<a id='n2344' href='#n2344'>2344</a>
<a id='n2345' href='#n2345'>2345</a>
<a id='n2346' href='#n2346'>2346</a>
<a id='n2347' href='#n2347'>2347</a>
<a id='n2348' href='#n2348'>2348</a>
<a id='n2349' href='#n2349'>2349</a>
<a id='n2350' href='#n2350'>2350</a>
<a id='n2351' href='#n2351'>2351</a>
<a id='n2352' href='#n2352'>2352</a>
<a id='n2353' href='#n2353'>2353</a>
<a id='n2354' href='#n2354'>2354</a>
<a id='n2355' href='#n2355'>2355</a>
<a id='n2356' href='#n2356'>2356</a>
<a id='n2357' href='#n2357'>2357</a>
<a id='n2358' href='#n2358'>2358</a>
<a id='n2359' href='#n2359'>2359</a>
<a id='n2360' href='#n2360'>2360</a>
<a id='n2361' href='#n2361'>2361</a>
<a id='n2362' href='#n2362'>2362</a>
<a id='n2363' href='#n2363'>2363</a>
<a id='n2364' href='#n2364'>2364</a>
<a id='n2365' href='#n2365'>2365</a>
<a id='n2366' href='#n2366'>2366</a>
<a id='n2367' href='#n2367'>2367</a>
<a id='n2368' href='#n2368'>2368</a>
<a id='n2369' href='#n2369'>2369</a>
<a id='n2370' href='#n2370'>2370</a>
<a id='n2371' href='#n2371'>2371</a>
<a id='n2372' href='#n2372'>2372</a>
<a id='n2373' href='#n2373'>2373</a>
<a id='n2374' href='#n2374'>2374</a>
<a id='n2375' href='#n2375'>2375</a>
<a id='n2376' href='#n2376'>2376</a>
<a id='n2377' href='#n2377'>2377</a>
<a id='n2378' href='#n2378'>2378</a>
<a id='n2379' href='#n2379'>2379</a>
<a id='n2380' href='#n2380'>2380</a>
<a id='n2381' href='#n2381'>2381</a>
<a id='n2382' href='#n2382'>2382</a>
<a id='n2383' href='#n2383'>2383</a>
<a id='n2384' href='#n2384'>2384</a>
<a id='n2385' href='#n2385'>2385</a>
<a id='n2386' href='#n2386'>2386</a>
<a id='n2387' href='#n2387'>2387</a>
<a id='n2388' href='#n2388'>2388</a>
<a id='n2389' href='#n2389'>2389</a>
<a id='n2390' href='#n2390'>2390</a>
<a id='n2391' href='#n2391'>2391</a>
<a id='n2392' href='#n2392'>2392</a>
<a id='n2393' href='#n2393'>2393</a>
<a id='n2394' href='#n2394'>2394</a>
<a id='n2395' href='#n2395'>2395</a>
<a id='n2396' href='#n2396'>2396</a>
<a id='n2397' href='#n2397'>2397</a>
<a id='n2398' href='#n2398'>2398</a>
<a id='n2399' href='#n2399'>2399</a>
<a id='n2400' href='#n2400'>2400</a>
<a id='n2401' href='#n2401'>2401</a>
<a id='n2402' href='#n2402'>2402</a>
<a id='n2403' href='#n2403'>2403</a>
<a id='n2404' href='#n2404'>2404</a>
<a id='n2405' href='#n2405'>2405</a>
<a id='n2406' href='#n2406'>2406</a>
<a id='n2407' href='#n2407'>2407</a>
<a id='n2408' href='#n2408'>2408</a>
<a id='n2409' href='#n2409'>2409</a>
<a id='n2410' href='#n2410'>2410</a>
<a id='n2411' href='#n2411'>2411</a>
<a id='n2412' href='#n2412'>2412</a>
<a id='n2413' href='#n2413'>2413</a>
<a id='n2414' href='#n2414'>2414</a>
<a id='n2415' href='#n2415'>2415</a>
<a id='n2416' href='#n2416'>2416</a>
<a id='n2417' href='#n2417'>2417</a>
<a id='n2418' href='#n2418'>2418</a>
<a id='n2419' href='#n2419'>2419</a>
<a id='n2420' href='#n2420'>2420</a>
<a id='n2421' href='#n2421'>2421</a>
<a id='n2422' href='#n2422'>2422</a>
<a id='n2423' href='#n2423'>2423</a>
<a id='n2424' href='#n2424'>2424</a>
<a id='n2425' href='#n2425'>2425</a>
<a id='n2426' href='#n2426'>2426</a>
<a id='n2427' href='#n2427'>2427</a>
<a id='n2428' href='#n2428'>2428</a>
<a id='n2429' href='#n2429'>2429</a>
<a id='n2430' href='#n2430'>2430</a>
<a id='n2431' href='#n2431'>2431</a>
<a id='n2432' href='#n2432'>2432</a>
<a id='n2433' href='#n2433'>2433</a>
<a id='n2434' href='#n2434'>2434</a>
<a id='n2435' href='#n2435'>2435</a>
<a id='n2436' href='#n2436'>2436</a>
<a id='n2437' href='#n2437'>2437</a>
<a id='n2438' href='#n2438'>2438</a>
<a id='n2439' href='#n2439'>2439</a>
<a id='n2440' href='#n2440'>2440</a>
<a id='n2441' href='#n2441'>2441</a>
<a id='n2442' href='#n2442'>2442</a>
<a id='n2443' href='#n2443'>2443</a>
<a id='n2444' href='#n2444'>2444</a>
<a id='n2445' href='#n2445'>2445</a>
<a id='n2446' href='#n2446'>2446</a>
<a id='n2447' href='#n2447'>2447</a>
<a id='n2448' href='#n2448'>2448</a>
<a id='n2449' href='#n2449'>2449</a>
<a id='n2450' href='#n2450'>2450</a>
<a id='n2451' href='#n2451'>2451</a>
<a id='n2452' href='#n2452'>2452</a>
<a id='n2453' href='#n2453'>2453</a>
<a id='n2454' href='#n2454'>2454</a>
<a id='n2455' href='#n2455'>2455</a>
<a id='n2456' href='#n2456'>2456</a>
<a id='n2457' href='#n2457'>2457</a>
<a id='n2458' href='#n2458'>2458</a>
<a id='n2459' href='#n2459'>2459</a>
<a id='n2460' href='#n2460'>2460</a>
<a id='n2461' href='#n2461'>2461</a>
<a id='n2462' href='#n2462'>2462</a>
<a id='n2463' href='#n2463'>2463</a>
<a id='n2464' href='#n2464'>2464</a>
<a id='n2465' href='#n2465'>2465</a>
<a id='n2466' href='#n2466'>2466</a>
<a id='n2467' href='#n2467'>2467</a>
<a id='n2468' href='#n2468'>2468</a>
<a id='n2469' href='#n2469'>2469</a>
<a id='n2470' href='#n2470'>2470</a>
<a id='n2471' href='#n2471'>2471</a>
<a id='n2472' href='#n2472'>2472</a>
<a id='n2473' href='#n2473'>2473</a>
<a id='n2474' href='#n2474'>2474</a>
<a id='n2475' href='#n2475'>2475</a>
<a id='n2476' href='#n2476'>2476</a>
<a id='n2477' href='#n2477'>2477</a>
<a id='n2478' href='#n2478'>2478</a>
<a id='n2479' href='#n2479'>2479</a>
<a id='n2480' href='#n2480'>2480</a>
<a id='n2481' href='#n2481'>2481</a>
<a id='n2482' href='#n2482'>2482</a>
<a id='n2483' href='#n2483'>2483</a>
<a id='n2484' href='#n2484'>2484</a>
<a id='n2485' href='#n2485'>2485</a>
<a id='n2486' href='#n2486'>2486</a>
<a id='n2487' href='#n2487'>2487</a>
<a id='n2488' href='#n2488'>2488</a>
<a id='n2489' href='#n2489'>2489</a>
<a id='n2490' href='#n2490'>2490</a>
<a id='n2491' href='#n2491'>2491</a>
<a id='n2492' href='#n2492'>2492</a>
<a id='n2493' href='#n2493'>2493</a>
<a id='n2494' href='#n2494'>2494</a>
<a id='n2495' href='#n2495'>2495</a>
<a id='n2496' href='#n2496'>2496</a>
<a id='n2497' href='#n2497'>2497</a>
<a id='n2498' href='#n2498'>2498</a>
<a id='n2499' href='#n2499'>2499</a>
<a id='n2500' href='#n2500'>2500</a>
<a id='n2501' href='#n2501'>2501</a>
<a id='n2502' href='#n2502'>2502</a>
<a id='n2503' href='#n2503'>2503</a>
<a id='n2504' href='#n2504'>2504</a>
<a id='n2505' href='#n2505'>2505</a>
<a id='n2506' href='#n2506'>2506</a>
<a id='n2507' href='#n2507'>2507</a>
<a id='n2508' href='#n2508'>2508</a>
<a id='n2509' href='#n2509'>2509</a>
<a id='n2510' href='#n2510'>2510</a>
<a id='n2511' href='#n2511'>2511</a>
<a id='n2512' href='#n2512'>2512</a>
<a id='n2513' href='#n2513'>2513</a>
<a id='n2514' href='#n2514'>2514</a>
<a id='n2515' href='#n2515'>2515</a>
<a id='n2516' href='#n2516'>2516</a>
<a id='n2517' href='#n2517'>2517</a>
<a id='n2518' href='#n2518'>2518</a>
<a id='n2519' href='#n2519'>2519</a>
<a id='n2520' href='#n2520'>2520</a>
<a id='n2521' href='#n2521'>2521</a>
<a id='n2522' href='#n2522'>2522</a>
<a id='n2523' href='#n2523'>2523</a>
<a id='n2524' href='#n2524'>2524</a>
<a id='n2525' href='#n2525'>2525</a>
<a id='n2526' href='#n2526'>2526</a>
<a id='n2527' href='#n2527'>2527</a>
<a id='n2528' href='#n2528'>2528</a>
<a id='n2529' href='#n2529'>2529</a>
<a id='n2530' href='#n2530'>2530</a>
<a id='n2531' href='#n2531'>2531</a>
<a id='n2532' href='#n2532'>2532</a>
<a id='n2533' href='#n2533'>2533</a>
<a id='n2534' href='#n2534'>2534</a>
<a id='n2535' href='#n2535'>2535</a>
<a id='n2536' href='#n2536'>2536</a>
<a id='n2537' href='#n2537'>2537</a>
<a id='n2538' href='#n2538'>2538</a>
<a id='n2539' href='#n2539'>2539</a>
<a id='n2540' href='#n2540'>2540</a>
<a id='n2541' href='#n2541'>2541</a>
<a id='n2542' href='#n2542'>2542</a>
<a id='n2543' href='#n2543'>2543</a>
<a id='n2544' href='#n2544'>2544</a>
<a id='n2545' href='#n2545'>2545</a>
<a id='n2546' href='#n2546'>2546</a>
<a id='n2547' href='#n2547'>2547</a>
<a id='n2548' href='#n2548'>2548</a>
<a id='n2549' href='#n2549'>2549</a>
<a id='n2550' href='#n2550'>2550</a>
<a id='n2551' href='#n2551'>2551</a>
<a id='n2552' href='#n2552'>2552</a>
<a id='n2553' href='#n2553'>2553</a>
<a id='n2554' href='#n2554'>2554</a>
<a id='n2555' href='#n2555'>2555</a>
<a id='n2556' href='#n2556'>2556</a>
<a id='n2557' href='#n2557'>2557</a>
<a id='n2558' href='#n2558'>2558</a>
<a id='n2559' href='#n2559'>2559</a>
<a id='n2560' href='#n2560'>2560</a>
<a id='n2561' href='#n2561'>2561</a>
<a id='n2562' href='#n2562'>2562</a>
<a id='n2563' href='#n2563'>2563</a>
<a id='n2564' href='#n2564'>2564</a>
<a id='n2565' href='#n2565'>2565</a>
<a id='n2566' href='#n2566'>2566</a>
<a id='n2567' href='#n2567'>2567</a>
<a id='n2568' href='#n2568'>2568</a>
<a id='n2569' href='#n2569'>2569</a>
<a id='n2570' href='#n2570'>2570</a>
<a id='n2571' href='#n2571'>2571</a>
<a id='n2572' href='#n2572'>2572</a>
<a id='n2573' href='#n2573'>2573</a>
<a id='n2574' href='#n2574'>2574</a>
<a id='n2575' href='#n2575'>2575</a>
<a id='n2576' href='#n2576'>2576</a>
<a id='n2577' href='#n2577'>2577</a>
<a id='n2578' href='#n2578'>2578</a>
<a id='n2579' href='#n2579'>2579</a>
<a id='n2580' href='#n2580'>2580</a>
<a id='n2581' href='#n2581'>2581</a>
<a id='n2582' href='#n2582'>2582</a>
<a id='n2583' href='#n2583'>2583</a>
<a id='n2584' href='#n2584'>2584</a>
<a id='n2585' href='#n2585'>2585</a>
<a id='n2586' href='#n2586'>2586</a>
<a id='n2587' href='#n2587'>2587</a>
<a id='n2588' href='#n2588'>2588</a>
<a id='n2589' href='#n2589'>2589</a>
<a id='n2590' href='#n2590'>2590</a>
<a id='n2591' href='#n2591'>2591</a>
<a id='n2592' href='#n2592'>2592</a>
<a id='n2593' href='#n2593'>2593</a>
<a id='n2594' href='#n2594'>2594</a>
<a id='n2595' href='#n2595'>2595</a>
<a id='n2596' href='#n2596'>2596</a>
<a id='n2597' href='#n2597'>2597</a>
<a id='n2598' href='#n2598'>2598</a>
<a id='n2599' href='#n2599'>2599</a>
<a id='n2600' href='#n2600'>2600</a>
<a id='n2601' href='#n2601'>2601</a>
<a id='n2602' href='#n2602'>2602</a>
<a id='n2603' href='#n2603'>2603</a>
<a id='n2604' href='#n2604'>2604</a>
<a id='n2605' href='#n2605'>2605</a>
<a id='n2606' href='#n2606'>2606</a>
<a id='n2607' href='#n2607'>2607</a>
<a id='n2608' href='#n2608'>2608</a>
<a id='n2609' href='#n2609'>2609</a>
<a id='n2610' href='#n2610'>2610</a>
<a id='n2611' href='#n2611'>2611</a>
<a id='n2612' href='#n2612'>2612</a>
<a id='n2613' href='#n2613'>2613</a>
<a id='n2614' href='#n2614'>2614</a>
<a id='n2615' href='#n2615'>2615</a>
<a id='n2616' href='#n2616'>2616</a>
<a id='n2617' href='#n2617'>2617</a>
<a id='n2618' href='#n2618'>2618</a>
<a id='n2619' href='#n2619'>2619</a>
<a id='n2620' href='#n2620'>2620</a>
<a id='n2621' href='#n2621'>2621</a>
<a id='n2622' href='#n2622'>2622</a>
<a id='n2623' href='#n2623'>2623</a>
<a id='n2624' href='#n2624'>2624</a>
<a id='n2625' href='#n2625'>2625</a>
<a id='n2626' href='#n2626'>2626</a>
<a id='n2627' href='#n2627'>2627</a>
<a id='n2628' href='#n2628'>2628</a>
<a id='n2629' href='#n2629'>2629</a>
<a id='n2630' href='#n2630'>2630</a>
<a id='n2631' href='#n2631'>2631</a>
<a id='n2632' href='#n2632'>2632</a>
<a id='n2633' href='#n2633'>2633</a>
<a id='n2634' href='#n2634'>2634</a>
<a id='n2635' href='#n2635'>2635</a>
<a id='n2636' href='#n2636'>2636</a>
<a id='n2637' href='#n2637'>2637</a>
<a id='n2638' href='#n2638'>2638</a>
<a id='n2639' href='#n2639'>2639</a>
<a id='n2640' href='#n2640'>2640</a>
<a id='n2641' href='#n2641'>2641</a>
<a id='n2642' href='#n2642'>2642</a>
<a id='n2643' href='#n2643'>2643</a>
<a id='n2644' href='#n2644'>2644</a>
<a id='n2645' href='#n2645'>2645</a>
<a id='n2646' href='#n2646'>2646</a>
<a id='n2647' href='#n2647'>2647</a>
<a id='n2648' href='#n2648'>2648</a>
<a id='n2649' href='#n2649'>2649</a>
<a id='n2650' href='#n2650'>2650</a>
<a id='n2651' href='#n2651'>2651</a>
<a id='n2652' href='#n2652'>2652</a>
<a id='n2653' href='#n2653'>2653</a>
<a id='n2654' href='#n2654'>2654</a>
<a id='n2655' href='#n2655'>2655</a>
<a id='n2656' href='#n2656'>2656</a>
<a id='n2657' href='#n2657'>2657</a>
<a id='n2658' href='#n2658'>2658</a>
<a id='n2659' href='#n2659'>2659</a>
<a id='n2660' href='#n2660'>2660</a>
<a id='n2661' href='#n2661'>2661</a>
<a id='n2662' href='#n2662'>2662</a>
<a id='n2663' href='#n2663'>2663</a>
<a id='n2664' href='#n2664'>2664</a>
<a id='n2665' href='#n2665'>2665</a>
<a id='n2666' href='#n2666'>2666</a>
<a id='n2667' href='#n2667'>2667</a>
<a id='n2668' href='#n2668'>2668</a>
<a id='n2669' href='#n2669'>2669</a>
<a id='n2670' href='#n2670'>2670</a>
<a id='n2671' href='#n2671'>2671</a>
<a id='n2672' href='#n2672'>2672</a>
<a id='n2673' href='#n2673'>2673</a>
<a id='n2674' href='#n2674'>2674</a>
<a id='n2675' href='#n2675'>2675</a>
<a id='n2676' href='#n2676'>2676</a>
<a id='n2677' href='#n2677'>2677</a>
<a id='n2678' href='#n2678'>2678</a>
<a id='n2679' href='#n2679'>2679</a>
<a id='n2680' href='#n2680'>2680</a>
<a id='n2681' href='#n2681'>2681</a>
<a id='n2682' href='#n2682'>2682</a>
<a id='n2683' href='#n2683'>2683</a>
<a id='n2684' href='#n2684'>2684</a>
<a id='n2685' href='#n2685'>2685</a>
<a id='n2686' href='#n2686'>2686</a>
<a id='n2687' href='#n2687'>2687</a>
<a id='n2688' href='#n2688'>2688</a>
<a id='n2689' href='#n2689'>2689</a>
<a id='n2690' href='#n2690'>2690</a>
<a id='n2691' href='#n2691'>2691</a>
<a id='n2692' href='#n2692'>2692</a>
<a id='n2693' href='#n2693'>2693</a>
<a id='n2694' href='#n2694'>2694</a>
<a id='n2695' href='#n2695'>2695</a>
<a id='n2696' href='#n2696'>2696</a>
<a id='n2697' href='#n2697'>2697</a>
<a id='n2698' href='#n2698'>2698</a>
<a id='n2699' href='#n2699'>2699</a>
<a id='n2700' href='#n2700'>2700</a>
<a id='n2701' href='#n2701'>2701</a>
<a id='n2702' href='#n2702'>2702</a>
<a id='n2703' href='#n2703'>2703</a>
<a id='n2704' href='#n2704'>2704</a>
<a id='n2705' href='#n2705'>2705</a>
<a id='n2706' href='#n2706'>2706</a>
<a id='n2707' href='#n2707'>2707</a>
<a id='n2708' href='#n2708'>2708</a>
<a id='n2709' href='#n2709'>2709</a>
<a id='n2710' href='#n2710'>2710</a>
<a id='n2711' href='#n2711'>2711</a>
<a id='n2712' href='#n2712'>2712</a>
<a id='n2713' href='#n2713'>2713</a>
<a id='n2714' href='#n2714'>2714</a>
<a id='n2715' href='#n2715'>2715</a>
<a id='n2716' href='#n2716'>2716</a>
<a id='n2717' href='#n2717'>2717</a>
<a id='n2718' href='#n2718'>2718</a>
<a id='n2719' href='#n2719'>2719</a>
<a id='n2720' href='#n2720'>2720</a>
<a id='n2721' href='#n2721'>2721</a>
<a id='n2722' href='#n2722'>2722</a>
<a id='n2723' href='#n2723'>2723</a>
<a id='n2724' href='#n2724'>2724</a>
<a id='n2725' href='#n2725'>2725</a>
<a id='n2726' href='#n2726'>2726</a>
<a id='n2727' href='#n2727'>2727</a>
<a id='n2728' href='#n2728'>2728</a>
<a id='n2729' href='#n2729'>2729</a>
<a id='n2730' href='#n2730'>2730</a>
<a id='n2731' href='#n2731'>2731</a>
<a id='n2732' href='#n2732'>2732</a>
<a id='n2733' href='#n2733'>2733</a>
<a id='n2734' href='#n2734'>2734</a>
<a id='n2735' href='#n2735'>2735</a>
<a id='n2736' href='#n2736'>2736</a>
<a id='n2737' href='#n2737'>2737</a>
<a id='n2738' href='#n2738'>2738</a>
<a id='n2739' href='#n2739'>2739</a>
<a id='n2740' href='#n2740'>2740</a>
<a id='n2741' href='#n2741'>2741</a>
<a id='n2742' href='#n2742'>2742</a>
<a id='n2743' href='#n2743'>2743</a>
<a id='n2744' href='#n2744'>2744</a>
<a id='n2745' href='#n2745'>2745</a>
<a id='n2746' href='#n2746'>2746</a>
<a id='n2747' href='#n2747'>2747</a>
<a id='n2748' href='#n2748'>2748</a>
<a id='n2749' href='#n2749'>2749</a>
<a id='n2750' href='#n2750'>2750</a>
<a id='n2751' href='#n2751'>2751</a>
<a id='n2752' href='#n2752'>2752</a>
<a id='n2753' href='#n2753'>2753</a>
<a id='n2754' href='#n2754'>2754</a>
<a id='n2755' href='#n2755'>2755</a>
<a id='n2756' href='#n2756'>2756</a>
<a id='n2757' href='#n2757'>2757</a>
<a id='n2758' href='#n2758'>2758</a>
<a id='n2759' href='#n2759'>2759</a>
<a id='n2760' href='#n2760'>2760</a>
<a id='n2761' href='#n2761'>2761</a>
<a id='n2762' href='#n2762'>2762</a>
<a id='n2763' href='#n2763'>2763</a>
<a id='n2764' href='#n2764'>2764</a>
<a id='n2765' href='#n2765'>2765</a>
<a id='n2766' href='#n2766'>2766</a>
<a id='n2767' href='#n2767'>2767</a>
<a id='n2768' href='#n2768'>2768</a>
<a id='n2769' href='#n2769'>2769</a>
<a id='n2770' href='#n2770'>2770</a>
<a id='n2771' href='#n2771'>2771</a>
<a id='n2772' href='#n2772'>2772</a>
<a id='n2773' href='#n2773'>2773</a>
<a id='n2774' href='#n2774'>2774</a>
<a id='n2775' href='#n2775'>2775</a>
<a id='n2776' href='#n2776'>2776</a>
<a id='n2777' href='#n2777'>2777</a>
<a id='n2778' href='#n2778'>2778</a>
<a id='n2779' href='#n2779'>2779</a>
<a id='n2780' href='#n2780'>2780</a>
<a id='n2781' href='#n2781'>2781</a>
<a id='n2782' href='#n2782'>2782</a>
<a id='n2783' href='#n2783'>2783</a>
<a id='n2784' href='#n2784'>2784</a>
<a id='n2785' href='#n2785'>2785</a>
<a id='n2786' href='#n2786'>2786</a>
<a id='n2787' href='#n2787'>2787</a>
<a id='n2788' href='#n2788'>2788</a>
<a id='n2789' href='#n2789'>2789</a>
<a id='n2790' href='#n2790'>2790</a>
<a id='n2791' href='#n2791'>2791</a>
<a id='n2792' href='#n2792'>2792</a>
<a id='n2793' href='#n2793'>2793</a>
<a id='n2794' href='#n2794'>2794</a>
<a id='n2795' href='#n2795'>2795</a>
<a id='n2796' href='#n2796'>2796</a>
<a id='n2797' href='#n2797'>2797</a>
<a id='n2798' href='#n2798'>2798</a>
<a id='n2799' href='#n2799'>2799</a>
<a id='n2800' href='#n2800'>2800</a>
<a id='n2801' href='#n2801'>2801</a>
<a id='n2802' href='#n2802'>2802</a>
<a id='n2803' href='#n2803'>2803</a>
<a id='n2804' href='#n2804'>2804</a>
<a id='n2805' href='#n2805'>2805</a>
<a id='n2806' href='#n2806'>2806</a>
<a id='n2807' href='#n2807'>2807</a>
<a id='n2808' href='#n2808'>2808</a>
<a id='n2809' href='#n2809'>2809</a>
<a id='n2810' href='#n2810'>2810</a>
<a id='n2811' href='#n2811'>2811</a>
<a id='n2812' href='#n2812'>2812</a>
<a id='n2813' href='#n2813'>2813</a>
<a id='n2814' href='#n2814'>2814</a>
<a id='n2815' href='#n2815'>2815</a>
<a id='n2816' href='#n2816'>2816</a>
<a id='n2817' href='#n2817'>2817</a>
<a id='n2818' href='#n2818'>2818</a>
<a id='n2819' href='#n2819'>2819</a>
<a id='n2820' href='#n2820'>2820</a>
<a id='n2821' href='#n2821'>2821</a>
<a id='n2822' href='#n2822'>2822</a>
<a id='n2823' href='#n2823'>2823</a>
<a id='n2824' href='#n2824'>2824</a>
<a id='n2825' href='#n2825'>2825</a>
<a id='n2826' href='#n2826'>2826</a>
<a id='n2827' href='#n2827'>2827</a>
<a id='n2828' href='#n2828'>2828</a>
<a id='n2829' href='#n2829'>2829</a>
<a id='n2830' href='#n2830'>2830</a>
<a id='n2831' href='#n2831'>2831</a>
<a id='n2832' href='#n2832'>2832</a>
<a id='n2833' href='#n2833'>2833</a>
<a id='n2834' href='#n2834'>2834</a>
<a id='n2835' href='#n2835'>2835</a>
<a id='n2836' href='#n2836'>2836</a>
<a id='n2837' href='#n2837'>2837</a>
<a id='n2838' href='#n2838'>2838</a>
<a id='n2839' href='#n2839'>2839</a>
<a id='n2840' href='#n2840'>2840</a>
<a id='n2841' href='#n2841'>2841</a>
<a id='n2842' href='#n2842'>2842</a>
<a id='n2843' href='#n2843'>2843</a>
<a id='n2844' href='#n2844'>2844</a>
<a id='n2845' href='#n2845'>2845</a>
<a id='n2846' href='#n2846'>2846</a>
<a id='n2847' href='#n2847'>2847</a>
<a id='n2848' href='#n2848'>2848</a>
<a id='n2849' href='#n2849'>2849</a>
<a id='n2850' href='#n2850'>2850</a>
<a id='n2851' href='#n2851'>2851</a>
<a id='n2852' href='#n2852'>2852</a>
<a id='n2853' href='#n2853'>2853</a>
<a id='n2854' href='#n2854'>2854</a>
<a id='n2855' href='#n2855'>2855</a>
<a id='n2856' href='#n2856'>2856</a>
<a id='n2857' href='#n2857'>2857</a>
<a id='n2858' href='#n2858'>2858</a>
<a id='n2859' href='#n2859'>2859</a>
<a id='n2860' href='#n2860'>2860</a>
<a id='n2861' href='#n2861'>2861</a>
<a id='n2862' href='#n2862'>2862</a>
<a id='n2863' href='#n2863'>2863</a>
<a id='n2864' href='#n2864'>2864</a>
<a id='n2865' href='#n2865'>2865</a>
<a id='n2866' href='#n2866'>2866</a>
<a id='n2867' href='#n2867'>2867</a>
<a id='n2868' href='#n2868'>2868</a>
<a id='n2869' href='#n2869'>2869</a>
<a id='n2870' href='#n2870'>2870</a>
<a id='n2871' href='#n2871'>2871</a>
<a id='n2872' href='#n2872'>2872</a>
<a id='n2873' href='#n2873'>2873</a>
<a id='n2874' href='#n2874'>2874</a>
<a id='n2875' href='#n2875'>2875</a>
<a id='n2876' href='#n2876'>2876</a>
<a id='n2877' href='#n2877'>2877</a>
<a id='n2878' href='#n2878'>2878</a>
<a id='n2879' href='#n2879'>2879</a>
<a id='n2880' href='#n2880'>2880</a>
<a id='n2881' href='#n2881'>2881</a>
<a id='n2882' href='#n2882'>2882</a>
<a id='n2883' href='#n2883'>2883</a>
<a id='n2884' href='#n2884'>2884</a>
<a id='n2885' href='#n2885'>2885</a>
<a id='n2886' href='#n2886'>2886</a>
<a id='n2887' href='#n2887'>2887</a>
<a id='n2888' href='#n2888'>2888</a>
<a id='n2889' href='#n2889'>2889</a>
<a id='n2890' href='#n2890'>2890</a>
<a id='n2891' href='#n2891'>2891</a>
<a id='n2892' href='#n2892'>2892</a>
<a id='n2893' href='#n2893'>2893</a>
<a id='n2894' href='#n2894'>2894</a>
<a id='n2895' href='#n2895'>2895</a>
<a id='n2896' href='#n2896'>2896</a>
<a id='n2897' href='#n2897'>2897</a>
<a id='n2898' href='#n2898'>2898</a>
<a id='n2899' href='#n2899'>2899</a>
<a id='n2900' href='#n2900'>2900</a>
<a id='n2901' href='#n2901'>2901</a>
<a id='n2902' href='#n2902'>2902</a>
<a id='n2903' href='#n2903'>2903</a>
<a id='n2904' href='#n2904'>2904</a>
<a id='n2905' href='#n2905'>2905</a>
<a id='n2906' href='#n2906'>2906</a>
<a id='n2907' href='#n2907'>2907</a>
<a id='n2908' href='#n2908'>2908</a>
<a id='n2909' href='#n2909'>2909</a>
<a id='n2910' href='#n2910'>2910</a>
<a id='n2911' href='#n2911'>2911</a>
<a id='n2912' href='#n2912'>2912</a>
<a id='n2913' href='#n2913'>2913</a>
<a id='n2914' href='#n2914'>2914</a>
<a id='n2915' href='#n2915'>2915</a>
<a id='n2916' href='#n2916'>2916</a>
<a id='n2917' href='#n2917'>2917</a>
<a id='n2918' href='#n2918'>2918</a>
<a id='n2919' href='#n2919'>2919</a>
<a id='n2920' href='#n2920'>2920</a>
<a id='n2921' href='#n2921'>2921</a>
<a id='n2922' href='#n2922'>2922</a>
<a id='n2923' href='#n2923'>2923</a>
<a id='n2924' href='#n2924'>2924</a>
<a id='n2925' href='#n2925'>2925</a>
<a id='n2926' href='#n2926'>2926</a>
<a id='n2927' href='#n2927'>2927</a>
<a id='n2928' href='#n2928'>2928</a>
<a id='n2929' href='#n2929'>2929</a>
<a id='n2930' href='#n2930'>2930</a>
<a id='n2931' href='#n2931'>2931</a>
<a id='n2932' href='#n2932'>2932</a>
<a id='n2933' href='#n2933'>2933</a>
<a id='n2934' href='#n2934'>2934</a>
<a id='n2935' href='#n2935'>2935</a>
<a id='n2936' href='#n2936'>2936</a>
<a id='n2937' href='#n2937'>2937</a>
<a id='n2938' href='#n2938'>2938</a>
<a id='n2939' href='#n2939'>2939</a>
<a id='n2940' href='#n2940'>2940</a>
<a id='n2941' href='#n2941'>2941</a>
<a id='n2942' href='#n2942'>2942</a>
<a id='n2943' href='#n2943'>2943</a>
<a id='n2944' href='#n2944'>2944</a>
<a id='n2945' href='#n2945'>2945</a>
<a id='n2946' href='#n2946'>2946</a>
<a id='n2947' href='#n2947'>2947</a>
<a id='n2948' href='#n2948'>2948</a>
<a id='n2949' href='#n2949'>2949</a>
<a id='n2950' href='#n2950'>2950</a>
<a id='n2951' href='#n2951'>2951</a>
<a id='n2952' href='#n2952'>2952</a>
<a id='n2953' href='#n2953'>2953</a>
<a id='n2954' href='#n2954'>2954</a>
<a id='n2955' href='#n2955'>2955</a>
<a id='n2956' href='#n2956'>2956</a>
<a id='n2957' href='#n2957'>2957</a>
<a id='n2958' href='#n2958'>2958</a>
<a id='n2959' href='#n2959'>2959</a>
<a id='n2960' href='#n2960'>2960</a>
<a id='n2961' href='#n2961'>2961</a>
<a id='n2962' href='#n2962'>2962</a>
<a id='n2963' href='#n2963'>2963</a>
<a id='n2964' href='#n2964'>2964</a>
<a id='n2965' href='#n2965'>2965</a>
<a id='n2966' href='#n2966'>2966</a>
<a id='n2967' href='#n2967'>2967</a>
<a id='n2968' href='#n2968'>2968</a>
<a id='n2969' href='#n2969'>2969</a>
<a id='n2970' href='#n2970'>2970</a>
<a id='n2971' href='#n2971'>2971</a>
<a id='n2972' href='#n2972'>2972</a>
<a id='n2973' href='#n2973'>2973</a>
<a id='n2974' href='#n2974'>2974</a>
<a id='n2975' href='#n2975'>2975</a>
<a id='n2976' href='#n2976'>2976</a>
<a id='n2977' href='#n2977'>2977</a>
<a id='n2978' href='#n2978'>2978</a>
<a id='n2979' href='#n2979'>2979</a>
<a id='n2980' href='#n2980'>2980</a>
<a id='n2981' href='#n2981'>2981</a>
<a id='n2982' href='#n2982'>2982</a>
<a id='n2983' href='#n2983'>2983</a>
<a id='n2984' href='#n2984'>2984</a>
<a id='n2985' href='#n2985'>2985</a>
<a id='n2986' href='#n2986'>2986</a>
<a id='n2987' href='#n2987'>2987</a>
<a id='n2988' href='#n2988'>2988</a>
<a id='n2989' href='#n2989'>2989</a>
<a id='n2990' href='#n2990'>2990</a>
<a id='n2991' href='#n2991'>2991</a>
<a id='n2992' href='#n2992'>2992</a>
<a id='n2993' href='#n2993'>2993</a>
<a id='n2994' href='#n2994'>2994</a>
<a id='n2995' href='#n2995'>2995</a>
<a id='n2996' href='#n2996'>2996</a>
<a id='n2997' href='#n2997'>2997</a>
<a id='n2998' href='#n2998'>2998</a>
<a id='n2999' href='#n2999'>2999</a>
<a id='n3000' href='#n3000'>3000</a>
<a id='n3001' href='#n3001'>3001</a>
<a id='n3002' href='#n3002'>3002</a>
<a id='n3003' href='#n3003'>3003</a>
<a id='n3004' href='#n3004'>3004</a>
<a id='n3005' href='#n3005'>3005</a>
<a id='n3006' href='#n3006'>3006</a>
<a id='n3007' href='#n3007'>3007</a>
<a id='n3008' href='#n3008'>3008</a>
<a id='n3009' href='#n3009'>3009</a>
<a id='n3010' href='#n3010'>3010</a>
<a id='n3011' href='#n3011'>3011</a>
<a id='n3012' href='#n3012'>3012</a>
<a id='n3013' href='#n3013'>3013</a>
<a id='n3014' href='#n3014'>3014</a>
<a id='n3015' href='#n3015'>3015</a>
<a id='n3016' href='#n3016'>3016</a>
<a id='n3017' href='#n3017'>3017</a>
<a id='n3018' href='#n3018'>3018</a>
<a id='n3019' href='#n3019'>3019</a>
<a id='n3020' href='#n3020'>3020</a>
<a id='n3021' href='#n3021'>3021</a>
<a id='n3022' href='#n3022'>3022</a>
<a id='n3023' href='#n3023'>3023</a>
<a id='n3024' href='#n3024'>3024</a>
<a id='n3025' href='#n3025'>3025</a>
<a id='n3026' href='#n3026'>3026</a>
<a id='n3027' href='#n3027'>3027</a>
<a id='n3028' href='#n3028'>3028</a>
<a id='n3029' href='#n3029'>3029</a>
<a id='n3030' href='#n3030'>3030</a>
<a id='n3031' href='#n3031'>3031</a>
<a id='n3032' href='#n3032'>3032</a>
<a id='n3033' href='#n3033'>3033</a>
<a id='n3034' href='#n3034'>3034</a>
<a id='n3035' href='#n3035'>3035</a>
<a id='n3036' href='#n3036'>3036</a>
<a id='n3037' href='#n3037'>3037</a>
<a id='n3038' href='#n3038'>3038</a>
<a id='n3039' href='#n3039'>3039</a>
<a id='n3040' href='#n3040'>3040</a>
<a id='n3041' href='#n3041'>3041</a>
<a id='n3042' href='#n3042'>3042</a>
<a id='n3043' href='#n3043'>3043</a>
<a id='n3044' href='#n3044'>3044</a>
<a id='n3045' href='#n3045'>3045</a>
<a id='n3046' href='#n3046'>3046</a>
<a id='n3047' href='#n3047'>3047</a>
<a id='n3048' href='#n3048'>3048</a>
<a id='n3049' href='#n3049'>3049</a>
<a id='n3050' href='#n3050'>3050</a>
<a id='n3051' href='#n3051'>3051</a>
<a id='n3052' href='#n3052'>3052</a>
<a id='n3053' href='#n3053'>3053</a>
<a id='n3054' href='#n3054'>3054</a>
<a id='n3055' href='#n3055'>3055</a>
<a id='n3056' href='#n3056'>3056</a>
<a id='n3057' href='#n3057'>3057</a>
<a id='n3058' href='#n3058'>3058</a>
<a id='n3059' href='#n3059'>3059</a>
<a id='n3060' href='#n3060'>3060</a>
<a id='n3061' href='#n3061'>3061</a>
<a id='n3062' href='#n3062'>3062</a>
<a id='n3063' href='#n3063'>3063</a>
<a id='n3064' href='#n3064'>3064</a>
<a id='n3065' href='#n3065'>3065</a>
<a id='n3066' href='#n3066'>3066</a>
<a id='n3067' href='#n3067'>3067</a>
<a id='n3068' href='#n3068'>3068</a>
<a id='n3069' href='#n3069'>3069</a>
<a id='n3070' href='#n3070'>3070</a>
<a id='n3071' href='#n3071'>3071</a>
<a id='n3072' href='#n3072'>3072</a>
<a id='n3073' href='#n3073'>3073</a>
<a id='n3074' href='#n3074'>3074</a>
<a id='n3075' href='#n3075'>3075</a>
<a id='n3076' href='#n3076'>3076</a>
<a id='n3077' href='#n3077'>3077</a>
<a id='n3078' href='#n3078'>3078</a>
<a id='n3079' href='#n3079'>3079</a>
<a id='n3080' href='#n3080'>3080</a>
<a id='n3081' href='#n3081'>3081</a>
<a id='n3082' href='#n3082'>3082</a>
<a id='n3083' href='#n3083'>3083</a>
<a id='n3084' href='#n3084'>3084</a>
<a id='n3085' href='#n3085'>3085</a>
<a id='n3086' href='#n3086'>3086</a>
<a id='n3087' href='#n3087'>3087</a>
<a id='n3088' href='#n3088'>3088</a>
<a id='n3089' href='#n3089'>3089</a>
<a id='n3090' href='#n3090'>3090</a>
<a id='n3091' href='#n3091'>3091</a>
<a id='n3092' href='#n3092'>3092</a>
<a id='n3093' href='#n3093'>3093</a>
<a id='n3094' href='#n3094'>3094</a>
<a id='n3095' href='#n3095'>3095</a>
<a id='n3096' href='#n3096'>3096</a>
<a id='n3097' href='#n3097'>3097</a>
<a id='n3098' href='#n3098'>3098</a>
<a id='n3099' href='#n3099'>3099</a>
<a id='n3100' href='#n3100'>3100</a>
<a id='n3101' href='#n3101'>3101</a>
<a id='n3102' href='#n3102'>3102</a>
<a id='n3103' href='#n3103'>3103</a>
<a id='n3104' href='#n3104'>3104</a>
<a id='n3105' href='#n3105'>3105</a>
<a id='n3106' href='#n3106'>3106</a>
<a id='n3107' href='#n3107'>3107</a>
<a id='n3108' href='#n3108'>3108</a>
<a id='n3109' href='#n3109'>3109</a>
<a id='n3110' href='#n3110'>3110</a>
<a id='n3111' href='#n3111'>3111</a>
<a id='n3112' href='#n3112'>3112</a>
<a id='n3113' href='#n3113'>3113</a>
<a id='n3114' href='#n3114'>3114</a>
<a id='n3115' href='#n3115'>3115</a>
<a id='n3116' href='#n3116'>3116</a>
<a id='n3117' href='#n3117'>3117</a>
<a id='n3118' href='#n3118'>3118</a>
<a id='n3119' href='#n3119'>3119</a>
<a id='n3120' href='#n3120'>3120</a>
<a id='n3121' href='#n3121'>3121</a>
<a id='n3122' href='#n3122'>3122</a>
<a id='n3123' href='#n3123'>3123</a>
<a id='n3124' href='#n3124'>3124</a>
<a id='n3125' href='#n3125'>3125</a>
<a id='n3126' href='#n3126'>3126</a>
<a id='n3127' href='#n3127'>3127</a>
<a id='n3128' href='#n3128'>3128</a>
<a id='n3129' href='#n3129'>3129</a>
<a id='n3130' href='#n3130'>3130</a>
<a id='n3131' href='#n3131'>3131</a>
<a id='n3132' href='#n3132'>3132</a>
<a id='n3133' href='#n3133'>3133</a>
<a id='n3134' href='#n3134'>3134</a>
<a id='n3135' href='#n3135'>3135</a>
<a id='n3136' href='#n3136'>3136</a>
<a id='n3137' href='#n3137'>3137</a>
<a id='n3138' href='#n3138'>3138</a>
<a id='n3139' href='#n3139'>3139</a>
<a id='n3140' href='#n3140'>3140</a>
<a id='n3141' href='#n3141'>3141</a>
<a id='n3142' href='#n3142'>3142</a>
<a id='n3143' href='#n3143'>3143</a>
<a id='n3144' href='#n3144'>3144</a>
<a id='n3145' href='#n3145'>3145</a>
<a id='n3146' href='#n3146'>3146</a>
<a id='n3147' href='#n3147'>3147</a>
<a id='n3148' href='#n3148'>3148</a>
<a id='n3149' href='#n3149'>3149</a>
<a id='n3150' href='#n3150'>3150</a>
<a id='n3151' href='#n3151'>3151</a>
<a id='n3152' href='#n3152'>3152</a>
<a id='n3153' href='#n3153'>3153</a>
<a id='n3154' href='#n3154'>3154</a>
<a id='n3155' href='#n3155'>3155</a>
<a id='n3156' href='#n3156'>3156</a>
<a id='n3157' href='#n3157'>3157</a>
<a id='n3158' href='#n3158'>3158</a>
<a id='n3159' href='#n3159'>3159</a>
<a id='n3160' href='#n3160'>3160</a>
<a id='n3161' href='#n3161'>3161</a>
<a id='n3162' href='#n3162'>3162</a>
<a id='n3163' href='#n3163'>3163</a>
<a id='n3164' href='#n3164'>3164</a>
<a id='n3165' href='#n3165'>3165</a>
<a id='n3166' href='#n3166'>3166</a>
<a id='n3167' href='#n3167'>3167</a>
<a id='n3168' href='#n3168'>3168</a>
<a id='n3169' href='#n3169'>3169</a>
<a id='n3170' href='#n3170'>3170</a>
<a id='n3171' href='#n3171'>3171</a>
<a id='n3172' href='#n3172'>3172</a>
<a id='n3173' href='#n3173'>3173</a>
<a id='n3174' href='#n3174'>3174</a>
<a id='n3175' href='#n3175'>3175</a>
<a id='n3176' href='#n3176'>3176</a>
<a id='n3177' href='#n3177'>3177</a>
<a id='n3178' href='#n3178'>3178</a>
<a id='n3179' href='#n3179'>3179</a>
<a id='n3180' href='#n3180'>3180</a>
<a id='n3181' href='#n3181'>3181</a>
<a id='n3182' href='#n3182'>3182</a>
<a id='n3183' href='#n3183'>3183</a>
<a id='n3184' href='#n3184'>3184</a>
<a id='n3185' href='#n3185'>3185</a>
<a id='n3186' href='#n3186'>3186</a>
<a id='n3187' href='#n3187'>3187</a>
<a id='n3188' href='#n3188'>3188</a>
<a id='n3189' href='#n3189'>3189</a>
<a id='n3190' href='#n3190'>3190</a>
<a id='n3191' href='#n3191'>3191</a>
<a id='n3192' href='#n3192'>3192</a>
<a id='n3193' href='#n3193'>3193</a>
<a id='n3194' href='#n3194'>3194</a>
<a id='n3195' href='#n3195'>3195</a>
<a id='n3196' href='#n3196'>3196</a>
<a id='n3197' href='#n3197'>3197</a>
<a id='n3198' href='#n3198'>3198</a>
<a id='n3199' href='#n3199'>3199</a>
<a id='n3200' href='#n3200'>3200</a>
<a id='n3201' href='#n3201'>3201</a>
<a id='n3202' href='#n3202'>3202</a>
<a id='n3203' href='#n3203'>3203</a>
<a id='n3204' href='#n3204'>3204</a>
<a id='n3205' href='#n3205'>3205</a>
<a id='n3206' href='#n3206'>3206</a>
<a id='n3207' href='#n3207'>3207</a>
<a id='n3208' href='#n3208'>3208</a>
<a id='n3209' href='#n3209'>3209</a>
<a id='n3210' href='#n3210'>3210</a>
<a id='n3211' href='#n3211'>3211</a>
<a id='n3212' href='#n3212'>3212</a>
<a id='n3213' href='#n3213'>3213</a>
<a id='n3214' href='#n3214'>3214</a>
<a id='n3215' href='#n3215'>3215</a>
<a id='n3216' href='#n3216'>3216</a>
<a id='n3217' href='#n3217'>3217</a>
<a id='n3218' href='#n3218'>3218</a>
<a id='n3219' href='#n3219'>3219</a>
<a id='n3220' href='#n3220'>3220</a>
<a id='n3221' href='#n3221'>3221</a>
<a id='n3222' href='#n3222'>3222</a>
<a id='n3223' href='#n3223'>3223</a>
<a id='n3224' href='#n3224'>3224</a>
<a id='n3225' href='#n3225'>3225</a>
<a id='n3226' href='#n3226'>3226</a>
<a id='n3227' href='#n3227'>3227</a>
<a id='n3228' href='#n3228'>3228</a>
<a id='n3229' href='#n3229'>3229</a>
<a id='n3230' href='#n3230'>3230</a>
<a id='n3231' href='#n3231'>3231</a>
<a id='n3232' href='#n3232'>3232</a>
<a id='n3233' href='#n3233'>3233</a>
<a id='n3234' href='#n3234'>3234</a>
<a id='n3235' href='#n3235'>3235</a>
<a id='n3236' href='#n3236'>3236</a>
<a id='n3237' href='#n3237'>3237</a>
<a id='n3238' href='#n3238'>3238</a>
<a id='n3239' href='#n3239'>3239</a>
<a id='n3240' href='#n3240'>3240</a>
<a id='n3241' href='#n3241'>3241</a>
<a id='n3242' href='#n3242'>3242</a>
<a id='n3243' href='#n3243'>3243</a>
<a id='n3244' href='#n3244'>3244</a>
<a id='n3245' href='#n3245'>3245</a>
<a id='n3246' href='#n3246'>3246</a>
<a id='n3247' href='#n3247'>3247</a>
<a id='n3248' href='#n3248'>3248</a>
<a id='n3249' href='#n3249'>3249</a>
<a id='n3250' href='#n3250'>3250</a>
<a id='n3251' href='#n3251'>3251</a>
<a id='n3252' href='#n3252'>3252</a>
<a id='n3253' href='#n3253'>3253</a>
<a id='n3254' href='#n3254'>3254</a>
<a id='n3255' href='#n3255'>3255</a>
<a id='n3256' href='#n3256'>3256</a>
<a id='n3257' href='#n3257'>3257</a>
<a id='n3258' href='#n3258'>3258</a>
<a id='n3259' href='#n3259'>3259</a>
<a id='n3260' href='#n3260'>3260</a>
<a id='n3261' href='#n3261'>3261</a>
<a id='n3262' href='#n3262'>3262</a>
<a id='n3263' href='#n3263'>3263</a>
<a id='n3264' href='#n3264'>3264</a>
<a id='n3265' href='#n3265'>3265</a>
<a id='n3266' href='#n3266'>3266</a>
<a id='n3267' href='#n3267'>3267</a>
<a id='n3268' href='#n3268'>3268</a>
<a id='n3269' href='#n3269'>3269</a>
<a id='n3270' href='#n3270'>3270</a>
<a id='n3271' href='#n3271'>3271</a>
<a id='n3272' href='#n3272'>3272</a>
<a id='n3273' href='#n3273'>3273</a>
<a id='n3274' href='#n3274'>3274</a>
<a id='n3275' href='#n3275'>3275</a>
<a id='n3276' href='#n3276'>3276</a>
<a id='n3277' href='#n3277'>3277</a>
<a id='n3278' href='#n3278'>3278</a>
<a id='n3279' href='#n3279'>3279</a>
<a id='n3280' href='#n3280'>3280</a>
<a id='n3281' href='#n3281'>3281</a>
<a id='n3282' href='#n3282'>3282</a>
<a id='n3283' href='#n3283'>3283</a>
<a id='n3284' href='#n3284'>3284</a>
<a id='n3285' href='#n3285'>3285</a>
<a id='n3286' href='#n3286'>3286</a>
<a id='n3287' href='#n3287'>3287</a>
<a id='n3288' href='#n3288'>3288</a>
<a id='n3289' href='#n3289'>3289</a>
<a id='n3290' href='#n3290'>3290</a>
<a id='n3291' href='#n3291'>3291</a>
<a id='n3292' href='#n3292'>3292</a>
<a id='n3293' href='#n3293'>3293</a>
<a id='n3294' href='#n3294'>3294</a>
<a id='n3295' href='#n3295'>3295</a>
<a id='n3296' href='#n3296'>3296</a>
<a id='n3297' href='#n3297'>3297</a>
<a id='n3298' href='#n3298'>3298</a>
<a id='n3299' href='#n3299'>3299</a>
<a id='n3300' href='#n3300'>3300</a>
<a id='n3301' href='#n3301'>3301</a>
<a id='n3302' href='#n3302'>3302</a>
<a id='n3303' href='#n3303'>3303</a>
<a id='n3304' href='#n3304'>3304</a>
<a id='n3305' href='#n3305'>3305</a>
<a id='n3306' href='#n3306'>3306</a>
<a id='n3307' href='#n3307'>3307</a>
<a id='n3308' href='#n3308'>3308</a>
<a id='n3309' href='#n3309'>3309</a>
<a id='n3310' href='#n3310'>3310</a>
<a id='n3311' href='#n3311'>3311</a>
<a id='n3312' href='#n3312'>3312</a>
<a id='n3313' href='#n3313'>3313</a>
<a id='n3314' href='#n3314'>3314</a>
<a id='n3315' href='#n3315'>3315</a>
<a id='n3316' href='#n3316'>3316</a>
<a id='n3317' href='#n3317'>3317</a>
<a id='n3318' href='#n3318'>3318</a>
<a id='n3319' href='#n3319'>3319</a>
<a id='n3320' href='#n3320'>3320</a>
<a id='n3321' href='#n3321'>3321</a>
<a id='n3322' href='#n3322'>3322</a>
<a id='n3323' href='#n3323'>3323</a>
<a id='n3324' href='#n3324'>3324</a>
<a id='n3325' href='#n3325'>3325</a>
<a id='n3326' href='#n3326'>3326</a>
<a id='n3327' href='#n3327'>3327</a>
<a id='n3328' href='#n3328'>3328</a>
<a id='n3329' href='#n3329'>3329</a>
<a id='n3330' href='#n3330'>3330</a>
<a id='n3331' href='#n3331'>3331</a>
<a id='n3332' href='#n3332'>3332</a>
<a id='n3333' href='#n3333'>3333</a>
<a id='n3334' href='#n3334'>3334</a>
<a id='n3335' href='#n3335'>3335</a>
<a id='n3336' href='#n3336'>3336</a>
<a id='n3337' href='#n3337'>3337</a>
<a id='n3338' href='#n3338'>3338</a>
<a id='n3339' href='#n3339'>3339</a>
<a id='n3340' href='#n3340'>3340</a>
<a id='n3341' href='#n3341'>3341</a>
<a id='n3342' href='#n3342'>3342</a>
<a id='n3343' href='#n3343'>3343</a>
<a id='n3344' href='#n3344'>3344</a>
<a id='n3345' href='#n3345'>3345</a>
<a id='n3346' href='#n3346'>3346</a>
<a id='n3347' href='#n3347'>3347</a>
<a id='n3348' href='#n3348'>3348</a>
<a id='n3349' href='#n3349'>3349</a>
<a id='n3350' href='#n3350'>3350</a>
<a id='n3351' href='#n3351'>3351</a>
<a id='n3352' href='#n3352'>3352</a>
<a id='n3353' href='#n3353'>3353</a>
<a id='n3354' href='#n3354'>3354</a>
<a id='n3355' href='#n3355'>3355</a>
<a id='n3356' href='#n3356'>3356</a>
<a id='n3357' href='#n3357'>3357</a>
<a id='n3358' href='#n3358'>3358</a>
<a id='n3359' href='#n3359'>3359</a>
<a id='n3360' href='#n3360'>3360</a>
<a id='n3361' href='#n3361'>3361</a>
<a id='n3362' href='#n3362'>3362</a>
<a id='n3363' href='#n3363'>3363</a>
<a id='n3364' href='#n3364'>3364</a>
<a id='n3365' href='#n3365'>3365</a>
<a id='n3366' href='#n3366'>3366</a>
<a id='n3367' href='#n3367'>3367</a>
<a id='n3368' href='#n3368'>3368</a>
<a id='n3369' href='#n3369'>3369</a>
<a id='n3370' href='#n3370'>3370</a>
<a id='n3371' href='#n3371'>3371</a>
<a id='n3372' href='#n3372'>3372</a>
<a id='n3373' href='#n3373'>3373</a>
<a id='n3374' href='#n3374'>3374</a>
<a id='n3375' href='#n3375'>3375</a>
<a id='n3376' href='#n3376'>3376</a>
<a id='n3377' href='#n3377'>3377</a>
<a id='n3378' href='#n3378'>3378</a>
<a id='n3379' href='#n3379'>3379</a>
<a id='n3380' href='#n3380'>3380</a>
<a id='n3381' href='#n3381'>3381</a>
<a id='n3382' href='#n3382'>3382</a>
<a id='n3383' href='#n3383'>3383</a>
<a id='n3384' href='#n3384'>3384</a>
<a id='n3385' href='#n3385'>3385</a>
<a id='n3386' href='#n3386'>3386</a>
<a id='n3387' href='#n3387'>3387</a>
<a id='n3388' href='#n3388'>3388</a>
<a id='n3389' href='#n3389'>3389</a>
<a id='n3390' href='#n3390'>3390</a>
<a id='n3391' href='#n3391'>3391</a>
<a id='n3392' href='#n3392'>3392</a>
<a id='n3393' href='#n3393'>3393</a>
<a id='n3394' href='#n3394'>3394</a>
<a id='n3395' href='#n3395'>3395</a>
<a id='n3396' href='#n3396'>3396</a>
<a id='n3397' href='#n3397'>3397</a>
<a id='n3398' href='#n3398'>3398</a>
<a id='n3399' href='#n3399'>3399</a>
<a id='n3400' href='#n3400'>3400</a>
<a id='n3401' href='#n3401'>3401</a>
<a id='n3402' href='#n3402'>3402</a>
<a id='n3403' href='#n3403'>3403</a>
<a id='n3404' href='#n3404'>3404</a>
<a id='n3405' href='#n3405'>3405</a>
<a id='n3406' href='#n3406'>3406</a>
<a id='n3407' href='#n3407'>3407</a>
<a id='n3408' href='#n3408'>3408</a>
<a id='n3409' href='#n3409'>3409</a>
<a id='n3410' href='#n3410'>3410</a>
<a id='n3411' href='#n3411'>3411</a>
<a id='n3412' href='#n3412'>3412</a>
<a id='n3413' href='#n3413'>3413</a>
<a id='n3414' href='#n3414'>3414</a>
<a id='n3415' href='#n3415'>3415</a>
<a id='n3416' href='#n3416'>3416</a>
<a id='n3417' href='#n3417'>3417</a>
<a id='n3418' href='#n3418'>3418</a>
<a id='n3419' href='#n3419'>3419</a>
<a id='n3420' href='#n3420'>3420</a>
<a id='n3421' href='#n3421'>3421</a>
<a id='n3422' href='#n3422'>3422</a>
<a id='n3423' href='#n3423'>3423</a>
<a id='n3424' href='#n3424'>3424</a>
<a id='n3425' href='#n3425'>3425</a>
<a id='n3426' href='#n3426'>3426</a>
<a id='n3427' href='#n3427'>3427</a>
<a id='n3428' href='#n3428'>3428</a>
<a id='n3429' href='#n3429'>3429</a>
<a id='n3430' href='#n3430'>3430</a>
<a id='n3431' href='#n3431'>3431</a>
<a id='n3432' href='#n3432'>3432</a>
<a id='n3433' href='#n3433'>3433</a>
<a id='n3434' href='#n3434'>3434</a>
<a id='n3435' href='#n3435'>3435</a>
<a id='n3436' href='#n3436'>3436</a>
<a id='n3437' href='#n3437'>3437</a>
<a id='n3438' href='#n3438'>3438</a>
<a id='n3439' href='#n3439'>3439</a>
<a id='n3440' href='#n3440'>3440</a>
<a id='n3441' href='#n3441'>3441</a>
<a id='n3442' href='#n3442'>3442</a>
<a id='n3443' href='#n3443'>3443</a>
<a id='n3444' href='#n3444'>3444</a>
<a id='n3445' href='#n3445'>3445</a>
<a id='n3446' href='#n3446'>3446</a>
<a id='n3447' href='#n3447'>3447</a>
<a id='n3448' href='#n3448'>3448</a>
<a id='n3449' href='#n3449'>3449</a>
<a id='n3450' href='#n3450'>3450</a>
<a id='n3451' href='#n3451'>3451</a>
<a id='n3452' href='#n3452'>3452</a>
<a id='n3453' href='#n3453'>3453</a>
<a id='n3454' href='#n3454'>3454</a>
<a id='n3455' href='#n3455'>3455</a>
<a id='n3456' href='#n3456'>3456</a>
<a id='n3457' href='#n3457'>3457</a>
<a id='n3458' href='#n3458'>3458</a>
<a id='n3459' href='#n3459'>3459</a>
<a id='n3460' href='#n3460'>3460</a>
<a id='n3461' href='#n3461'>3461</a>
<a id='n3462' href='#n3462'>3462</a>
<a id='n3463' href='#n3463'>3463</a>
<a id='n3464' href='#n3464'>3464</a>
<a id='n3465' href='#n3465'>3465</a>
<a id='n3466' href='#n3466'>3466</a>
<a id='n3467' href='#n3467'>3467</a>
<a id='n3468' href='#n3468'>3468</a>
<a id='n3469' href='#n3469'>3469</a>
<a id='n3470' href='#n3470'>3470</a>
<a id='n3471' href='#n3471'>3471</a>
<a id='n3472' href='#n3472'>3472</a>
<a id='n3473' href='#n3473'>3473</a>
<a id='n3474' href='#n3474'>3474</a>
<a id='n3475' href='#n3475'>3475</a>
<a id='n3476' href='#n3476'>3476</a>
<a id='n3477' href='#n3477'>3477</a>
<a id='n3478' href='#n3478'>3478</a>
<a id='n3479' href='#n3479'>3479</a>
<a id='n3480' href='#n3480'>3480</a>
<a id='n3481' href='#n3481'>3481</a>
<a id='n3482' href='#n3482'>3482</a>
<a id='n3483' href='#n3483'>3483</a>
<a id='n3484' href='#n3484'>3484</a>
<a id='n3485' href='#n3485'>3485</a>
<a id='n3486' href='#n3486'>3486</a>
<a id='n3487' href='#n3487'>3487</a>
<a id='n3488' href='#n3488'>3488</a>
<a id='n3489' href='#n3489'>3489</a>
<a id='n3490' href='#n3490'>3490</a>
<a id='n3491' href='#n3491'>3491</a>
<a id='n3492' href='#n3492'>3492</a>
<a id='n3493' href='#n3493'>3493</a>
<a id='n3494' href='#n3494'>3494</a>
<a id='n3495' href='#n3495'>3495</a>
<a id='n3496' href='#n3496'>3496</a>
<a id='n3497' href='#n3497'>3497</a>
<a id='n3498' href='#n3498'>3498</a>
<a id='n3499' href='#n3499'>3499</a>
<a id='n3500' href='#n3500'>3500</a>
<a id='n3501' href='#n3501'>3501</a>
<a id='n3502' href='#n3502'>3502</a>
<a id='n3503' href='#n3503'>3503</a>
<a id='n3504' href='#n3504'>3504</a>
<a id='n3505' href='#n3505'>3505</a>
<a id='n3506' href='#n3506'>3506</a>
<a id='n3507' href='#n3507'>3507</a>
<a id='n3508' href='#n3508'>3508</a>
<a id='n3509' href='#n3509'>3509</a>
<a id='n3510' href='#n3510'>3510</a>
<a id='n3511' href='#n3511'>3511</a>
<a id='n3512' href='#n3512'>3512</a>
<a id='n3513' href='#n3513'>3513</a>
<a id='n3514' href='#n3514'>3514</a>
<a id='n3515' href='#n3515'>3515</a>
<a id='n3516' href='#n3516'>3516</a>
<a id='n3517' href='#n3517'>3517</a>
<a id='n3518' href='#n3518'>3518</a>
<a id='n3519' href='#n3519'>3519</a>
<a id='n3520' href='#n3520'>3520</a>
<a id='n3521' href='#n3521'>3521</a>
<a id='n3522' href='#n3522'>3522</a>
<a id='n3523' href='#n3523'>3523</a>
<a id='n3524' href='#n3524'>3524</a>
<a id='n3525' href='#n3525'>3525</a>
<a id='n3526' href='#n3526'>3526</a>
<a id='n3527' href='#n3527'>3527</a>
<a id='n3528' href='#n3528'>3528</a>
<a id='n3529' href='#n3529'>3529</a>
<a id='n3530' href='#n3530'>3530</a>
<a id='n3531' href='#n3531'>3531</a>
<a id='n3532' href='#n3532'>3532</a>
<a id='n3533' href='#n3533'>3533</a>
<a id='n3534' href='#n3534'>3534</a>
<a id='n3535' href='#n3535'>3535</a>
<a id='n3536' href='#n3536'>3536</a>
<a id='n3537' href='#n3537'>3537</a>
<a id='n3538' href='#n3538'>3538</a>
<a id='n3539' href='#n3539'>3539</a>
<a id='n3540' href='#n3540'>3540</a>
<a id='n3541' href='#n3541'>3541</a>
<a id='n3542' href='#n3542'>3542</a>
<a id='n3543' href='#n3543'>3543</a>
<a id='n3544' href='#n3544'>3544</a>
<a id='n3545' href='#n3545'>3545</a>
<a id='n3546' href='#n3546'>3546</a>
<a id='n3547' href='#n3547'>3547</a>
<a id='n3548' href='#n3548'>3548</a>
<a id='n3549' href='#n3549'>3549</a>
<a id='n3550' href='#n3550'>3550</a>
<a id='n3551' href='#n3551'>3551</a>
<a id='n3552' href='#n3552'>3552</a>
<a id='n3553' href='#n3553'>3553</a>
<a id='n3554' href='#n3554'>3554</a>
<a id='n3555' href='#n3555'>3555</a>
<a id='n3556' href='#n3556'>3556</a>
<a id='n3557' href='#n3557'>3557</a>
<a id='n3558' href='#n3558'>3558</a>
<a id='n3559' href='#n3559'>3559</a>
<a id='n3560' href='#n3560'>3560</a>
<a id='n3561' href='#n3561'>3561</a>
<a id='n3562' href='#n3562'>3562</a>
<a id='n3563' href='#n3563'>3563</a>
<a id='n3564' href='#n3564'>3564</a>
<a id='n3565' href='#n3565'>3565</a>
<a id='n3566' href='#n3566'>3566</a>
<a id='n3567' href='#n3567'>3567</a>
<a id='n3568' href='#n3568'>3568</a>
<a id='n3569' href='#n3569'>3569</a>
<a id='n3570' href='#n3570'>3570</a>
<a id='n3571' href='#n3571'>3571</a>
<a id='n3572' href='#n3572'>3572</a>
<a id='n3573' href='#n3573'>3573</a>
<a id='n3574' href='#n3574'>3574</a>
<a id='n3575' href='#n3575'>3575</a>
<a id='n3576' href='#n3576'>3576</a>
<a id='n3577' href='#n3577'>3577</a>
<a id='n3578' href='#n3578'>3578</a>
<a id='n3579' href='#n3579'>3579</a>
<a id='n3580' href='#n3580'>3580</a>
<a id='n3581' href='#n3581'>3581</a>
<a id='n3582' href='#n3582'>3582</a>
<a id='n3583' href='#n3583'>3583</a>
<a id='n3584' href='#n3584'>3584</a>
<a id='n3585' href='#n3585'>3585</a>
<a id='n3586' href='#n3586'>3586</a>
<a id='n3587' href='#n3587'>3587</a>
<a id='n3588' href='#n3588'>3588</a>
<a id='n3589' href='#n3589'>3589</a>
<a id='n3590' href='#n3590'>3590</a>
<a id='n3591' href='#n3591'>3591</a>
<a id='n3592' href='#n3592'>3592</a>
<a id='n3593' href='#n3593'>3593</a>
<a id='n3594' href='#n3594'>3594</a>
<a id='n3595' href='#n3595'>3595</a>
<a id='n3596' href='#n3596'>3596</a>
<a id='n3597' href='#n3597'>3597</a>
<a id='n3598' href='#n3598'>3598</a>
<a id='n3599' href='#n3599'>3599</a>
<a id='n3600' href='#n3600'>3600</a>
<a id='n3601' href='#n3601'>3601</a>
<a id='n3602' href='#n3602'>3602</a>
<a id='n3603' href='#n3603'>3603</a>
<a id='n3604' href='#n3604'>3604</a>
<a id='n3605' href='#n3605'>3605</a>
<a id='n3606' href='#n3606'>3606</a>
<a id='n3607' href='#n3607'>3607</a>
<a id='n3608' href='#n3608'>3608</a>
<a id='n3609' href='#n3609'>3609</a>
<a id='n3610' href='#n3610'>3610</a>
</pre></td>
<td class='lines'><pre><code><style>pre { line-height: 125%; margin: 0; }
td.linenos pre { color: #000000; background-color: #f0f0f0; padding: 0 5px 0 5px; }
span.linenos { color: #000000; background-color: #f0f0f0; padding: 0 5px 0 5px; }
td.linenos pre.special { color: #000000; background-color: #ffffc0; padding: 0 5px 0 5px; }
span.linenos.special { color: #000000; background-color: #ffffc0; padding: 0 5px 0 5px; }
.highlight .hll { background-color: #ffffcc }
.highlight { background: #ffffff; }
.highlight .c { color: #888888 } /* Comment */
.highlight .err { color: #a61717; background-color: #e3d2d2 } /* Error */
.highlight .k { color: #008800; font-weight: bold } /* Keyword */
.highlight .ch { color: #888888 } /* Comment.Hashbang */
.highlight .cm { color: #888888 } /* Comment.Multiline */
.highlight .cp { color: #cc0000; font-weight: bold } /* Comment.Preproc */
.highlight .cpf { color: #888888 } /* Comment.PreprocFile */
.highlight .c1 { color: #888888 } /* Comment.Single */
.highlight .cs { color: #cc0000; font-weight: bold; background-color: #fff0f0 } /* Comment.Special */
.highlight .gd { color: #000000; background-color: #ffdddd } /* Generic.Deleted */
.highlight .ge { font-style: italic } /* Generic.Emph */
.highlight .gr { color: #aa0000 } /* Generic.Error */
.highlight .gh { color: #333333 } /* Generic.Heading */
.highlight .gi { color: #000000; background-color: #ddffdd } /* Generic.Inserted */
.highlight .go { color: #888888 } /* Generic.Output */
.highlight .gp { color: #555555 } /* Generic.Prompt */
.highlight .gs { font-weight: bold } /* Generic.Strong */
.highlight .gu { color: #666666 } /* Generic.Subheading */
.highlight .gt { color: #aa0000 } /* Generic.Traceback */
.highlight .kc { color: #008800; font-weight: bold } /* Keyword.Constant */
.highlight .kd { color: #008800; font-weight: bold } /* Keyword.Declaration */
.highlight .kn { color: #008800; font-weight: bold } /* Keyword.Namespace */
.highlight .kp { color: #008800 } /* Keyword.Pseudo */
.highlight .kr { color: #008800; font-weight: bold } /* Keyword.Reserved */
.highlight .kt { color: #888888; font-weight: bold } /* Keyword.Type */
.highlight .m { color: #0000DD; font-weight: bold } /* Literal.Number */
.highlight .s { color: #dd2200; background-color: #fff0f0 } /* Literal.String */
.highlight .na { color: #336699 } /* Name.Attribute */
.highlight .nb { color: #003388 } /* Name.Builtin */
.highlight .nc { color: #bb0066; font-weight: bold } /* Name.Class */
.highlight .no { color: #003366; font-weight: bold } /* Name.Constant */
.highlight .nd { color: #555555 } /* Name.Decorator */
.highlight .ne { color: #bb0066; font-weight: bold } /* Name.Exception */
.highlight .nf { color: #0066bb; font-weight: bold } /* Name.Function */
.highlight .nl { color: #336699; font-style: italic } /* Name.Label */
.highlight .nn { color: #bb0066; font-weight: bold } /* Name.Namespace */
.highlight .py { color: #336699; font-weight: bold } /* Name.Property */
.highlight .nt { color: #bb0066; font-weight: bold } /* Name.Tag */
.highlight .nv { color: #336699 } /* Name.Variable */
.highlight .ow { color: #008800 } /* Operator.Word */
.highlight .w { color: #bbbbbb } /* Text.Whitespace */
.highlight .mb { color: #0000DD; font-weight: bold } /* Literal.Number.Bin */
.highlight .mf { color: #0000DD; font-weight: bold } /* Literal.Number.Float */
.highlight .mh { color: #0000DD; font-weight: bold } /* Literal.Number.Hex */
.highlight .mi { color: #0000DD; font-weight: bold } /* Literal.Number.Integer */
.highlight .mo { color: #0000DD; font-weight: bold } /* Literal.Number.Oct */
.highlight .sa { color: #dd2200; background-color: #fff0f0 } /* Literal.String.Affix */
.highlight .sb { color: #dd2200; background-color: #fff0f0 } /* Literal.String.Backtick */
.highlight .sc { color: #dd2200; background-color: #fff0f0 } /* Literal.String.Char */
.highlight .dl { color: #dd2200; background-color: #fff0f0 } /* Literal.String.Delimiter */
.highlight .sd { color: #dd2200; background-color: #fff0f0 } /* Literal.String.Doc */
.highlight .s2 { color: #dd2200; background-color: #fff0f0 } /* Literal.String.Double */
.highlight .se { color: #0044dd; background-color: #fff0f0 } /* Literal.String.Escape */
.highlight .sh { color: #dd2200; background-color: #fff0f0 } /* Literal.String.Heredoc */
.highlight .si { color: #3333bb; background-color: #fff0f0 } /* Literal.String.Interpol */
.highlight .sx { color: #22bb22; background-color: #f0fff0 } /* Literal.String.Other */
.highlight .sr { color: #008800; background-color: #fff0ff } /* Literal.String.Regex */
.highlight .s1 { color: #dd2200; background-color: #fff0f0 } /* Literal.String.Single */
.highlight .ss { color: #aa6600; background-color: #fff0f0 } /* Literal.String.Symbol */
.highlight .bp { color: #003388 } /* Name.Builtin.Pseudo */
.highlight .fm { color: #0066bb; font-weight: bold } /* Name.Function.Magic */
.highlight .vc { color: #336699 } /* Name.Variable.Class */
.highlight .vg { color: #dd7700 } /* Name.Variable.Global */
.highlight .vi { color: #3333bb } /* Name.Variable.Instance */
.highlight .vm { color: #336699 } /* Name.Variable.Magic */
.highlight .il { color: #0000DD; font-weight: bold } /* Literal.Number.Integer.Long */</style><div class="highlight"><pre><span></span><span class="cm">/*******************************************************************************</span>

<span class="cm">  </span>
<span class="cm">  Copyright(c) 1999 - 2002 Intel Corporation. All rights reserved.</span>
<span class="cm">  </span>
<span class="cm">  This program is free software; you can redistribute it and/or modify it </span>
<span class="cm">  under the terms of the GNU General Public License as published by the Free </span>
<span class="cm">  Software Foundation; either version 2 of the License, or (at your option) </span>
<span class="cm">  any later version.</span>
<span class="cm">  </span>
<span class="cm">  This program is distributed in the hope that it will be useful, but WITHOUT </span>
<span class="cm">  ANY WARRANTY; without even the implied warranty of MERCHANTABILITY or </span>
<span class="cm">  FITNESS FOR A PARTICULAR PURPOSE.  See the GNU General Public License for </span>
<span class="cm">  more details.</span>
<span class="cm">  </span>
<span class="cm">  You should have received a copy of the GNU General Public License along with</span>
<span class="cm">  this program; if not, write to the Free Software Foundation, Inc., 59 </span>
<span class="cm">  Temple Place - Suite 330, Boston, MA  02111-1307, USA.</span>
<span class="cm">  </span>
<span class="cm">  The full GNU General Public License is included in this distribution in the</span>
<span class="cm">  file called LICENSE.</span>
<span class="cm">  </span>
<span class="cm">  Contact Information:</span>
<span class="cm">  Linux NICS &lt;linux.nics@intel.com&gt;</span>
<span class="cm">  Intel Corporation, 5200 N.E. Elam Young Parkway, Hillsboro, OR 97124-6497</span>

<span class="cm">*******************************************************************************/</span>

<span class="cm">/* e1000_hw.c</span>
<span class="cm"> * Shared functions for accessing and configuring the MAC</span>
<span class="cm"> */</span>

<span class="cp">#include</span> <span class="cpf">&quot;e1000_hw.h&quot;</span><span class="cp"></span>

<span class="k">static</span> <span class="kt">int32_t</span> <span class="n">e1000_setup_fiber_link</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">);</span>
<span class="k">static</span> <span class="kt">int32_t</span> <span class="n">e1000_setup_copper_link</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">);</span>
<span class="k">static</span> <span class="kt">int32_t</span> <span class="n">e1000_phy_force_speed_duplex</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">);</span>
<span class="k">static</span> <span class="kt">int32_t</span> <span class="n">e1000_config_mac_to_phy</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">);</span>
<span class="k">static</span> <span class="kt">int32_t</span> <span class="n">e1000_force_mac_fc</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">);</span>
<span class="k">static</span> <span class="kt">void</span> <span class="n">e1000_raise_mdi_clk</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">,</span> <span class="kt">uint32_t</span> <span class="o">*</span><span class="n">ctrl</span><span class="p">);</span>
<span class="k">static</span> <span class="kt">void</span> <span class="n">e1000_lower_mdi_clk</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">,</span> <span class="kt">uint32_t</span> <span class="o">*</span><span class="n">ctrl</span><span class="p">);</span>
<span class="k">static</span> <span class="kt">void</span> <span class="n">e1000_shift_out_mdi_bits</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">,</span> <span class="kt">uint32_t</span> <span class="n">data</span><span class="p">,</span> <span class="kt">uint16_t</span> <span class="n">count</span><span class="p">);</span>
<span class="k">static</span> <span class="kt">uint16_t</span> <span class="n">e1000_shift_in_mdi_bits</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">);</span>
<span class="k">static</span> <span class="kt">int32_t</span> <span class="n">e1000_phy_reset_dsp</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">);</span>
<span class="k">static</span> <span class="kt">void</span> <span class="n">e1000_raise_ee_clk</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">,</span> <span class="kt">uint32_t</span> <span class="o">*</span><span class="n">eecd</span><span class="p">);</span>
<span class="k">static</span> <span class="kt">void</span> <span class="n">e1000_lower_ee_clk</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">,</span> <span class="kt">uint32_t</span> <span class="o">*</span><span class="n">eecd</span><span class="p">);</span>
<span class="k">static</span> <span class="kt">void</span> <span class="n">e1000_shift_out_ee_bits</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">,</span> <span class="kt">uint16_t</span> <span class="n">data</span><span class="p">,</span> <span class="kt">uint16_t</span> <span class="n">count</span><span class="p">);</span>
<span class="k">static</span> <span class="kt">uint16_t</span> <span class="n">e1000_shift_in_ee_bits</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">);</span>
<span class="k">static</span> <span class="kt">void</span> <span class="n">e1000_setup_eeprom</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">);</span>
<span class="k">static</span> <span class="kt">void</span> <span class="n">e1000_clock_eeprom</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">);</span>
<span class="k">static</span> <span class="kt">void</span> <span class="n">e1000_cleanup_eeprom</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">);</span>
<span class="k">static</span> <span class="kt">void</span> <span class="n">e1000_standby_eeprom</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">);</span>
<span class="k">static</span> <span class="kt">int32_t</span> <span class="n">e1000_id_led_init</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span> <span class="n">hw</span><span class="p">);</span>

<span class="cm">/******************************************************************************</span>
<span class="cm"> * Set the mac type member in the hw struct.</span>
<span class="cm"> * </span>
<span class="cm"> * hw - Struct containing variables accessed by shared code</span>
<span class="cm"> *****************************************************************************/</span>
<span class="kt">int32_t</span>
<span class="nf">e1000_set_mac_type</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">)</span>
<span class="p">{</span>
    <span class="n">DEBUGFUNC</span><span class="p">(</span><span class="s">&quot;e1000_set_mac_type&quot;</span><span class="p">);</span>

    <span class="k">switch</span> <span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">device_id</span><span class="p">)</span> <span class="p">{</span>
    <span class="k">case</span> <span class="nl">E1000_DEV_ID_82542</span><span class="p">:</span>
        <span class="k">switch</span> <span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">revision_id</span><span class="p">)</span> <span class="p">{</span>
        <span class="k">case</span> <span class="nl">E1000_82542_2_0_REV_ID</span><span class="p">:</span>
            <span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">=</span> <span class="n">e1000_82542_rev2_0</span><span class="p">;</span>
            <span class="k">break</span><span class="p">;</span>
        <span class="k">case</span> <span class="nl">E1000_82542_2_1_REV_ID</span><span class="p">:</span>
            <span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">=</span> <span class="n">e1000_82542_rev2_1</span><span class="p">;</span>
            <span class="k">break</span><span class="p">;</span>
        <span class="k">default</span><span class="o">:</span>
            <span class="cm">/* Invalid 82542 revision ID */</span>
            <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_MAC_TYPE</span><span class="p">;</span>
        <span class="p">}</span>
        <span class="k">break</span><span class="p">;</span>
    <span class="k">case</span> <span class="nl">E1000_DEV_ID_82543GC_FIBER</span><span class="p">:</span>
    <span class="k">case</span> <span class="nl">E1000_DEV_ID_82543GC_COPPER</span><span class="p">:</span>
        <span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">=</span> <span class="n">e1000_82543</span><span class="p">;</span>
        <span class="k">break</span><span class="p">;</span>
    <span class="k">case</span> <span class="nl">E1000_DEV_ID_82544EI_COPPER</span><span class="p">:</span>
    <span class="k">case</span> <span class="nl">E1000_DEV_ID_82544EI_FIBER</span><span class="p">:</span>
    <span class="k">case</span> <span class="nl">E1000_DEV_ID_82544GC_COPPER</span><span class="p">:</span>
    <span class="k">case</span> <span class="nl">E1000_DEV_ID_82544GC_LOM</span><span class="p">:</span>
        <span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">=</span> <span class="n">e1000_82544</span><span class="p">;</span>
        <span class="k">break</span><span class="p">;</span>
    <span class="k">case</span> <span class="nl">E1000_DEV_ID_82540EM</span><span class="p">:</span>
    <span class="k">case</span> <span class="nl">E1000_DEV_ID_82540EM_LOM</span><span class="p">:</span>
    <span class="k">case</span> <span class="nl">E1000_DEV_ID_82540EP</span><span class="p">:</span>
    <span class="k">case</span> <span class="nl">E1000_DEV_ID_82540EP_LOM</span><span class="p">:</span>
    <span class="k">case</span> <span class="nl">E1000_DEV_ID_82540EP_LP</span><span class="p">:</span>
        <span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">=</span> <span class="n">e1000_82540</span><span class="p">;</span>
        <span class="k">break</span><span class="p">;</span>
    <span class="k">case</span> <span class="nl">E1000_DEV_ID_82545EM_COPPER</span><span class="p">:</span>
    <span class="k">case</span> <span class="nl">E1000_DEV_ID_82545EM_FIBER</span><span class="p">:</span>
        <span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">=</span> <span class="n">e1000_82545</span><span class="p">;</span>
        <span class="k">break</span><span class="p">;</span>
    <span class="k">case</span> <span class="nl">E1000_DEV_ID_82546EB_COPPER</span><span class="p">:</span>
    <span class="k">case</span> <span class="nl">E1000_DEV_ID_82546EB_FIBER</span><span class="p">:</span>
        <span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">=</span> <span class="n">e1000_82546</span><span class="p">;</span>
        <span class="k">break</span><span class="p">;</span>
    <span class="k">default</span><span class="o">:</span>
        <span class="cm">/* Should never have loaded on this device */</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_MAC_TYPE</span><span class="p">;</span>
    <span class="p">}</span>
    <span class="k">return</span> <span class="n">E1000_SUCCESS</span><span class="p">;</span>
<span class="p">}</span>
<span class="cm">/******************************************************************************</span>
<span class="cm"> * Reset the transmit and receive units; mask and clear all interrupts.</span>
<span class="cm"> *</span>
<span class="cm"> * hw - Struct containing variables accessed by shared code</span>
<span class="cm"> *****************************************************************************/</span>
<span class="kt">void</span>
<span class="nf">e1000_reset_hw</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">uint32_t</span> <span class="n">ctrl</span><span class="p">;</span>
    <span class="kt">uint32_t</span> <span class="n">ctrl_ext</span><span class="p">;</span>
    <span class="kt">uint32_t</span> <span class="n">icr</span><span class="p">;</span>
    <span class="kt">uint32_t</span> <span class="n">manc</span><span class="p">;</span>

    <span class="n">DEBUGFUNC</span><span class="p">(</span><span class="s">&quot;e1000_reset_hw&quot;</span><span class="p">);</span>
    <span class="cm">/* For 82542 (rev 2.0), disable MWI before issuing a device reset */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">==</span> <span class="n">e1000_82542_rev2_0</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Disabling MWI on 82542 rev 2.0</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="n">e1000_pci_clear_mwi</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
    <span class="p">}</span>

    <span class="cm">/* Clear interrupt mask to stop board from generating interrupts */</span>
    <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Masking off all interrupts</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">IMC</span><span class="p">,</span> <span class="mh">0xffffffff</span><span class="p">);</span>

    <span class="cm">/* Disable the Transmit and Receive units.  Then delay to allow</span>
<span class="cm">     * any pending transactions to complete before we hit the MAC with</span>
<span class="cm">     * the global reset.</span>
<span class="cm">     */</span>
    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">RCTL</span><span class="p">,</span> <span class="mi">0</span><span class="p">);</span>
    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">TCTL</span><span class="p">,</span> <span class="n">E1000_TCTL_PSP</span><span class="p">);</span>
    <span class="n">E1000_WRITE_FLUSH</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>

    <span class="cm">/* The tbi_compatibility_on Flag must be cleared when Rctl is cleared. */</span>
    <span class="n">hw</span><span class="o">-&gt;</span><span class="n">tbi_compatibility_on</span> <span class="o">=</span> <span class="n">FALSE</span><span class="p">;</span>

    <span class="cm">/* Delay to allow any outstanding PCI transactions to complete before</span>
<span class="cm">     * resetting the device</span>
<span class="cm">     */</span> 
    <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Before delay</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
    <span class="n">msec_delay</span><span class="p">(</span><span class="mi">10</span><span class="p">);</span>

    <span class="cm">/* Issue a global reset to the MAC.  This will reset the chip&#39;s</span>
<span class="cm">     * transmit, receive, DMA, and link units.  It will not effect</span>
<span class="cm">     * the current PCI configuration.  The global reset bit is self-</span>
<span class="cm">     * clearing, and should clear within a microsecond.</span>
<span class="cm">     */</span>
    <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Issuing a global reset to MAC</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
    <span class="n">ctrl</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL</span><span class="p">);</span>

    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">&gt;</span> <span class="n">e1000_82543</span><span class="p">)</span>
        <span class="n">E1000_WRITE_REG_IO</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL</span><span class="p">,</span> <span class="p">(</span><span class="n">ctrl</span> <span class="o">|</span> <span class="n">E1000_CTRL_RST</span><span class="p">));</span>
    <span class="k">else</span>
        <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL</span><span class="p">,</span> <span class="p">(</span><span class="n">ctrl</span> <span class="o">|</span> <span class="n">E1000_CTRL_RST</span><span class="p">));</span>

    <span class="cm">/* Force a reload from the EEPROM if necessary */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">&lt;</span> <span class="n">e1000_82540</span><span class="p">)</span> <span class="p">{</span>
        <span class="cm">/* Wait for reset to complete */</span>
        <span class="n">udelay</span><span class="p">(</span><span class="mi">10</span><span class="p">);</span>
        <span class="n">ctrl_ext</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL_EXT</span><span class="p">);</span>
        <span class="n">ctrl_ext</span> <span class="o">|=</span> <span class="n">E1000_CTRL_EXT_EE_RST</span><span class="p">;</span>
        <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL_EXT</span><span class="p">,</span> <span class="n">ctrl_ext</span><span class="p">);</span>
        <span class="n">E1000_WRITE_FLUSH</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
        <span class="cm">/* Wait for EEPROM reload */</span>
        <span class="n">msec_delay</span><span class="p">(</span><span class="mi">2</span><span class="p">);</span>
    <span class="p">}</span> <span class="k">else</span> <span class="p">{</span>
        <span class="cm">/* Wait for EEPROM reload (it happens automatically) */</span>
        <span class="n">msec_delay</span><span class="p">(</span><span class="mi">4</span><span class="p">);</span>
        <span class="cm">/* Dissable HW ARPs on ASF enabled adapters */</span>
        <span class="n">manc</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">MANC</span><span class="p">);</span>
        <span class="n">manc</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="p">(</span><span class="n">E1000_MANC_ARP_EN</span><span class="p">);</span>
        <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">MANC</span><span class="p">,</span> <span class="n">manc</span><span class="p">);</span>
    <span class="p">}</span>
    
    <span class="cm">/* Clear interrupt mask to stop board from generating interrupts */</span>
    <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Masking off all interrupts</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">IMC</span><span class="p">,</span> <span class="mh">0xffffffff</span><span class="p">);</span>

    <span class="cm">/* Clear any pending interrupt events. */</span>
    <span class="n">icr</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">ICR</span><span class="p">);</span>

    <span class="cm">/* If MWI was previously enabled, reenable it. */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">==</span> <span class="n">e1000_82542_rev2_0</span><span class="p">)</span> <span class="p">{</span>
        <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">pci_cmd_word</span> <span class="o">&amp;</span> <span class="n">CMD_MEM_WRT_INVALIDATE</span><span class="p">)</span>
            <span class="n">e1000_pci_set_mwi</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
    <span class="p">}</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm"> * Performs basic configuration of the adapter.</span>
<span class="cm"> *</span>
<span class="cm"> * hw - Struct containing variables accessed by shared code</span>
<span class="cm"> * </span>
<span class="cm"> * Assumes that the controller has previously been reset and is in a </span>
<span class="cm"> * post-reset uninitialized state. Initializes the receive address registers,</span>
<span class="cm"> * multicast table, and VLAN filter table. Calls routines to setup link</span>
<span class="cm"> * configuration and flow control settings. Clears all on-chip counters. Leaves</span>
<span class="cm"> * the transmit and receive units disabled and uninitialized.</span>
<span class="cm"> *****************************************************************************/</span>
<span class="kt">int32_t</span>
<span class="nf">e1000_init_hw</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">uint32_t</span> <span class="n">ctrl</span><span class="p">,</span> <span class="n">status</span><span class="p">;</span>
    <span class="kt">uint32_t</span> <span class="n">i</span><span class="p">;</span>
    <span class="kt">int32_t</span> <span class="n">ret_val</span><span class="p">;</span>
    <span class="kt">uint16_t</span> <span class="n">pcix_cmd_word</span><span class="p">;</span>
    <span class="kt">uint16_t</span> <span class="n">pcix_stat_hi_word</span><span class="p">;</span>
    <span class="kt">uint16_t</span> <span class="n">cmd_mmrbc</span><span class="p">;</span>
    <span class="kt">uint16_t</span> <span class="n">stat_mmrbc</span><span class="p">;</span>

    <span class="n">DEBUGFUNC</span><span class="p">(</span><span class="s">&quot;e1000_init_hw&quot;</span><span class="p">);</span>

    <span class="cm">/* Initialize Identification LED */</span>
    <span class="n">ret_val</span> <span class="o">=</span> <span class="n">e1000_id_led_init</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
    <span class="k">if</span><span class="p">(</span><span class="n">ret_val</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Error Initializing Identification LED</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="k">return</span> <span class="n">ret_val</span><span class="p">;</span>
    <span class="p">}</span>
    
    <span class="cm">/* Set the Media Type and exit with error if it is not valid. */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">!=</span> <span class="n">e1000_82543</span><span class="p">)</span> <span class="p">{</span>
        <span class="cm">/* tbi_compatibility is only valid on 82543 */</span>
        <span class="n">hw</span><span class="o">-&gt;</span><span class="n">tbi_compatibility_en</span> <span class="o">=</span> <span class="n">FALSE</span><span class="p">;</span>
    <span class="p">}</span>

    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">&gt;=</span> <span class="n">e1000_82543</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">status</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">STATUS</span><span class="p">);</span>
        <span class="k">if</span><span class="p">(</span><span class="n">status</span> <span class="o">&amp;</span> <span class="n">E1000_STATUS_TBIMODE</span><span class="p">)</span> <span class="p">{</span>
            <span class="n">hw</span><span class="o">-&gt;</span><span class="n">media_type</span> <span class="o">=</span> <span class="n">e1000_media_type_fiber</span><span class="p">;</span>
            <span class="cm">/* tbi_compatibility not valid on fiber */</span>
            <span class="n">hw</span><span class="o">-&gt;</span><span class="n">tbi_compatibility_en</span> <span class="o">=</span> <span class="n">FALSE</span><span class="p">;</span>
        <span class="p">}</span> <span class="k">else</span> <span class="p">{</span>
            <span class="n">hw</span><span class="o">-&gt;</span><span class="n">media_type</span> <span class="o">=</span> <span class="n">e1000_media_type_copper</span><span class="p">;</span>
        <span class="p">}</span>
    <span class="p">}</span> <span class="k">else</span> <span class="p">{</span>
        <span class="cm">/* This is an 82542 (fiber only) */</span>
        <span class="n">hw</span><span class="o">-&gt;</span><span class="n">media_type</span> <span class="o">=</span> <span class="n">e1000_media_type_fiber</span><span class="p">;</span>
    <span class="p">}</span>

    <span class="cm">/* Disabling VLAN filtering. */</span>
    <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Initializing the IEEE VLAN</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">VET</span><span class="p">,</span> <span class="mi">0</span><span class="p">);</span>

    <span class="n">e1000_clear_vfta</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>

    <span class="cm">/* For 82542 (rev 2.0), disable MWI and put the receiver into reset */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">==</span> <span class="n">e1000_82542_rev2_0</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Disabling MWI on 82542 rev 2.0</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="n">e1000_pci_clear_mwi</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
        <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">RCTL</span><span class="p">,</span> <span class="n">E1000_RCTL_RST</span><span class="p">);</span>
        <span class="n">E1000_WRITE_FLUSH</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
        <span class="n">msec_delay</span><span class="p">(</span><span class="mi">5</span><span class="p">);</span>
    <span class="p">}</span>

    <span class="cm">/* Setup the receive address. This involves initializing all of the Receive</span>
<span class="cm">     * Address Registers (RARs 0 - 15).</span>
<span class="cm">     */</span>
    <span class="n">e1000_init_rx_addrs</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>

    <span class="cm">/* For 82542 (rev 2.0), take the receiver out of reset and enable MWI */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">==</span> <span class="n">e1000_82542_rev2_0</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">RCTL</span><span class="p">,</span> <span class="mi">0</span><span class="p">);</span>
        <span class="n">E1000_WRITE_FLUSH</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
        <span class="n">msec_delay</span><span class="p">(</span><span class="mi">1</span><span class="p">);</span>
        <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">pci_cmd_word</span> <span class="o">&amp;</span> <span class="n">CMD_MEM_WRT_INVALIDATE</span><span class="p">)</span>
            <span class="n">e1000_pci_set_mwi</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
    <span class="p">}</span>

    <span class="cm">/* Zero out the Multicast HASH table */</span>
    <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Zeroing the MTA</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
    <span class="k">for</span><span class="p">(</span><span class="n">i</span> <span class="o">=</span> <span class="mi">0</span><span class="p">;</span> <span class="n">i</span> <span class="o">&lt;</span> <span class="n">E1000_MC_TBL_SIZE</span><span class="p">;</span> <span class="n">i</span><span class="o">++</span><span class="p">)</span>
        <span class="n">E1000_WRITE_REG_ARRAY</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">MTA</span><span class="p">,</span> <span class="n">i</span><span class="p">,</span> <span class="mi">0</span><span class="p">);</span>

    <span class="cm">/* Set the PCI priority bit correctly in the CTRL register.  This</span>
<span class="cm">     * determines if the adapter gives priority to receives, or if it</span>
<span class="cm">     * gives equal priority to transmits and receives.</span>
<span class="cm">     */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">dma_fairness</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">ctrl</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL</span><span class="p">);</span>
        <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL</span><span class="p">,</span> <span class="n">ctrl</span> <span class="o">|</span> <span class="n">E1000_CTRL_PRIOR</span><span class="p">);</span>
    <span class="p">}</span>

    <span class="cm">/* Workaround for PCI-X problem when BIOS sets MMRBC incorrectly. */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">bus_type</span> <span class="o">==</span> <span class="n">e1000_bus_type_pcix</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">e1000_read_pci_cfg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PCIX_COMMAND_REGISTER</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">pcix_cmd_word</span><span class="p">);</span>
        <span class="n">e1000_read_pci_cfg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PCIX_STATUS_REGISTER_HI</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">pcix_stat_hi_word</span><span class="p">);</span>
        <span class="n">cmd_mmrbc</span> <span class="o">=</span> <span class="p">(</span><span class="n">pcix_cmd_word</span> <span class="o">&amp;</span> <span class="n">PCIX_COMMAND_MMRBC_MASK</span><span class="p">)</span> <span class="o">&gt;&gt;</span>
            <span class="n">PCIX_COMMAND_MMRBC_SHIFT</span><span class="p">;</span>
        <span class="n">stat_mmrbc</span> <span class="o">=</span> <span class="p">(</span><span class="n">pcix_stat_hi_word</span> <span class="o">&amp;</span> <span class="n">PCIX_STATUS_HI_MMRBC_MASK</span><span class="p">)</span> <span class="o">&gt;&gt;</span>
            <span class="n">PCIX_STATUS_HI_MMRBC_SHIFT</span><span class="p">;</span>
        <span class="k">if</span><span class="p">(</span><span class="n">stat_mmrbc</span> <span class="o">==</span> <span class="n">PCIX_STATUS_HI_MMRBC_4K</span><span class="p">)</span>
            <span class="n">stat_mmrbc</span> <span class="o">=</span> <span class="n">PCIX_STATUS_HI_MMRBC_2K</span><span class="p">;</span>
        <span class="k">if</span><span class="p">(</span><span class="n">cmd_mmrbc</span> <span class="o">&gt;</span> <span class="n">stat_mmrbc</span><span class="p">)</span> <span class="p">{</span>
            <span class="n">pcix_cmd_word</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="n">PCIX_COMMAND_MMRBC_MASK</span><span class="p">;</span>
            <span class="n">pcix_cmd_word</span> <span class="o">|=</span> <span class="n">stat_mmrbc</span> <span class="o">&lt;&lt;</span> <span class="n">PCIX_COMMAND_MMRBC_SHIFT</span><span class="p">;</span>
            <span class="n">e1000_write_pci_cfg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PCIX_COMMAND_REGISTER</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">pcix_cmd_word</span><span class="p">);</span>
        <span class="p">}</span>
    <span class="p">}</span>

    <span class="cm">/* Call a subroutine to configure the link and setup flow control. */</span>
    <span class="n">ret_val</span> <span class="o">=</span> <span class="n">e1000_setup_link</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>

    <span class="cm">/* Set the transmit descriptor write-back policy */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">&gt;</span> <span class="n">e1000_82544</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">ctrl</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">TXDCTL</span><span class="p">);</span>
        <span class="n">ctrl</span> <span class="o">=</span> <span class="p">(</span><span class="n">ctrl</span> <span class="o">&amp;</span> <span class="o">~</span><span class="n">E1000_TXDCTL_WTHRESH</span><span class="p">)</span> <span class="o">|</span> <span class="n">E1000_TXDCTL_FULL_TX_DESC_WB</span><span class="p">;</span>
        <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">TXDCTL</span><span class="p">,</span> <span class="n">ctrl</span><span class="p">);</span>
    <span class="p">}</span>

    <span class="cm">/* Clear all of the statistics registers (clear on read).  It is</span>
<span class="cm">     * important that we do this after we have tried to establish link</span>
<span class="cm">     * because the symbol error count will increment wildly if there</span>
<span class="cm">     * is no link.</span>
<span class="cm">     */</span>
    <span class="n">e1000_clear_hw_cntrs</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>

    <span class="k">return</span> <span class="n">ret_val</span><span class="p">;</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm"> * Configures flow control and link settings.</span>
<span class="cm"> * </span>
<span class="cm"> * hw - Struct containing variables accessed by shared code</span>
<span class="cm"> * </span>
<span class="cm"> * Determines which flow control settings to use. Calls the apropriate media-</span>
<span class="cm"> * specific link configuration function. Configures the flow control settings.</span>
<span class="cm"> * Assuming the adapter has a valid link partner, a valid link should be</span>
<span class="cm"> * established. Assumes the hardware has previously been reset and the </span>
<span class="cm"> * transmitter and receiver are not enabled.</span>
<span class="cm"> *****************************************************************************/</span>
<span class="kt">int32_t</span>
<span class="nf">e1000_setup_link</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">uint32_t</span> <span class="n">ctrl_ext</span><span class="p">;</span>
    <span class="kt">int32_t</span> <span class="n">ret_val</span><span class="p">;</span>
    <span class="kt">uint16_t</span> <span class="n">eeprom_data</span><span class="p">;</span>

    <span class="n">DEBUGFUNC</span><span class="p">(</span><span class="s">&quot;e1000_setup_link&quot;</span><span class="p">);</span>

    <span class="cm">/* Read and store word 0x0F of the EEPROM. This word contains bits</span>
<span class="cm">     * that determine the hardware&#39;s default PAUSE (flow control) mode,</span>
<span class="cm">     * a bit that determines whether the HW defaults to enabling or</span>
<span class="cm">     * disabling auto-negotiation, and the direction of the</span>
<span class="cm">     * SW defined pins. If there is no SW over-ride of the flow</span>
<span class="cm">     * control setting, then the variable hw-&gt;fc will</span>
<span class="cm">     * be initialized based on a value in the EEPROM.</span>
<span class="cm">     */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_eeprom</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EEPROM_INIT_CONTROL2_REG</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">eeprom_data</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;EEPROM Read Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_EEPROM</span><span class="p">;</span>
    <span class="p">}</span>

    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">fc</span> <span class="o">==</span> <span class="n">e1000_fc_default</span><span class="p">)</span> <span class="p">{</span>
        <span class="k">if</span><span class="p">((</span><span class="n">eeprom_data</span> <span class="o">&amp;</span> <span class="n">EEPROM_WORD0F_PAUSE_MASK</span><span class="p">)</span> <span class="o">==</span> <span class="mi">0</span><span class="p">)</span>
            <span class="n">hw</span><span class="o">-&gt;</span><span class="n">fc</span> <span class="o">=</span> <span class="n">e1000_fc_none</span><span class="p">;</span>
        <span class="k">else</span> <span class="k">if</span><span class="p">((</span><span class="n">eeprom_data</span> <span class="o">&amp;</span> <span class="n">EEPROM_WORD0F_PAUSE_MASK</span><span class="p">)</span> <span class="o">==</span> 
                <span class="n">EEPROM_WORD0F_ASM_DIR</span><span class="p">)</span>
            <span class="n">hw</span><span class="o">-&gt;</span><span class="n">fc</span> <span class="o">=</span> <span class="n">e1000_fc_tx_pause</span><span class="p">;</span>
        <span class="k">else</span>
            <span class="n">hw</span><span class="o">-&gt;</span><span class="n">fc</span> <span class="o">=</span> <span class="n">e1000_fc_full</span><span class="p">;</span>
    <span class="p">}</span>

    <span class="cm">/* We want to save off the original Flow Control configuration just</span>
<span class="cm">     * in case we get disconnected and then reconnected into a different</span>
<span class="cm">     * hub or switch with different Flow Control capabilities.</span>
<span class="cm">     */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">==</span> <span class="n">e1000_82542_rev2_0</span><span class="p">)</span>
        <span class="n">hw</span><span class="o">-&gt;</span><span class="n">fc</span> <span class="o">&amp;=</span> <span class="p">(</span><span class="o">~</span><span class="n">e1000_fc_tx_pause</span><span class="p">);</span>

    <span class="k">if</span><span class="p">((</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">&lt;</span> <span class="n">e1000_82543</span><span class="p">)</span> <span class="o">&amp;&amp;</span> <span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">report_tx_early</span> <span class="o">==</span> <span class="mi">1</span><span class="p">))</span>
        <span class="n">hw</span><span class="o">-&gt;</span><span class="n">fc</span> <span class="o">&amp;=</span> <span class="p">(</span><span class="o">~</span><span class="n">e1000_fc_rx_pause</span><span class="p">);</span>

    <span class="n">hw</span><span class="o">-&gt;</span><span class="n">original_fc</span> <span class="o">=</span> <span class="n">hw</span><span class="o">-&gt;</span><span class="n">fc</span><span class="p">;</span>

    <span class="n">DEBUGOUT1</span><span class="p">(</span><span class="s">&quot;After fix-ups FlowControl is now = %x</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">,</span> <span class="n">hw</span><span class="o">-&gt;</span><span class="n">fc</span><span class="p">);</span>

    <span class="cm">/* Take the 4 bits from EEPROM word 0x0F that determine the initial</span>
<span class="cm">     * polarity value for the SW controlled pins, and setup the</span>
<span class="cm">     * Extended Device Control reg with that info.</span>
<span class="cm">     * This is needed because one of the SW controlled pins is used for</span>
<span class="cm">     * signal detection.  So this should be done before e1000_setup_pcs_link()</span>
<span class="cm">     * or e1000_phy_setup() is called.</span>
<span class="cm">     */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">==</span> <span class="n">e1000_82543</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">ctrl_ext</span> <span class="o">=</span> <span class="p">((</span><span class="n">eeprom_data</span> <span class="o">&amp;</span> <span class="n">EEPROM_WORD0F_SWPDIO_EXT</span><span class="p">)</span> <span class="o">&lt;&lt;</span> 
                    <span class="n">SWDPIO__EXT_SHIFT</span><span class="p">);</span>
        <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL_EXT</span><span class="p">,</span> <span class="n">ctrl_ext</span><span class="p">);</span>
    <span class="p">}</span>

    <span class="cm">/* Call the necessary subroutine to configure the link. */</span>
    <span class="n">ret_val</span> <span class="o">=</span> <span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">media_type</span> <span class="o">==</span> <span class="n">e1000_media_type_fiber</span><span class="p">)</span> <span class="o">?</span>
              <span class="n">e1000_setup_fiber_link</span><span class="p">(</span><span class="n">hw</span><span class="p">)</span> <span class="o">:</span>
              <span class="n">e1000_setup_copper_link</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>

    <span class="cm">/* Initialize the flow control address, type, and PAUSE timer</span>
<span class="cm">     * registers to their default values.  This is done even if flow</span>
<span class="cm">     * control is disabled, because it does not hurt anything to</span>
<span class="cm">     * initialize these registers.</span>
<span class="cm">     */</span>
    <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Initializing the Flow Control address, type and timer regs</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>

    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">FCAL</span><span class="p">,</span> <span class="n">FLOW_CONTROL_ADDRESS_LOW</span><span class="p">);</span>
    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">FCAH</span><span class="p">,</span> <span class="n">FLOW_CONTROL_ADDRESS_HIGH</span><span class="p">);</span>
    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">FCT</span><span class="p">,</span> <span class="n">FLOW_CONTROL_TYPE</span><span class="p">);</span>
    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">FCTTV</span><span class="p">,</span> <span class="n">hw</span><span class="o">-&gt;</span><span class="n">fc_pause_time</span><span class="p">);</span>

    <span class="cm">/* Set the flow control receive threshold registers.  Normally,</span>
<span class="cm">     * these registers will be set to a default threshold that may be</span>
<span class="cm">     * adjusted later by the driver&#39;s runtime code.  However, if the</span>
<span class="cm">     * ability to transmit pause frames in not enabled, then these</span>
<span class="cm">     * registers will be set to 0. </span>
<span class="cm">     */</span>
    <span class="k">if</span><span class="p">(</span><span class="o">!</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">fc</span> <span class="o">&amp;</span> <span class="n">e1000_fc_tx_pause</span><span class="p">))</span> <span class="p">{</span>
        <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">FCRTL</span><span class="p">,</span> <span class="mi">0</span><span class="p">);</span>
        <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">FCRTH</span><span class="p">,</span> <span class="mi">0</span><span class="p">);</span>
    <span class="p">}</span> <span class="k">else</span> <span class="p">{</span>
        <span class="cm">/* We need to set up the Receive Threshold high and low water marks</span>
<span class="cm">         * as well as (optionally) enabling the transmission of XON frames.</span>
<span class="cm">         */</span>
        <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">fc_send_xon</span><span class="p">)</span> <span class="p">{</span>
            <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">FCRTL</span><span class="p">,</span> <span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">fc_low_water</span> <span class="o">|</span> <span class="n">E1000_FCRTL_XONE</span><span class="p">));</span>
            <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">FCRTH</span><span class="p">,</span> <span class="n">hw</span><span class="o">-&gt;</span><span class="n">fc_high_water</span><span class="p">);</span>
        <span class="p">}</span> <span class="k">else</span> <span class="p">{</span>
            <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">FCRTL</span><span class="p">,</span> <span class="n">hw</span><span class="o">-&gt;</span><span class="n">fc_low_water</span><span class="p">);</span>
            <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">FCRTH</span><span class="p">,</span> <span class="n">hw</span><span class="o">-&gt;</span><span class="n">fc_high_water</span><span class="p">);</span>
        <span class="p">}</span>
    <span class="p">}</span>
    <span class="k">return</span> <span class="n">ret_val</span><span class="p">;</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm"> * Sets up link for a fiber based adapter</span>
<span class="cm"> *</span>
<span class="cm"> * hw - Struct containing variables accessed by shared code</span>
<span class="cm"> *</span>
<span class="cm"> * Manipulates Physical Coding Sublayer functions in order to configure</span>
<span class="cm"> * link. Assumes the hardware has been previously reset and the transmitter</span>
<span class="cm"> * and receiver are not enabled.</span>
<span class="cm"> *****************************************************************************/</span>
<span class="k">static</span> <span class="kt">int32_t</span> 
<span class="n">e1000_setup_fiber_link</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">uint32_t</span> <span class="n">ctrl</span><span class="p">;</span>
    <span class="kt">uint32_t</span> <span class="n">status</span><span class="p">;</span>
    <span class="kt">uint32_t</span> <span class="n">txcw</span> <span class="o">=</span> <span class="mi">0</span><span class="p">;</span>
    <span class="kt">uint32_t</span> <span class="n">i</span><span class="p">;</span>
    <span class="kt">uint32_t</span> <span class="n">signal</span><span class="p">;</span>
    <span class="kt">int32_t</span> <span class="n">ret_val</span><span class="p">;</span>

    <span class="n">DEBUGFUNC</span><span class="p">(</span><span class="s">&quot;e1000_setup_fiber_link&quot;</span><span class="p">);</span>

    <span class="cm">/* On adapters with a MAC newer that 82544, SW Defineable pin 1 will be </span>
<span class="cm">     * set when the optics detect a signal. On older adapters, it will be </span>
<span class="cm">     * cleared when there is a signal</span>
<span class="cm">     */</span>
    <span class="n">ctrl</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL</span><span class="p">);</span>
    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">&gt;</span> <span class="n">e1000_82544</span><span class="p">)</span> <span class="n">signal</span> <span class="o">=</span> <span class="n">E1000_CTRL_SWDPIN1</span><span class="p">;</span>
    <span class="k">else</span> <span class="n">signal</span> <span class="o">=</span> <span class="mi">0</span><span class="p">;</span>
   
    <span class="cm">/* Take the link out of reset */</span>
    <span class="n">ctrl</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="p">(</span><span class="n">E1000_CTRL_LRST</span><span class="p">);</span>
    
    <span class="n">e1000_config_collision_dist</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>

    <span class="cm">/* Check for a software override of the flow control settings, and setup</span>
<span class="cm">     * the device accordingly.  If auto-negotiation is enabled, then software</span>
<span class="cm">     * will have to set the &quot;PAUSE&quot; bits to the correct value in the Tranmsit</span>
<span class="cm">     * Config Word Register (TXCW) and re-start auto-negotiation.  However, if</span>
<span class="cm">     * auto-negotiation is disabled, then software will have to manually </span>
<span class="cm">     * configure the two flow control enable bits in the CTRL register.</span>
<span class="cm">     *</span>
<span class="cm">     * The possible values of the &quot;fc&quot; parameter are:</span>
<span class="cm">     *      0:  Flow control is completely disabled</span>
<span class="cm">     *      1:  Rx flow control is enabled (we can receive pause frames, but </span>
<span class="cm">     *          not send pause frames).</span>
<span class="cm">     *      2:  Tx flow control is enabled (we can send pause frames but we do</span>
<span class="cm">     *          not support receiving pause frames).</span>
<span class="cm">     *      3:  Both Rx and TX flow control (symmetric) are enabled.</span>
<span class="cm">     */</span>
    <span class="k">switch</span> <span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">fc</span><span class="p">)</span> <span class="p">{</span>
    <span class="k">case</span> <span class="nl">e1000_fc_none</span><span class="p">:</span>
        <span class="cm">/* Flow control is completely disabled by a software over-ride. */</span>
        <span class="n">txcw</span> <span class="o">=</span> <span class="p">(</span><span class="n">E1000_TXCW_ANE</span> <span class="o">|</span> <span class="n">E1000_TXCW_FD</span><span class="p">);</span>
        <span class="k">break</span><span class="p">;</span>
    <span class="k">case</span> <span class="nl">e1000_fc_rx_pause</span><span class="p">:</span>
        <span class="cm">/* RX Flow control is enabled and TX Flow control is disabled by a </span>
<span class="cm">         * software over-ride. Since there really isn&#39;t a way to advertise </span>
<span class="cm">         * that we are capable of RX Pause ONLY, we will advertise that we</span>
<span class="cm">         * support both symmetric and asymmetric RX PAUSE. Later, we will</span>
<span class="cm">         *  disable the adapter&#39;s ability to send PAUSE frames.</span>
<span class="cm">         */</span>
        <span class="n">txcw</span> <span class="o">=</span> <span class="p">(</span><span class="n">E1000_TXCW_ANE</span> <span class="o">|</span> <span class="n">E1000_TXCW_FD</span> <span class="o">|</span> <span class="n">E1000_TXCW_PAUSE_MASK</span><span class="p">);</span>
        <span class="k">break</span><span class="p">;</span>
    <span class="k">case</span> <span class="nl">e1000_fc_tx_pause</span><span class="p">:</span>
        <span class="cm">/* TX Flow control is enabled, and RX Flow control is disabled, by a </span>
<span class="cm">         * software over-ride.</span>
<span class="cm">         */</span>
        <span class="n">txcw</span> <span class="o">=</span> <span class="p">(</span><span class="n">E1000_TXCW_ANE</span> <span class="o">|</span> <span class="n">E1000_TXCW_FD</span> <span class="o">|</span> <span class="n">E1000_TXCW_ASM_DIR</span><span class="p">);</span>
        <span class="k">break</span><span class="p">;</span>
    <span class="k">case</span> <span class="nl">e1000_fc_full</span><span class="p">:</span>
        <span class="cm">/* Flow control (both RX and TX) is enabled by a software over-ride. */</span>
        <span class="n">txcw</span> <span class="o">=</span> <span class="p">(</span><span class="n">E1000_TXCW_ANE</span> <span class="o">|</span> <span class="n">E1000_TXCW_FD</span> <span class="o">|</span> <span class="n">E1000_TXCW_PAUSE_MASK</span><span class="p">);</span>
        <span class="k">break</span><span class="p">;</span>
    <span class="k">default</span><span class="o">:</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Flow control param set incorrectly</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_CONFIG</span><span class="p">;</span>
        <span class="k">break</span><span class="p">;</span>
    <span class="p">}</span>

    <span class="cm">/* Since auto-negotiation is enabled, take the link out of reset (the link</span>
<span class="cm">     * will be in reset, because we previously reset the chip). This will</span>
<span class="cm">     * restart auto-negotiation.  If auto-neogtiation is successful then the</span>
<span class="cm">     * link-up status bit will be set and the flow control enable bits (RFCE</span>
<span class="cm">     * and TFCE) will be set according to their negotiated value.</span>
<span class="cm">     */</span>
    <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Auto-negotiation enabled</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>

    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">TXCW</span><span class="p">,</span> <span class="n">txcw</span><span class="p">);</span>
    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL</span><span class="p">,</span> <span class="n">ctrl</span><span class="p">);</span>
    <span class="n">E1000_WRITE_FLUSH</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>

    <span class="n">hw</span><span class="o">-&gt;</span><span class="n">txcw</span> <span class="o">=</span> <span class="n">txcw</span><span class="p">;</span>
    <span class="n">msec_delay</span><span class="p">(</span><span class="mi">1</span><span class="p">);</span>

    <span class="cm">/* If we have a signal (the cable is plugged in) then poll for a &quot;Link-Up&quot;</span>
<span class="cm">     * indication in the Device Status Register.  Time-out if a link isn&#39;t </span>
<span class="cm">     * seen in 500 milliseconds seconds (Auto-negotiation should complete in </span>
<span class="cm">     * less than 500 milliseconds even if the other end is doing it in SW).</span>
<span class="cm">     */</span>
    <span class="k">if</span><span class="p">((</span><span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL</span><span class="p">)</span> <span class="o">&amp;</span> <span class="n">E1000_CTRL_SWDPIN1</span><span class="p">)</span> <span class="o">==</span> <span class="n">signal</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Looking for Link</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="k">for</span><span class="p">(</span><span class="n">i</span> <span class="o">=</span> <span class="mi">0</span><span class="p">;</span> <span class="n">i</span> <span class="o">&lt;</span> <span class="p">(</span><span class="n">LINK_UP_TIMEOUT</span> <span class="o">/</span> <span class="mi">10</span><span class="p">);</span> <span class="n">i</span><span class="o">++</span><span class="p">)</span> <span class="p">{</span>
            <span class="n">msec_delay</span><span class="p">(</span><span class="mi">10</span><span class="p">);</span>
            <span class="n">status</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">STATUS</span><span class="p">);</span>
            <span class="k">if</span><span class="p">(</span><span class="n">status</span> <span class="o">&amp;</span> <span class="n">E1000_STATUS_LU</span><span class="p">)</span> <span class="k">break</span><span class="p">;</span>
        <span class="p">}</span>
        <span class="k">if</span><span class="p">(</span><span class="n">i</span> <span class="o">==</span> <span class="p">(</span><span class="n">LINK_UP_TIMEOUT</span> <span class="o">/</span> <span class="mi">10</span><span class="p">))</span> <span class="p">{</span>
            <span class="cm">/* AutoNeg failed to achieve a link, so we&#39;ll call </span>
<span class="cm">             * e1000_check_for_link. This routine will force the link up if we</span>
<span class="cm">             * detect a signal. This will allow us to communicate with</span>
<span class="cm">             * non-autonegotiating link partners.</span>
<span class="cm">             */</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Never got a valid link from auto-neg!!!</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
            <span class="n">hw</span><span class="o">-&gt;</span><span class="n">autoneg_failed</span> <span class="o">=</span> <span class="mi">1</span><span class="p">;</span>
            <span class="n">ret_val</span> <span class="o">=</span> <span class="n">e1000_check_for_link</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
            <span class="k">if</span><span class="p">(</span><span class="n">ret_val</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
                <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Error while checking for link</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
                <span class="k">return</span> <span class="n">ret_val</span><span class="p">;</span>
            <span class="p">}</span>
            <span class="n">hw</span><span class="o">-&gt;</span><span class="n">autoneg_failed</span> <span class="o">=</span> <span class="mi">0</span><span class="p">;</span>
        <span class="p">}</span> <span class="k">else</span> <span class="p">{</span>
            <span class="n">hw</span><span class="o">-&gt;</span><span class="n">autoneg_failed</span> <span class="o">=</span> <span class="mi">0</span><span class="p">;</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Valid Link Found</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="p">}</span>
    <span class="p">}</span> <span class="k">else</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;No Signal Detected</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
    <span class="p">}</span>
    <span class="k">return</span> <span class="mi">0</span><span class="p">;</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm">* Detects which PHY is present and the speed and duplex</span>
<span class="cm">*</span>
<span class="cm">* hw - Struct containing variables accessed by shared code</span>
<span class="cm">******************************************************************************/</span>
<span class="k">static</span> <span class="kt">int32_t</span> 
<span class="n">e1000_setup_copper_link</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">uint32_t</span> <span class="n">ctrl</span><span class="p">;</span>
    <span class="kt">int32_t</span> <span class="n">ret_val</span><span class="p">;</span>
    <span class="kt">uint16_t</span> <span class="n">i</span><span class="p">;</span>
    <span class="kt">uint16_t</span> <span class="n">phy_data</span><span class="p">;</span>

    <span class="n">DEBUGFUNC</span><span class="p">(</span><span class="s">&quot;e1000_setup_copper_link&quot;</span><span class="p">);</span>

    <span class="n">ctrl</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL</span><span class="p">);</span>
    <span class="cm">/* With 82543, we need to force speed and duplex on the MAC equal to what</span>
<span class="cm">     * the PHY speed and duplex configuration is. In addition, we need to</span>
<span class="cm">     * perform a hardware reset on the PHY to take it out of reset.</span>
<span class="cm">     */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">&gt;</span> <span class="n">e1000_82543</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">ctrl</span> <span class="o">|=</span> <span class="n">E1000_CTRL_SLU</span><span class="p">;</span>
        <span class="n">ctrl</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="p">(</span><span class="n">E1000_CTRL_FRCSPD</span> <span class="o">|</span> <span class="n">E1000_CTRL_FRCDPX</span><span class="p">);</span>
        <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL</span><span class="p">,</span> <span class="n">ctrl</span><span class="p">);</span>
    <span class="p">}</span> <span class="k">else</span> <span class="p">{</span>
        <span class="n">ctrl</span> <span class="o">|=</span> <span class="p">(</span><span class="n">E1000_CTRL_FRCSPD</span> <span class="o">|</span> <span class="n">E1000_CTRL_FRCDPX</span> <span class="o">|</span> <span class="n">E1000_CTRL_SLU</span><span class="p">);</span>
        <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL</span><span class="p">,</span> <span class="n">ctrl</span><span class="p">);</span>
        <span class="n">e1000_phy_hw_reset</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
    <span class="p">}</span>

    <span class="cm">/* Make sure we have a valid PHY */</span>
    <span class="n">ret_val</span> <span class="o">=</span> <span class="n">e1000_detect_gig_phy</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
    <span class="k">if</span><span class="p">(</span><span class="n">ret_val</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Error, did not detect valid phy.</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="k">return</span> <span class="n">ret_val</span><span class="p">;</span>
    <span class="p">}</span>
    <span class="n">DEBUGOUT1</span><span class="p">(</span><span class="s">&quot;Phy ID = %x </span><span class="se">\n</span><span class="s">&quot;</span><span class="p">,</span> <span class="n">hw</span><span class="o">-&gt;</span><span class="n">phy_id</span><span class="p">);</span>

    <span class="cm">/* Enable CRS on TX. This must be set for half-duplex operation. */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">M88E1000_PHY_SPEC_CTRL</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">phy_data</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Read Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
    <span class="p">}</span>
    <span class="n">phy_data</span> <span class="o">|=</span> <span class="n">M88E1000_PSCR_ASSERT_CRS_ON_TX</span><span class="p">;</span>

    <span class="cm">/* Options:</span>
<span class="cm">     *   MDI/MDI-X = 0 (default)</span>
<span class="cm">     *   0 - Auto for all speeds</span>
<span class="cm">     *   1 - MDI mode</span>
<span class="cm">     *   2 - MDI-X mode</span>
<span class="cm">     *   3 - Auto for 1000Base-T only (MDI-X for 10/100Base-T modes)</span>
<span class="cm">     */</span>
    <span class="n">phy_data</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="n">M88E1000_PSCR_AUTO_X_MODE</span><span class="p">;</span>

    <span class="k">switch</span> <span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">mdix</span><span class="p">)</span> <span class="p">{</span>
    <span class="k">case</span> <span class="mi">1</span><span class="o">:</span>
        <span class="n">phy_data</span> <span class="o">|=</span> <span class="n">M88E1000_PSCR_MDI_MANUAL_MODE</span><span class="p">;</span>
        <span class="k">break</span><span class="p">;</span>
    <span class="k">case</span> <span class="mi">2</span><span class="o">:</span>
        <span class="n">phy_data</span> <span class="o">|=</span> <span class="n">M88E1000_PSCR_MDIX_MANUAL_MODE</span><span class="p">;</span>
        <span class="k">break</span><span class="p">;</span>
    <span class="k">case</span> <span class="mi">3</span><span class="o">:</span>
        <span class="n">phy_data</span> <span class="o">|=</span> <span class="n">M88E1000_PSCR_AUTO_X_1000T</span><span class="p">;</span>
        <span class="k">break</span><span class="p">;</span>
    <span class="k">case</span> <span class="mi">0</span><span class="o">:</span>
    <span class="k">default</span><span class="o">:</span>
        <span class="n">phy_data</span> <span class="o">|=</span> <span class="n">M88E1000_PSCR_AUTO_X_MODE</span><span class="p">;</span>
        <span class="k">break</span><span class="p">;</span>
    <span class="p">}</span>

    <span class="cm">/* Options:</span>
<span class="cm">     *   disable_polarity_correction = 0 (default)</span>
<span class="cm">     *       Automatic Correction for Reversed Cable Polarity</span>
<span class="cm">     *   0 - Disabled</span>
<span class="cm">     *   1 - Enabled</span>
<span class="cm">     */</span>
    <span class="n">phy_data</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="n">M88E1000_PSCR_POLARITY_REVERSAL</span><span class="p">;</span>
    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">disable_polarity_correction</span> <span class="o">==</span> <span class="mi">1</span><span class="p">)</span>
        <span class="n">phy_data</span> <span class="o">|=</span> <span class="n">M88E1000_PSCR_POLARITY_REVERSAL</span><span class="p">;</span>
    <span class="k">if</span><span class="p">(</span><span class="n">e1000_write_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">M88E1000_PHY_SPEC_CTRL</span><span class="p">,</span> <span class="n">phy_data</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Write Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
    <span class="p">}</span>

    <span class="cm">/* Force TX_CLK in the Extended PHY Specific Control Register</span>
<span class="cm">     * to 25MHz clock.</span>
<span class="cm">     */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">M88E1000_EXT_PHY_SPEC_CTRL</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">phy_data</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Read Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
    <span class="p">}</span>
    <span class="n">phy_data</span> <span class="o">|=</span> <span class="n">M88E1000_EPSCR_TX_CLK_25</span><span class="p">;</span>

    <span class="k">if</span> <span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">phy_revision</span> <span class="o">&lt;</span> <span class="n">M88E1011_I_REV_4</span><span class="p">)</span> <span class="p">{</span>
        <span class="cm">/* Configure Master and Slave downshift values */</span>
        <span class="n">phy_data</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="p">(</span><span class="n">M88E1000_EPSCR_MASTER_DOWNSHIFT_MASK</span> <span class="o">|</span>
                      <span class="n">M88E1000_EPSCR_SLAVE_DOWNSHIFT_MASK</span><span class="p">);</span>
        <span class="n">phy_data</span> <span class="o">|=</span> <span class="p">(</span><span class="n">M88E1000_EPSCR_MASTER_DOWNSHIFT_1X</span> <span class="o">|</span>
                     <span class="n">M88E1000_EPSCR_SLAVE_DOWNSHIFT_1X</span><span class="p">);</span>
        <span class="k">if</span><span class="p">(</span><span class="n">e1000_write_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">M88E1000_EXT_PHY_SPEC_CTRL</span><span class="p">,</span> <span class="n">phy_data</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Write Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
            <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
        <span class="p">}</span>
    <span class="p">}</span>

    <span class="cm">/* SW Reset the PHY so all changes take effect */</span>
    <span class="n">ret_val</span> <span class="o">=</span> <span class="n">e1000_phy_reset</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
    <span class="k">if</span><span class="p">(</span><span class="n">ret_val</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Error Resetting the PHY</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="k">return</span> <span class="n">ret_val</span><span class="p">;</span>
    <span class="p">}</span>
    
    <span class="cm">/* Options:</span>
<span class="cm">     *   autoneg = 1 (default)</span>
<span class="cm">     *      PHY will advertise value(s) parsed from</span>
<span class="cm">     *      autoneg_advertised and fc</span>
<span class="cm">     *   autoneg = 0</span>
<span class="cm">     *      PHY will be set to 10H, 10F, 100H, or 100F</span>
<span class="cm">     *      depending on value parsed from forced_speed_duplex.</span>
<span class="cm">     */</span>

    <span class="cm">/* Is autoneg enabled?  This is enabled by default or by software override.</span>
<span class="cm">     * If so, call e1000_phy_setup_autoneg routine to parse the</span>
<span class="cm">     * autoneg_advertised and fc options. If autoneg is NOT enabled, then the</span>
<span class="cm">     * user should have provided a speed/duplex override.  If so, then call</span>
<span class="cm">     * e1000_phy_force_speed_duplex to parse and set this up.</span>
<span class="cm">     */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">autoneg</span><span class="p">)</span> <span class="p">{</span>
        <span class="cm">/* Perform some bounds checking on the hw-&gt;autoneg_advertised</span>
<span class="cm">         * parameter.  If this variable is zero, then set it to the default.</span>
<span class="cm">         */</span>
        <span class="n">hw</span><span class="o">-&gt;</span><span class="n">autoneg_advertised</span> <span class="o">&amp;=</span> <span class="n">AUTONEG_ADVERTISE_SPEED_DEFAULT</span><span class="p">;</span>

        <span class="cm">/* If autoneg_advertised is zero, we assume it was not defaulted</span>
<span class="cm">         * by the calling code so we set to advertise full capability.</span>
<span class="cm">         */</span>
        <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">autoneg_advertised</span> <span class="o">==</span> <span class="mi">0</span><span class="p">)</span>
            <span class="n">hw</span><span class="o">-&gt;</span><span class="n">autoneg_advertised</span> <span class="o">=</span> <span class="n">AUTONEG_ADVERTISE_SPEED_DEFAULT</span><span class="p">;</span>

        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Reconfiguring auto-neg advertisement params</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="n">ret_val</span> <span class="o">=</span> <span class="n">e1000_phy_setup_autoneg</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
        <span class="k">if</span><span class="p">(</span><span class="n">ret_val</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Error Setting up Auto-Negotiation</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
            <span class="k">return</span> <span class="n">ret_val</span><span class="p">;</span>
        <span class="p">}</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Restarting Auto-Neg</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>

        <span class="cm">/* Restart auto-negotiation by setting the Auto Neg Enable bit and</span>
<span class="cm">         * the Auto Neg Restart bit in the PHY control register.</span>
<span class="cm">         */</span>
        <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_CTRL</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">phy_data</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Read Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
            <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
        <span class="p">}</span>
        <span class="n">phy_data</span> <span class="o">|=</span> <span class="p">(</span><span class="n">MII_CR_AUTO_NEG_EN</span> <span class="o">|</span> <span class="n">MII_CR_RESTART_AUTO_NEG</span><span class="p">);</span>
        <span class="k">if</span><span class="p">(</span><span class="n">e1000_write_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_CTRL</span><span class="p">,</span> <span class="n">phy_data</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Write Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
            <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
        <span class="p">}</span>

        <span class="cm">/* Does the user want to wait for Auto-Neg to complete here, or</span>
<span class="cm">         * check at a later time (for example, callback routine).</span>
<span class="cm">         */</span>
        <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">wait_autoneg_complete</span><span class="p">)</span> <span class="p">{</span>
            <span class="n">ret_val</span> <span class="o">=</span> <span class="n">e1000_wait_autoneg</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
            <span class="k">if</span><span class="p">(</span><span class="n">ret_val</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
                <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Error while waiting for autoneg to complete</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
                <span class="k">return</span> <span class="n">ret_val</span><span class="p">;</span>
            <span class="p">}</span>
        <span class="p">}</span>
    <span class="p">}</span> <span class="k">else</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Forcing speed and duplex</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="n">ret_val</span> <span class="o">=</span> <span class="n">e1000_phy_force_speed_duplex</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
        <span class="k">if</span><span class="p">(</span><span class="n">ret_val</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Error Forcing Speed and Duplex</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
            <span class="k">return</span> <span class="n">ret_val</span><span class="p">;</span>
        <span class="p">}</span>
    <span class="p">}</span>

    <span class="cm">/* Check link status. Wait up to 100 microseconds for link to become</span>
<span class="cm">     * valid.</span>
<span class="cm">     */</span>
    <span class="k">for</span><span class="p">(</span><span class="n">i</span> <span class="o">=</span> <span class="mi">0</span><span class="p">;</span> <span class="n">i</span> <span class="o">&lt;</span> <span class="mi">10</span><span class="p">;</span> <span class="n">i</span><span class="o">++</span><span class="p">)</span> <span class="p">{</span>
        <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_STATUS</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">phy_data</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Read Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
            <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
        <span class="p">}</span>
        <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_STATUS</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">phy_data</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Read Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
            <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
        <span class="p">}</span>
        <span class="k">if</span><span class="p">(</span><span class="n">phy_data</span> <span class="o">&amp;</span> <span class="n">MII_SR_LINK_STATUS</span><span class="p">)</span> <span class="p">{</span>
            <span class="cm">/* We have link, so we need to finish the config process:</span>
<span class="cm">             *   1) Set up the MAC to the current PHY speed/duplex</span>
<span class="cm">             *      if we are on 82543.  If we</span>
<span class="cm">             *      are on newer silicon, we only need to configure</span>
<span class="cm">             *      collision distance in the Transmit Control Register.</span>
<span class="cm">             *   2) Set up flow control on the MAC to that established with</span>
<span class="cm">             *      the link partner.</span>
<span class="cm">             */</span>
            <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">&gt;=</span> <span class="n">e1000_82544</span><span class="p">)</span> <span class="p">{</span>
                <span class="n">e1000_config_collision_dist</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
            <span class="p">}</span> <span class="k">else</span> <span class="p">{</span>
                <span class="n">ret_val</span> <span class="o">=</span> <span class="n">e1000_config_mac_to_phy</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
                <span class="k">if</span><span class="p">(</span><span class="n">ret_val</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
                    <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Error configuring MAC to PHY settings</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
                    <span class="k">return</span> <span class="n">ret_val</span><span class="p">;</span>
                  <span class="p">}</span>
            <span class="p">}</span>
            <span class="n">ret_val</span> <span class="o">=</span> <span class="n">e1000_config_fc_after_link_up</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
            <span class="k">if</span><span class="p">(</span><span class="n">ret_val</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
                <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Error Configuring Flow Control</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
                <span class="k">return</span> <span class="n">ret_val</span><span class="p">;</span>
            <span class="p">}</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Valid link established!!!</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
            <span class="k">return</span> <span class="mi">0</span><span class="p">;</span>
        <span class="p">}</span>
        <span class="n">udelay</span><span class="p">(</span><span class="mi">10</span><span class="p">);</span>
    <span class="p">}</span>

    <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Unable to establish link!!!</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
    <span class="k">return</span> <span class="mi">0</span><span class="p">;</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm">* Configures PHY autoneg and flow control advertisement settings</span>
<span class="cm">*</span>
<span class="cm">* hw - Struct containing variables accessed by shared code</span>
<span class="cm">******************************************************************************/</span>
<span class="kt">int32_t</span>
<span class="n">e1000_phy_setup_autoneg</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">uint16_t</span> <span class="n">mii_autoneg_adv_reg</span><span class="p">;</span>
    <span class="kt">uint16_t</span> <span class="n">mii_1000t_ctrl_reg</span><span class="p">;</span>

    <span class="n">DEBUGFUNC</span><span class="p">(</span><span class="s">&quot;e1000_phy_setup_autoneg&quot;</span><span class="p">);</span>

    <span class="cm">/* Read the MII Auto-Neg Advertisement Register (Address 4). */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_AUTONEG_ADV</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">mii_autoneg_adv_reg</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Read Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
    <span class="p">}</span>

    <span class="cm">/* Read the MII 1000Base-T Control Register (Address 9). */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_1000T_CTRL</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">mii_1000t_ctrl_reg</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Read Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
    <span class="p">}</span>

    <span class="cm">/* Need to parse both autoneg_advertised and fc and set up</span>
<span class="cm">     * the appropriate PHY registers.  First we will parse for</span>
<span class="cm">     * autoneg_advertised software override.  Since we can advertise</span>
<span class="cm">     * a plethora of combinations, we need to check each bit</span>
<span class="cm">     * individually.</span>
<span class="cm">     */</span>

    <span class="cm">/* First we clear all the 10/100 mb speed bits in the Auto-Neg</span>
<span class="cm">     * Advertisement Register (Address 4) and the 1000 mb speed bits in</span>
<span class="cm">     * the  1000Base-T Control Register (Address 9).</span>
<span class="cm">     */</span>
    <span class="n">mii_autoneg_adv_reg</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="n">REG4_SPEED_MASK</span><span class="p">;</span>
    <span class="n">mii_1000t_ctrl_reg</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="n">REG9_SPEED_MASK</span><span class="p">;</span>

    <span class="n">DEBUGOUT1</span><span class="p">(</span><span class="s">&quot;autoneg_advertised %x</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">,</span> <span class="n">hw</span><span class="o">-&gt;</span><span class="n">autoneg_advertised</span><span class="p">);</span>

    <span class="cm">/* Do we want to advertise 10 Mb Half Duplex? */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">autoneg_advertised</span> <span class="o">&amp;</span> <span class="n">ADVERTISE_10_HALF</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Advertise 10mb Half duplex</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="n">mii_autoneg_adv_reg</span> <span class="o">|=</span> <span class="n">NWAY_AR_10T_HD_CAPS</span><span class="p">;</span>
    <span class="p">}</span>

    <span class="cm">/* Do we want to advertise 10 Mb Full Duplex? */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">autoneg_advertised</span> <span class="o">&amp;</span> <span class="n">ADVERTISE_10_FULL</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Advertise 10mb Full duplex</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="n">mii_autoneg_adv_reg</span> <span class="o">|=</span> <span class="n">NWAY_AR_10T_FD_CAPS</span><span class="p">;</span>
    <span class="p">}</span>

    <span class="cm">/* Do we want to advertise 100 Mb Half Duplex? */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">autoneg_advertised</span> <span class="o">&amp;</span> <span class="n">ADVERTISE_100_HALF</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Advertise 100mb Half duplex</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="n">mii_autoneg_adv_reg</span> <span class="o">|=</span> <span class="n">NWAY_AR_100TX_HD_CAPS</span><span class="p">;</span>
    <span class="p">}</span>

    <span class="cm">/* Do we want to advertise 100 Mb Full Duplex? */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">autoneg_advertised</span> <span class="o">&amp;</span> <span class="n">ADVERTISE_100_FULL</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Advertise 100mb Full duplex</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="n">mii_autoneg_adv_reg</span> <span class="o">|=</span> <span class="n">NWAY_AR_100TX_FD_CAPS</span><span class="p">;</span>
    <span class="p">}</span>

    <span class="cm">/* We do not allow the Phy to advertise 1000 Mb Half Duplex */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">autoneg_advertised</span> <span class="o">&amp;</span> <span class="n">ADVERTISE_1000_HALF</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Advertise 1000mb Half duplex requested, request denied!</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
    <span class="p">}</span>

    <span class="cm">/* Do we want to advertise 1000 Mb Full Duplex? */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">autoneg_advertised</span> <span class="o">&amp;</span> <span class="n">ADVERTISE_1000_FULL</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Advertise 1000mb Full duplex</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="n">mii_1000t_ctrl_reg</span> <span class="o">|=</span> <span class="n">CR_1000T_FD_CAPS</span><span class="p">;</span>
    <span class="p">}</span>

    <span class="cm">/* Check for a software override of the flow control settings, and</span>
<span class="cm">     * setup the PHY advertisement registers accordingly.  If</span>
<span class="cm">     * auto-negotiation is enabled, then software will have to set the</span>
<span class="cm">     * &quot;PAUSE&quot; bits to the correct value in the Auto-Negotiation</span>
<span class="cm">     * Advertisement Register (PHY_AUTONEG_ADV) and re-start auto-negotiation.</span>
<span class="cm">     *</span>
<span class="cm">     * The possible values of the &quot;fc&quot; parameter are:</span>
<span class="cm">     *      0:  Flow control is completely disabled</span>
<span class="cm">     *      1:  Rx flow control is enabled (we can receive pause frames</span>
<span class="cm">     *          but not send pause frames).</span>
<span class="cm">     *      2:  Tx flow control is enabled (we can send pause frames</span>
<span class="cm">     *          but we do not support receiving pause frames).</span>
<span class="cm">     *      3:  Both Rx and TX flow control (symmetric) are enabled.</span>
<span class="cm">     *  other:  No software override.  The flow control configuration</span>
<span class="cm">     *          in the EEPROM is used.</span>
<span class="cm">     */</span>
    <span class="k">switch</span> <span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">fc</span><span class="p">)</span> <span class="p">{</span>
    <span class="k">case</span> <span class="nl">e1000_fc_none</span><span class="p">:</span> <span class="cm">/* 0 */</span>
        <span class="cm">/* Flow control (RX &amp; TX) is completely disabled by a</span>
<span class="cm">         * software over-ride.</span>
<span class="cm">         */</span>
        <span class="n">mii_autoneg_adv_reg</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="p">(</span><span class="n">NWAY_AR_ASM_DIR</span> <span class="o">|</span> <span class="n">NWAY_AR_PAUSE</span><span class="p">);</span>
        <span class="k">break</span><span class="p">;</span>
    <span class="k">case</span> <span class="nl">e1000_fc_rx_pause</span><span class="p">:</span> <span class="cm">/* 1 */</span>
        <span class="cm">/* RX Flow control is enabled, and TX Flow control is</span>
<span class="cm">         * disabled, by a software over-ride.</span>
<span class="cm">         */</span>
        <span class="cm">/* Since there really isn&#39;t a way to advertise that we are</span>
<span class="cm">         * capable of RX Pause ONLY, we will advertise that we</span>
<span class="cm">         * support both symmetric and asymmetric RX PAUSE.  Later</span>
<span class="cm">         * (in e1000_config_fc_after_link_up) we will disable the</span>
<span class="cm">         *hw&#39;s ability to send PAUSE frames.</span>
<span class="cm">         */</span>
        <span class="n">mii_autoneg_adv_reg</span> <span class="o">|=</span> <span class="p">(</span><span class="n">NWAY_AR_ASM_DIR</span> <span class="o">|</span> <span class="n">NWAY_AR_PAUSE</span><span class="p">);</span>
        <span class="k">break</span><span class="p">;</span>
    <span class="k">case</span> <span class="nl">e1000_fc_tx_pause</span><span class="p">:</span> <span class="cm">/* 2 */</span>
        <span class="cm">/* TX Flow control is enabled, and RX Flow control is</span>
<span class="cm">         * disabled, by a software over-ride.</span>
<span class="cm">         */</span>
        <span class="n">mii_autoneg_adv_reg</span> <span class="o">|=</span> <span class="n">NWAY_AR_ASM_DIR</span><span class="p">;</span>
        <span class="n">mii_autoneg_adv_reg</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="n">NWAY_AR_PAUSE</span><span class="p">;</span>
        <span class="k">break</span><span class="p">;</span>
    <span class="k">case</span> <span class="nl">e1000_fc_full</span><span class="p">:</span> <span class="cm">/* 3 */</span>
        <span class="cm">/* Flow control (both RX and TX) is enabled by a software</span>
<span class="cm">         * over-ride.</span>
<span class="cm">         */</span>
        <span class="n">mii_autoneg_adv_reg</span> <span class="o">|=</span> <span class="p">(</span><span class="n">NWAY_AR_ASM_DIR</span> <span class="o">|</span> <span class="n">NWAY_AR_PAUSE</span><span class="p">);</span>
        <span class="k">break</span><span class="p">;</span>
    <span class="k">default</span><span class="o">:</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Flow control param set incorrectly</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_CONFIG</span><span class="p">;</span>
    <span class="p">}</span>

    <span class="k">if</span><span class="p">(</span><span class="n">e1000_write_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_AUTONEG_ADV</span><span class="p">,</span> <span class="n">mii_autoneg_adv_reg</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Write Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
    <span class="p">}</span>

    <span class="n">DEBUGOUT1</span><span class="p">(</span><span class="s">&quot;Auto-Neg Advertising %x</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">,</span> <span class="n">mii_autoneg_adv_reg</span><span class="p">);</span>

    <span class="k">if</span><span class="p">(</span><span class="n">e1000_write_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_1000T_CTRL</span><span class="p">,</span> <span class="n">mii_1000t_ctrl_reg</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Write Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
    <span class="p">}</span>
    <span class="k">return</span> <span class="mi">0</span><span class="p">;</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm">* Force PHY speed and duplex settings to hw-&gt;forced_speed_duplex</span>
<span class="cm">*</span>
<span class="cm">* hw - Struct containing variables accessed by shared code</span>
<span class="cm">******************************************************************************/</span>
<span class="k">static</span> <span class="kt">int32_t</span>
<span class="n">e1000_phy_force_speed_duplex</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">uint32_t</span> <span class="n">ctrl</span><span class="p">;</span>
    <span class="kt">int32_t</span> <span class="n">ret_val</span><span class="p">;</span>
    <span class="kt">uint16_t</span> <span class="n">mii_ctrl_reg</span><span class="p">;</span>
    <span class="kt">uint16_t</span> <span class="n">mii_status_reg</span><span class="p">;</span>
    <span class="kt">uint16_t</span> <span class="n">phy_data</span><span class="p">;</span>
    <span class="kt">uint16_t</span> <span class="n">i</span><span class="p">;</span>

    <span class="n">DEBUGFUNC</span><span class="p">(</span><span class="s">&quot;e1000_phy_force_speed_duplex&quot;</span><span class="p">);</span>

    <span class="cm">/* Turn off Flow control if we are forcing speed and duplex. */</span>
    <span class="n">hw</span><span class="o">-&gt;</span><span class="n">fc</span> <span class="o">=</span> <span class="n">e1000_fc_none</span><span class="p">;</span>

    <span class="n">DEBUGOUT1</span><span class="p">(</span><span class="s">&quot;hw-&gt;fc = %d</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">,</span> <span class="n">hw</span><span class="o">-&gt;</span><span class="n">fc</span><span class="p">);</span>

    <span class="cm">/* Read the Device Control Register. */</span>
    <span class="n">ctrl</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL</span><span class="p">);</span>

    <span class="cm">/* Set the bits to Force Speed and Duplex in the Device Ctrl Reg. */</span>
    <span class="n">ctrl</span> <span class="o">|=</span> <span class="p">(</span><span class="n">E1000_CTRL_FRCSPD</span> <span class="o">|</span> <span class="n">E1000_CTRL_FRCDPX</span><span class="p">);</span>
    <span class="n">ctrl</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="p">(</span><span class="n">DEVICE_SPEED_MASK</span><span class="p">);</span>

    <span class="cm">/* Clear the Auto Speed Detect Enable bit. */</span>
    <span class="n">ctrl</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="n">E1000_CTRL_ASDE</span><span class="p">;</span>

    <span class="cm">/* Read the MII Control Register. */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_CTRL</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">mii_ctrl_reg</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Read Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
    <span class="p">}</span>

    <span class="cm">/* We need to disable autoneg in order to force link and duplex. */</span>

    <span class="n">mii_ctrl_reg</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="n">MII_CR_AUTO_NEG_EN</span><span class="p">;</span>

    <span class="cm">/* Are we forcing Full or Half Duplex? */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">forced_speed_duplex</span> <span class="o">==</span> <span class="n">e1000_100_full</span> <span class="o">||</span>
       <span class="n">hw</span><span class="o">-&gt;</span><span class="n">forced_speed_duplex</span> <span class="o">==</span> <span class="n">e1000_10_full</span><span class="p">)</span> <span class="p">{</span>
        <span class="cm">/* We want to force full duplex so we SET the full duplex bits in the</span>
<span class="cm">         * Device and MII Control Registers.</span>
<span class="cm">         */</span>
        <span class="n">ctrl</span> <span class="o">|=</span> <span class="n">E1000_CTRL_FD</span><span class="p">;</span>
        <span class="n">mii_ctrl_reg</span> <span class="o">|=</span> <span class="n">MII_CR_FULL_DUPLEX</span><span class="p">;</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Full Duplex</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
    <span class="p">}</span> <span class="k">else</span> <span class="p">{</span>
        <span class="cm">/* We want to force half duplex so we CLEAR the full duplex bits in</span>
<span class="cm">         * the Device and MII Control Registers.</span>
<span class="cm">         */</span>
        <span class="n">ctrl</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="n">E1000_CTRL_FD</span><span class="p">;</span>
        <span class="n">mii_ctrl_reg</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="n">MII_CR_FULL_DUPLEX</span><span class="p">;</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Half Duplex</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
    <span class="p">}</span>

    <span class="cm">/* Are we forcing 100Mbps??? */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">forced_speed_duplex</span> <span class="o">==</span> <span class="n">e1000_100_full</span> <span class="o">||</span>
       <span class="n">hw</span><span class="o">-&gt;</span><span class="n">forced_speed_duplex</span> <span class="o">==</span> <span class="n">e1000_100_half</span><span class="p">)</span> <span class="p">{</span>
        <span class="cm">/* Set the 100Mb bit and turn off the 1000Mb and 10Mb bits. */</span>
        <span class="n">ctrl</span> <span class="o">|=</span> <span class="n">E1000_CTRL_SPD_100</span><span class="p">;</span>
        <span class="n">mii_ctrl_reg</span> <span class="o">|=</span> <span class="n">MII_CR_SPEED_100</span><span class="p">;</span>
        <span class="n">mii_ctrl_reg</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="p">(</span><span class="n">MII_CR_SPEED_1000</span> <span class="o">|</span> <span class="n">MII_CR_SPEED_10</span><span class="p">);</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Forcing 100mb &quot;</span><span class="p">);</span>
    <span class="p">}</span> <span class="k">else</span> <span class="p">{</span>
        <span class="cm">/* Set the 10Mb bit and turn off the 1000Mb and 100Mb bits. */</span>
        <span class="n">ctrl</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="p">(</span><span class="n">E1000_CTRL_SPD_1000</span> <span class="o">|</span> <span class="n">E1000_CTRL_SPD_100</span><span class="p">);</span>
        <span class="n">mii_ctrl_reg</span> <span class="o">|=</span> <span class="n">MII_CR_SPEED_10</span><span class="p">;</span>
        <span class="n">mii_ctrl_reg</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="p">(</span><span class="n">MII_CR_SPEED_1000</span> <span class="o">|</span> <span class="n">MII_CR_SPEED_100</span><span class="p">);</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Forcing 10mb &quot;</span><span class="p">);</span>
    <span class="p">}</span>

    <span class="n">e1000_config_collision_dist</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>

    <span class="cm">/* Write the configured values back to the Device Control Reg. */</span>
    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL</span><span class="p">,</span> <span class="n">ctrl</span><span class="p">);</span>

    <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">M88E1000_PHY_SPEC_CTRL</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">phy_data</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Read Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
    <span class="p">}</span>

    <span class="cm">/* Clear Auto-Crossover to force MDI manually. M88E1000 requires MDI</span>
<span class="cm">     * forced whenever speed are duplex are forced.</span>
<span class="cm">     */</span>
    <span class="n">phy_data</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="n">M88E1000_PSCR_AUTO_X_MODE</span><span class="p">;</span>
    <span class="k">if</span><span class="p">(</span><span class="n">e1000_write_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">M88E1000_PHY_SPEC_CTRL</span><span class="p">,</span> <span class="n">phy_data</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Write Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
    <span class="p">}</span>
    <span class="n">DEBUGOUT1</span><span class="p">(</span><span class="s">&quot;M88E1000 PSCR: %x </span><span class="se">\n</span><span class="s">&quot;</span><span class="p">,</span> <span class="n">phy_data</span><span class="p">);</span>

    <span class="cm">/* Need to reset the PHY or these changes will be ignored */</span>
    <span class="n">mii_ctrl_reg</span> <span class="o">|=</span> <span class="n">MII_CR_RESET</span><span class="p">;</span>

    <span class="cm">/* Write back the modified PHY MII control register. */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">e1000_write_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_CTRL</span><span class="p">,</span> <span class="n">mii_ctrl_reg</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Write Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
    <span class="p">}</span>
    <span class="n">udelay</span><span class="p">(</span><span class="mi">1</span><span class="p">);</span>

    <span class="cm">/* The wait_autoneg_complete flag may be a little misleading here.</span>
<span class="cm">     * Since we are forcing speed and duplex, Auto-Neg is not enabled.</span>
<span class="cm">     * But we do want to delay for a period while forcing only so we</span>
<span class="cm">     * don&#39;t generate false No Link messages.  So we will wait here</span>
<span class="cm">     * only if the user has set wait_autoneg_complete to 1, which is</span>
<span class="cm">     * the default.</span>
<span class="cm">     */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">wait_autoneg_complete</span><span class="p">)</span> <span class="p">{</span>
        <span class="cm">/* We will wait for autoneg to complete. */</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Waiting for forced speed/duplex link.</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="n">mii_status_reg</span> <span class="o">=</span> <span class="mi">0</span><span class="p">;</span>

        <span class="cm">/* We will wait for autoneg to complete or 4.5 seconds to expire. */</span>
        <span class="k">for</span><span class="p">(</span><span class="n">i</span> <span class="o">=</span> <span class="n">PHY_FORCE_TIME</span><span class="p">;</span> <span class="n">i</span> <span class="o">&gt;</span> <span class="mi">0</span><span class="p">;</span> <span class="n">i</span><span class="o">--</span><span class="p">)</span> <span class="p">{</span>
            <span class="cm">/* Read the MII Status Register and wait for Auto-Neg Complete bit</span>
<span class="cm">             * to be set.</span>
<span class="cm">             */</span>
            <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_STATUS</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">mii_status_reg</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
                <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Read Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
                <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
            <span class="p">}</span>
            <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_STATUS</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">mii_status_reg</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
                <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Read Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
                <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
            <span class="p">}</span>
            <span class="k">if</span><span class="p">(</span><span class="n">mii_status_reg</span> <span class="o">&amp;</span> <span class="n">MII_SR_LINK_STATUS</span><span class="p">)</span> <span class="k">break</span><span class="p">;</span>
            <span class="n">msec_delay</span><span class="p">(</span><span class="mi">100</span><span class="p">);</span>
        <span class="p">}</span>
        <span class="k">if</span><span class="p">(</span><span class="n">i</span> <span class="o">==</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span> <span class="cm">/* We didn&#39;t get link */</span>
            <span class="cm">/* Reset the DSP and wait again for link. */</span>
            
            <span class="n">ret_val</span> <span class="o">=</span> <span class="n">e1000_phy_reset_dsp</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
            <span class="k">if</span><span class="p">(</span><span class="n">ret_val</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
                <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Error Resetting PHY DSP</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
                <span class="k">return</span> <span class="n">ret_val</span><span class="p">;</span>
            <span class="p">}</span>
        <span class="p">}</span>
        <span class="cm">/* This loop will early-out if the link condition has been met.  */</span>
        <span class="k">for</span><span class="p">(</span><span class="n">i</span> <span class="o">=</span> <span class="n">PHY_FORCE_TIME</span><span class="p">;</span> <span class="n">i</span> <span class="o">&gt;</span> <span class="mi">0</span><span class="p">;</span> <span class="n">i</span><span class="o">--</span><span class="p">)</span> <span class="p">{</span>
            <span class="k">if</span><span class="p">(</span><span class="n">mii_status_reg</span> <span class="o">&amp;</span> <span class="n">MII_SR_LINK_STATUS</span><span class="p">)</span> <span class="k">break</span><span class="p">;</span>
            <span class="n">msec_delay</span><span class="p">(</span><span class="mi">100</span><span class="p">);</span>
            <span class="cm">/* Read the MII Status Register and wait for Auto-Neg Complete bit</span>
<span class="cm">             * to be set.</span>
<span class="cm">             */</span>
            <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_STATUS</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">mii_status_reg</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
                <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Read Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
                <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
            <span class="p">}</span>
            <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_STATUS</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">mii_status_reg</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
                <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Read Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
                <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
            <span class="p">}</span>
        <span class="p">}</span>
    <span class="p">}</span>
    
    <span class="cm">/* Because we reset the PHY above, we need to re-force TX_CLK in the</span>
<span class="cm">     * Extended PHY Specific Control Register to 25MHz clock.  This value</span>
<span class="cm">     * defaults back to a 2.5MHz clock when the PHY is reset.</span>
<span class="cm">     */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">M88E1000_EXT_PHY_SPEC_CTRL</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">phy_data</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Read Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
    <span class="p">}</span>
    <span class="n">phy_data</span> <span class="o">|=</span> <span class="n">M88E1000_EPSCR_TX_CLK_25</span><span class="p">;</span>
    <span class="k">if</span><span class="p">(</span><span class="n">e1000_write_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">M88E1000_EXT_PHY_SPEC_CTRL</span><span class="p">,</span> <span class="n">phy_data</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Write Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
    <span class="p">}</span>

    <span class="cm">/* In addition, because of the s/w reset above, we need to enable CRS on</span>
<span class="cm">     * TX.  This must be set for both full and half duplex operation.</span>
<span class="cm">     */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">M88E1000_PHY_SPEC_CTRL</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">phy_data</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Read Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
    <span class="p">}</span>
    <span class="n">phy_data</span> <span class="o">|=</span> <span class="n">M88E1000_PSCR_ASSERT_CRS_ON_TX</span><span class="p">;</span>
    <span class="k">if</span><span class="p">(</span><span class="n">e1000_write_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">M88E1000_PHY_SPEC_CTRL</span><span class="p">,</span> <span class="n">phy_data</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Write Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
    <span class="p">}</span>
    <span class="k">return</span> <span class="mi">0</span><span class="p">;</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm">* Sets the collision distance in the Transmit Control register</span>
<span class="cm">*</span>
<span class="cm">* hw - Struct containing variables accessed by shared code</span>
<span class="cm">*</span>
<span class="cm">* Link should have been established previously. Reads the speed and duplex</span>
<span class="cm">* information from the Device Status register.</span>
<span class="cm">******************************************************************************/</span>
<span class="kt">void</span>
<span class="n">e1000_config_collision_dist</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">uint32_t</span> <span class="n">tctl</span><span class="p">;</span>

    <span class="n">tctl</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">TCTL</span><span class="p">);</span>

    <span class="n">tctl</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="n">E1000_TCTL_COLD</span><span class="p">;</span>
    <span class="n">tctl</span> <span class="o">|=</span> <span class="n">E1000_COLLISION_DISTANCE</span> <span class="o">&lt;&lt;</span> <span class="n">E1000_COLD_SHIFT</span><span class="p">;</span>

    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">TCTL</span><span class="p">,</span> <span class="n">tctl</span><span class="p">);</span>
    <span class="n">E1000_WRITE_FLUSH</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm">* Sets MAC speed and duplex settings to reflect the those in the PHY</span>
<span class="cm">*</span>
<span class="cm">* hw - Struct containing variables accessed by shared code</span>
<span class="cm">* mii_reg - data to write to the MII control register</span>
<span class="cm">*</span>
<span class="cm">* The contents of the PHY register containing the needed information need to</span>
<span class="cm">* be passed in.</span>
<span class="cm">******************************************************************************/</span>
<span class="k">static</span> <span class="kt">int32_t</span>
<span class="n">e1000_config_mac_to_phy</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">uint32_t</span> <span class="n">ctrl</span><span class="p">;</span>
    <span class="kt">uint16_t</span> <span class="n">phy_data</span><span class="p">;</span>

    <span class="n">DEBUGFUNC</span><span class="p">(</span><span class="s">&quot;e1000_config_mac_to_phy&quot;</span><span class="p">);</span>

    <span class="cm">/* Read the Device Control Register and set the bits to Force Speed</span>
<span class="cm">     * and Duplex.</span>
<span class="cm">     */</span>
    <span class="n">ctrl</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL</span><span class="p">);</span>
    <span class="n">ctrl</span> <span class="o">|=</span> <span class="p">(</span><span class="n">E1000_CTRL_FRCSPD</span> <span class="o">|</span> <span class="n">E1000_CTRL_FRCDPX</span><span class="p">);</span>
    <span class="n">ctrl</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="p">(</span><span class="n">E1000_CTRL_SPD_SEL</span> <span class="o">|</span> <span class="n">E1000_CTRL_ILOS</span><span class="p">);</span>

    <span class="cm">/* Set up duplex in the Device Control and Transmit Control</span>
<span class="cm">     * registers depending on negotiated values.</span>
<span class="cm">     */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">M88E1000_PHY_SPEC_STATUS</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">phy_data</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Read Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
    <span class="p">}</span>
    <span class="k">if</span><span class="p">(</span><span class="n">phy_data</span> <span class="o">&amp;</span> <span class="n">M88E1000_PSSR_DPLX</span><span class="p">)</span> <span class="n">ctrl</span> <span class="o">|=</span> <span class="n">E1000_CTRL_FD</span><span class="p">;</span>
    <span class="k">else</span> <span class="n">ctrl</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="n">E1000_CTRL_FD</span><span class="p">;</span>

    <span class="n">e1000_config_collision_dist</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>

    <span class="cm">/* Set up speed in the Device Control register depending on</span>
<span class="cm">     * negotiated values.</span>
<span class="cm">     */</span>
    <span class="k">if</span><span class="p">((</span><span class="n">phy_data</span> <span class="o">&amp;</span> <span class="n">M88E1000_PSSR_SPEED</span><span class="p">)</span> <span class="o">==</span> <span class="n">M88E1000_PSSR_1000MBS</span><span class="p">)</span>
        <span class="n">ctrl</span> <span class="o">|=</span> <span class="n">E1000_CTRL_SPD_1000</span><span class="p">;</span>
    <span class="k">else</span> <span class="nf">if</span><span class="p">((</span><span class="n">phy_data</span> <span class="o">&amp;</span> <span class="n">M88E1000_PSSR_SPEED</span><span class="p">)</span> <span class="o">==</span> <span class="n">M88E1000_PSSR_100MBS</span><span class="p">)</span>
        <span class="n">ctrl</span> <span class="o">|=</span> <span class="n">E1000_CTRL_SPD_100</span><span class="p">;</span>
    <span class="cm">/* Write the configured values back to the Device Control Reg. */</span>
    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL</span><span class="p">,</span> <span class="n">ctrl</span><span class="p">);</span>
    <span class="k">return</span> <span class="mi">0</span><span class="p">;</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm"> * Forces the MAC&#39;s flow control settings.</span>
<span class="cm"> * </span>
<span class="cm"> * hw - Struct containing variables accessed by shared code</span>
<span class="cm"> *</span>
<span class="cm"> * Sets the TFCE and RFCE bits in the device control register to reflect</span>
<span class="cm"> * the adapter settings. TFCE and RFCE need to be explicitly set by</span>
<span class="cm"> * software when a Copper PHY is used because autonegotiation is managed</span>
<span class="cm"> * by the PHY rather than the MAC. Software must also configure these</span>
<span class="cm"> * bits when link is forced on a fiber connection.</span>
<span class="cm"> *****************************************************************************/</span>
<span class="k">static</span> <span class="kt">int32_t</span>
<span class="n">e1000_force_mac_fc</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">uint32_t</span> <span class="n">ctrl</span><span class="p">;</span>

    <span class="n">DEBUGFUNC</span><span class="p">(</span><span class="s">&quot;e1000_force_mac_fc&quot;</span><span class="p">);</span>

    <span class="cm">/* Get the current configuration of the Device Control Register */</span>
    <span class="n">ctrl</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL</span><span class="p">);</span>

    <span class="cm">/* Because we didn&#39;t get link via the internal auto-negotiation</span>
<span class="cm">     * mechanism (we either forced link or we got link via PHY</span>
<span class="cm">     * auto-neg), we have to manually enable/disable transmit an</span>
<span class="cm">     * receive flow control.</span>
<span class="cm">     *</span>
<span class="cm">     * The &quot;Case&quot; statement below enables/disable flow control</span>
<span class="cm">     * according to the &quot;hw-&gt;fc&quot; parameter.</span>
<span class="cm">     *</span>
<span class="cm">     * The possible values of the &quot;fc&quot; parameter are:</span>
<span class="cm">     *      0:  Flow control is completely disabled</span>
<span class="cm">     *      1:  Rx flow control is enabled (we can receive pause</span>
<span class="cm">     *          frames but not send pause frames).</span>
<span class="cm">     *      2:  Tx flow control is enabled (we can send pause frames</span>
<span class="cm">     *          frames but we do not receive pause frames).</span>
<span class="cm">     *      3:  Both Rx and TX flow control (symmetric) is enabled.</span>
<span class="cm">     *  other:  No other values should be possible at this point.</span>
<span class="cm">     */</span>

    <span class="k">switch</span> <span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">fc</span><span class="p">)</span> <span class="p">{</span>
    <span class="k">case</span> <span class="nl">e1000_fc_none</span><span class="p">:</span>
        <span class="n">ctrl</span> <span class="o">&amp;=</span> <span class="p">(</span><span class="o">~</span><span class="p">(</span><span class="n">E1000_CTRL_TFCE</span> <span class="o">|</span> <span class="n">E1000_CTRL_RFCE</span><span class="p">));</span>
        <span class="k">break</span><span class="p">;</span>
    <span class="k">case</span> <span class="nl">e1000_fc_rx_pause</span><span class="p">:</span>
        <span class="n">ctrl</span> <span class="o">&amp;=</span> <span class="p">(</span><span class="o">~</span><span class="n">E1000_CTRL_TFCE</span><span class="p">);</span>
        <span class="n">ctrl</span> <span class="o">|=</span> <span class="n">E1000_CTRL_RFCE</span><span class="p">;</span>
        <span class="k">break</span><span class="p">;</span>
    <span class="k">case</span> <span class="nl">e1000_fc_tx_pause</span><span class="p">:</span>
        <span class="n">ctrl</span> <span class="o">&amp;=</span> <span class="p">(</span><span class="o">~</span><span class="n">E1000_CTRL_RFCE</span><span class="p">);</span>
        <span class="n">ctrl</span> <span class="o">|=</span> <span class="n">E1000_CTRL_TFCE</span><span class="p">;</span>
        <span class="k">break</span><span class="p">;</span>
    <span class="k">case</span> <span class="nl">e1000_fc_full</span><span class="p">:</span>
        <span class="n">ctrl</span> <span class="o">|=</span> <span class="p">(</span><span class="n">E1000_CTRL_TFCE</span> <span class="o">|</span> <span class="n">E1000_CTRL_RFCE</span><span class="p">);</span>
        <span class="k">break</span><span class="p">;</span>
    <span class="k">default</span><span class="o">:</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Flow control param set incorrectly</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_CONFIG</span><span class="p">;</span>
    <span class="p">}</span>

    <span class="cm">/* Disable TX Flow Control for 82542 (rev 2.0) */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">==</span> <span class="n">e1000_82542_rev2_0</span><span class="p">)</span>
        <span class="n">ctrl</span> <span class="o">&amp;=</span> <span class="p">(</span><span class="o">~</span><span class="n">E1000_CTRL_TFCE</span><span class="p">);</span>

    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL</span><span class="p">,</span> <span class="n">ctrl</span><span class="p">);</span>
    <span class="k">return</span> <span class="mi">0</span><span class="p">;</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm"> * Configures flow control settings after link is established</span>
<span class="cm"> * </span>
<span class="cm"> * hw - Struct containing variables accessed by shared code</span>
<span class="cm"> *</span>
<span class="cm"> * Should be called immediately after a valid link has been established.</span>
<span class="cm"> * Forces MAC flow control settings if link was forced. When in MII/GMII mode</span>
<span class="cm"> * and autonegotiation is enabled, the MAC flow control settings will be set</span>
<span class="cm"> * based on the flow control negotiated by the PHY. In TBI mode, the TFCE</span>
<span class="cm"> * and RFCE bits will be automaticaly set to the negotiated flow control mode.</span>
<span class="cm"> *****************************************************************************/</span>
<span class="kt">int32_t</span>
<span class="n">e1000_config_fc_after_link_up</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">int32_t</span> <span class="n">ret_val</span><span class="p">;</span>
    <span class="kt">uint16_t</span> <span class="n">mii_status_reg</span><span class="p">;</span>
    <span class="kt">uint16_t</span> <span class="n">mii_nway_adv_reg</span><span class="p">;</span>
    <span class="kt">uint16_t</span> <span class="n">mii_nway_lp_ability_reg</span><span class="p">;</span>
    <span class="kt">uint16_t</span> <span class="n">speed</span><span class="p">;</span>
    <span class="kt">uint16_t</span> <span class="n">duplex</span><span class="p">;</span>

    <span class="n">DEBUGFUNC</span><span class="p">(</span><span class="s">&quot;e1000_config_fc_after_link_up&quot;</span><span class="p">);</span>

    <span class="cm">/* Check for the case where we have fiber media and auto-neg failed</span>
<span class="cm">     * so we had to force link.  In this case, we need to force the</span>
<span class="cm">     * configuration of the MAC to match the &quot;fc&quot; parameter.</span>
<span class="cm">     */</span>
    <span class="k">if</span><span class="p">(((</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">media_type</span> <span class="o">==</span> <span class="n">e1000_media_type_fiber</span><span class="p">)</span> <span class="o">&amp;&amp;</span> <span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">autoneg_failed</span><span class="p">))</span> <span class="o">||</span>
       <span class="p">((</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">media_type</span> <span class="o">==</span> <span class="n">e1000_media_type_copper</span><span class="p">)</span> <span class="o">&amp;&amp;</span> <span class="p">(</span><span class="o">!</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">autoneg</span><span class="p">)))</span> <span class="p">{</span>
        <span class="n">ret_val</span> <span class="o">=</span> <span class="n">e1000_force_mac_fc</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
        <span class="k">if</span><span class="p">(</span><span class="n">ret_val</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Error forcing flow control settings</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
            <span class="k">return</span> <span class="n">ret_val</span><span class="p">;</span>
        <span class="p">}</span>
    <span class="p">}</span>

    <span class="cm">/* Check for the case where we have copper media and auto-neg is</span>
<span class="cm">     * enabled.  In this case, we need to check and see if Auto-Neg</span>
<span class="cm">     * has completed, and if so, how the PHY and link partner has</span>
<span class="cm">     * flow control configured.</span>
<span class="cm">     */</span>
    <span class="k">if</span><span class="p">((</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">media_type</span> <span class="o">==</span> <span class="n">e1000_media_type_copper</span><span class="p">)</span> <span class="o">&amp;&amp;</span> <span class="n">hw</span><span class="o">-&gt;</span><span class="n">autoneg</span><span class="p">)</span> <span class="p">{</span>
        <span class="cm">/* Read the MII Status Register and check to see if AutoNeg</span>
<span class="cm">         * has completed.  We read this twice because this reg has</span>
<span class="cm">         * some &quot;sticky&quot; (latched) bits.</span>
<span class="cm">         */</span>
        <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_STATUS</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">mii_status_reg</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Read Error </span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
            <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
        <span class="p">}</span>
        <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_STATUS</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">mii_status_reg</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Read Error </span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
            <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
        <span class="p">}</span>

        <span class="k">if</span><span class="p">(</span><span class="n">mii_status_reg</span> <span class="o">&amp;</span> <span class="n">MII_SR_AUTONEG_COMPLETE</span><span class="p">)</span> <span class="p">{</span>
            <span class="cm">/* The AutoNeg process has completed, so we now need to</span>
<span class="cm">             * read both the Auto Negotiation Advertisement Register</span>
<span class="cm">             * (Address 4) and the Auto_Negotiation Base Page Ability</span>
<span class="cm">             * Register (Address 5) to determine how flow control was</span>
<span class="cm">             * negotiated.</span>
<span class="cm">             */</span>
            <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_AUTONEG_ADV</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">mii_nway_adv_reg</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
                <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Read Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
                <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
            <span class="p">}</span>
            <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_LP_ABILITY</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">mii_nway_lp_ability_reg</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
                <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Read Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
                <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
            <span class="p">}</span>

            <span class="cm">/* Two bits in the Auto Negotiation Advertisement Register</span>
<span class="cm">             * (Address 4) and two bits in the Auto Negotiation Base</span>
<span class="cm">             * Page Ability Register (Address 5) determine flow control</span>
<span class="cm">             * for both the PHY and the link partner.  The following</span>
<span class="cm">             * table, taken out of the IEEE 802.3ab/D6.0 dated March 25,</span>
<span class="cm">             * 1999, describes these PAUSE resolution bits and how flow</span>
<span class="cm">             * control is determined based upon these settings.</span>
<span class="cm">             * NOTE:  DC = Don&#39;t Care</span>
<span class="cm">             *</span>
<span class="cm">             *   LOCAL DEVICE  |   LINK PARTNER</span>
<span class="cm">             * PAUSE | ASM_DIR | PAUSE | ASM_DIR | NIC Resolution</span>
<span class="cm">             *-------|---------|-------|---------|--------------------</span>
<span class="cm">             *   0   |    0    |  DC   |   DC    | e1000_fc_none</span>
<span class="cm">             *   0   |    1    |   0   |   DC    | e1000_fc_none</span>
<span class="cm">             *   0   |    1    |   1   |    0    | e1000_fc_none</span>
<span class="cm">             *   0   |    1    |   1   |    1    | e1000_fc_tx_pause</span>
<span class="cm">             *   1   |    0    |   0   |   DC    | e1000_fc_none</span>
<span class="cm">             *   1   |   DC    |   1   |   DC    | e1000_fc_full</span>
<span class="cm">             *   1   |    1    |   0   |    0    | e1000_fc_none</span>
<span class="cm">             *   1   |    1    |   0   |    1    | e1000_fc_rx_pause</span>
<span class="cm">             *</span>
<span class="cm">             */</span>
            <span class="cm">/* Are both PAUSE bits set to 1?  If so, this implies</span>
<span class="cm">             * Symmetric Flow Control is enabled at both ends.  The</span>
<span class="cm">             * ASM_DIR bits are irrelevant per the spec.</span>
<span class="cm">             *</span>
<span class="cm">             * For Symmetric Flow Control:</span>
<span class="cm">             *</span>
<span class="cm">             *   LOCAL DEVICE  |   LINK PARTNER</span>
<span class="cm">             * PAUSE | ASM_DIR | PAUSE | ASM_DIR | Result</span>
<span class="cm">             *-------|---------|-------|---------|--------------------</span>
<span class="cm">             *   1   |   DC    |   1   |   DC    | e1000_fc_full</span>
<span class="cm">             *</span>
<span class="cm">             */</span>
            <span class="k">if</span><span class="p">((</span><span class="n">mii_nway_adv_reg</span> <span class="o">&amp;</span> <span class="n">NWAY_AR_PAUSE</span><span class="p">)</span> <span class="o">&amp;&amp;</span>
               <span class="p">(</span><span class="n">mii_nway_lp_ability_reg</span> <span class="o">&amp;</span> <span class="n">NWAY_LPAR_PAUSE</span><span class="p">))</span> <span class="p">{</span>
                <span class="cm">/* Now we need to check if the user selected RX ONLY</span>
<span class="cm">                 * of pause frames.  In this case, we had to advertise</span>
<span class="cm">                 * FULL flow control because we could not advertise RX</span>
<span class="cm">                 * ONLY. Hence, we must now check to see if we need to</span>
<span class="cm">                 * turn OFF  the TRANSMISSION of PAUSE frames.</span>
<span class="cm">                 */</span>
                <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">original_fc</span> <span class="o">==</span> <span class="n">e1000_fc_full</span><span class="p">)</span> <span class="p">{</span>
                    <span class="n">hw</span><span class="o">-&gt;</span><span class="n">fc</span> <span class="o">=</span> <span class="n">e1000_fc_full</span><span class="p">;</span>
                    <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Flow Control = FULL.</span><span class="se">\r\n</span><span class="s">&quot;</span><span class="p">);</span>
                <span class="p">}</span> <span class="k">else</span> <span class="p">{</span>
                    <span class="n">hw</span><span class="o">-&gt;</span><span class="n">fc</span> <span class="o">=</span> <span class="n">e1000_fc_rx_pause</span><span class="p">;</span>
                    <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Flow Control = RX PAUSE frames only.</span><span class="se">\r\n</span><span class="s">&quot;</span><span class="p">);</span>
                <span class="p">}</span>
            <span class="p">}</span>
            <span class="cm">/* For receiving PAUSE frames ONLY.</span>
<span class="cm">             *</span>
<span class="cm">             *   LOCAL DEVICE  |   LINK PARTNER</span>
<span class="cm">             * PAUSE | ASM_DIR | PAUSE | ASM_DIR | Result</span>
<span class="cm">             *-------|---------|-------|---------|--------------------</span>
<span class="cm">             *   0   |    1    |   1   |    1    | e1000_fc_tx_pause</span>
<span class="cm">             *</span>
<span class="cm">             */</span>
            <span class="k">else</span> <span class="k">if</span><span class="p">(</span><span class="o">!</span><span class="p">(</span><span class="n">mii_nway_adv_reg</span> <span class="o">&amp;</span> <span class="n">NWAY_AR_PAUSE</span><span class="p">)</span> <span class="o">&amp;&amp;</span>
                    <span class="p">(</span><span class="n">mii_nway_adv_reg</span> <span class="o">&amp;</span> <span class="n">NWAY_AR_ASM_DIR</span><span class="p">)</span> <span class="o">&amp;&amp;</span>
                    <span class="p">(</span><span class="n">mii_nway_lp_ability_reg</span> <span class="o">&amp;</span> <span class="n">NWAY_LPAR_PAUSE</span><span class="p">)</span> <span class="o">&amp;&amp;</span>
                    <span class="p">(</span><span class="n">mii_nway_lp_ability_reg</span> <span class="o">&amp;</span> <span class="n">NWAY_LPAR_ASM_DIR</span><span class="p">))</span> <span class="p">{</span>
                <span class="n">hw</span><span class="o">-&gt;</span><span class="n">fc</span> <span class="o">=</span> <span class="n">e1000_fc_tx_pause</span><span class="p">;</span>
                <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Flow Control = TX PAUSE frames only.</span><span class="se">\r\n</span><span class="s">&quot;</span><span class="p">);</span>
            <span class="p">}</span>
            <span class="cm">/* For transmitting PAUSE frames ONLY.</span>
<span class="cm">             *</span>
<span class="cm">             *   LOCAL DEVICE  |   LINK PARTNER</span>
<span class="cm">             * PAUSE | ASM_DIR | PAUSE | ASM_DIR | Result</span>
<span class="cm">             *-------|---------|-------|---------|--------------------</span>
<span class="cm">             *   1   |    1    |   0   |    1    | e1000_fc_rx_pause</span>
<span class="cm">             *</span>
<span class="cm">             */</span>
            <span class="k">else</span> <span class="k">if</span><span class="p">((</span><span class="n">mii_nway_adv_reg</span> <span class="o">&amp;</span> <span class="n">NWAY_AR_PAUSE</span><span class="p">)</span> <span class="o">&amp;&amp;</span>
                    <span class="p">(</span><span class="n">mii_nway_adv_reg</span> <span class="o">&amp;</span> <span class="n">NWAY_AR_ASM_DIR</span><span class="p">)</span> <span class="o">&amp;&amp;</span>
                    <span class="o">!</span><span class="p">(</span><span class="n">mii_nway_lp_ability_reg</span> <span class="o">&amp;</span> <span class="n">NWAY_LPAR_PAUSE</span><span class="p">)</span> <span class="o">&amp;&amp;</span>
                    <span class="p">(</span><span class="n">mii_nway_lp_ability_reg</span> <span class="o">&amp;</span> <span class="n">NWAY_LPAR_ASM_DIR</span><span class="p">))</span> <span class="p">{</span>
                <span class="n">hw</span><span class="o">-&gt;</span><span class="n">fc</span> <span class="o">=</span> <span class="n">e1000_fc_rx_pause</span><span class="p">;</span>
                <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Flow Control = RX PAUSE frames only.</span><span class="se">\r\n</span><span class="s">&quot;</span><span class="p">);</span>
            <span class="p">}</span>
            <span class="cm">/* Per the IEEE spec, at this point flow control should be</span>
<span class="cm">             * disabled.  However, we want to consider that we could</span>
<span class="cm">             * be connected to a legacy switch that doesn&#39;t advertise</span>
<span class="cm">             * desired flow control, but can be forced on the link</span>
<span class="cm">             * partner.  So if we advertised no flow control, that is</span>
<span class="cm">             * what we will resolve to.  If we advertised some kind of</span>
<span class="cm">             * receive capability (Rx Pause Only or Full Flow Control)</span>
<span class="cm">             * and the link partner advertised none, we will configure</span>
<span class="cm">             * ourselves to enable Rx Flow Control only.  We can do</span>
<span class="cm">             * this safely for two reasons:  If the link partner really</span>
<span class="cm">             * didn&#39;t want flow control enabled, and we enable Rx, no</span>
<span class="cm">             * harm done since we won&#39;t be receiving any PAUSE frames</span>
<span class="cm">             * anyway.  If the intent on the link partner was to have</span>
<span class="cm">             * flow control enabled, then by us enabling RX only, we</span>
<span class="cm">             * can at least receive pause frames and process them.</span>
<span class="cm">             * This is a good idea because in most cases, since we are</span>
<span class="cm">             * predominantly a server NIC, more times than not we will</span>
<span class="cm">             * be asked to delay transmission of packets than asking</span>
<span class="cm">             * our link partner to pause transmission of frames.</span>
<span class="cm">             */</span>
            <span class="k">else</span> <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">original_fc</span> <span class="o">==</span> <span class="n">e1000_fc_none</span> <span class="o">||</span>
                    <span class="n">hw</span><span class="o">-&gt;</span><span class="n">original_fc</span> <span class="o">==</span> <span class="n">e1000_fc_tx_pause</span><span class="p">)</span> <span class="p">{</span>
                <span class="n">hw</span><span class="o">-&gt;</span><span class="n">fc</span> <span class="o">=</span> <span class="n">e1000_fc_none</span><span class="p">;</span>
                <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Flow Control = NONE.</span><span class="se">\r\n</span><span class="s">&quot;</span><span class="p">);</span>
            <span class="p">}</span> <span class="k">else</span> <span class="p">{</span>
                <span class="n">hw</span><span class="o">-&gt;</span><span class="n">fc</span> <span class="o">=</span> <span class="n">e1000_fc_rx_pause</span><span class="p">;</span>
                <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Flow Control = RX PAUSE frames only.</span><span class="se">\r\n</span><span class="s">&quot;</span><span class="p">);</span>
            <span class="p">}</span>

            <span class="cm">/* Now we need to do one last check...  If we auto-</span>
<span class="cm">             * negotiated to HALF DUPLEX, flow control should not be</span>
<span class="cm">             * enabled per IEEE 802.3 spec.</span>
<span class="cm">             */</span>
            <span class="n">e1000_get_speed_and_duplex</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">speed</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">duplex</span><span class="p">);</span>

            <span class="k">if</span><span class="p">(</span><span class="n">duplex</span> <span class="o">==</span> <span class="n">HALF_DUPLEX</span><span class="p">)</span>
                <span class="n">hw</span><span class="o">-&gt;</span><span class="n">fc</span> <span class="o">=</span> <span class="n">e1000_fc_none</span><span class="p">;</span>

            <span class="cm">/* Now we call a subroutine to actually force the MAC</span>
<span class="cm">             * controller to use the correct flow control settings.</span>
<span class="cm">             */</span>
            <span class="n">ret_val</span> <span class="o">=</span> <span class="n">e1000_force_mac_fc</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
            <span class="k">if</span><span class="p">(</span><span class="n">ret_val</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
                <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Error forcing flow control settings</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
                <span class="k">return</span> <span class="n">ret_val</span><span class="p">;</span>
             <span class="p">}</span>
        <span class="p">}</span> <span class="k">else</span> <span class="p">{</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Copper PHY and Auto Neg has not completed.</span><span class="se">\r\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="p">}</span>
    <span class="p">}</span>
    <span class="k">return</span> <span class="mi">0</span><span class="p">;</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm"> * Checks to see if the link status of the hardware has changed.</span>
<span class="cm"> *</span>
<span class="cm"> * hw - Struct containing variables accessed by shared code</span>
<span class="cm"> *</span>
<span class="cm"> * Called by any function that needs to check the link status of the adapter.</span>
<span class="cm"> *****************************************************************************/</span>
<span class="kt">int32_t</span>
<span class="n">e1000_check_for_link</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">uint32_t</span> <span class="n">rxcw</span><span class="p">;</span>
    <span class="kt">uint32_t</span> <span class="n">ctrl</span><span class="p">;</span>
    <span class="kt">uint32_t</span> <span class="n">status</span><span class="p">;</span>
    <span class="kt">uint32_t</span> <span class="n">rctl</span><span class="p">;</span>
    <span class="kt">uint32_t</span> <span class="n">signal</span><span class="p">;</span>
    <span class="kt">int32_t</span> <span class="n">ret_val</span><span class="p">;</span>
    <span class="kt">uint16_t</span> <span class="n">phy_data</span><span class="p">;</span>
    <span class="kt">uint16_t</span> <span class="n">lp_capability</span><span class="p">;</span>

    <span class="n">DEBUGFUNC</span><span class="p">(</span><span class="s">&quot;e1000_check_for_link&quot;</span><span class="p">);</span>
    
    <span class="cm">/* On adapters with a MAC newer that 82544, SW Defineable pin 1 will be </span>
<span class="cm">     * set when the optics detect a signal. On older adapters, it will be </span>
<span class="cm">     * cleared when there is a signal</span>
<span class="cm">     */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">&gt;</span> <span class="n">e1000_82544</span><span class="p">)</span> <span class="n">signal</span> <span class="o">=</span> <span class="n">E1000_CTRL_SWDPIN1</span><span class="p">;</span>
    <span class="k">else</span> <span class="n">signal</span> <span class="o">=</span> <span class="mi">0</span><span class="p">;</span>

    <span class="n">ctrl</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL</span><span class="p">);</span>
    <span class="n">status</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">STATUS</span><span class="p">);</span>
    <span class="n">rxcw</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">RXCW</span><span class="p">);</span>

    <span class="cm">/* If we have a copper PHY then we only want to go out to the PHY</span>
<span class="cm">     * registers to see if Auto-Neg has completed and/or if our link</span>
<span class="cm">     * status has changed.  The get_link_status flag will be set if we</span>
<span class="cm">     * receive a Link Status Change interrupt or we have Rx Sequence</span>
<span class="cm">     * Errors.</span>
<span class="cm">     */</span>
    <span class="k">if</span><span class="p">((</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">media_type</span> <span class="o">==</span> <span class="n">e1000_media_type_copper</span><span class="p">)</span> <span class="o">&amp;&amp;</span> <span class="n">hw</span><span class="o">-&gt;</span><span class="n">get_link_status</span><span class="p">)</span> <span class="p">{</span>
        <span class="cm">/* First we want to see if the MII Status Register reports</span>
<span class="cm">         * link.  If so, then we want to get the current speed/duplex</span>
<span class="cm">         * of the PHY.</span>
<span class="cm">         * Read the register twice since the link bit is sticky.</span>
<span class="cm">         */</span>
        <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_STATUS</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">phy_data</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Read Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
            <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
        <span class="p">}</span>
        <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_STATUS</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">phy_data</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Read Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
            <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
        <span class="p">}</span>

        <span class="k">if</span><span class="p">(</span><span class="n">phy_data</span> <span class="o">&amp;</span> <span class="n">MII_SR_LINK_STATUS</span><span class="p">)</span> <span class="p">{</span>
            <span class="n">hw</span><span class="o">-&gt;</span><span class="n">get_link_status</span> <span class="o">=</span> <span class="n">FALSE</span><span class="p">;</span>
        <span class="p">}</span> <span class="k">else</span> <span class="p">{</span>
            <span class="cm">/* No link detected */</span>
            <span class="k">return</span> <span class="mi">0</span><span class="p">;</span>
        <span class="p">}</span>

        <span class="cm">/* If we are forcing speed/duplex, then we simply return since</span>
<span class="cm">         * we have already determined whether we have link or not.</span>
<span class="cm">         */</span>
        <span class="k">if</span><span class="p">(</span><span class="o">!</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">autoneg</span><span class="p">)</span> <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_CONFIG</span><span class="p">;</span>

        <span class="cm">/* We have a M88E1000 PHY and Auto-Neg is enabled.  If we</span>
<span class="cm">         * have Si on board that is 82544 or newer, Auto</span>
<span class="cm">         * Speed Detection takes care of MAC speed/duplex</span>
<span class="cm">         * configuration.  So we only need to configure Collision</span>
<span class="cm">         * Distance in the MAC.  Otherwise, we need to force</span>
<span class="cm">         * speed/duplex on the MAC to the current PHY speed/duplex</span>
<span class="cm">         * settings.</span>
<span class="cm">         */</span>
        <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">&gt;=</span> <span class="n">e1000_82544</span><span class="p">)</span>
            <span class="n">e1000_config_collision_dist</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
        <span class="k">else</span> <span class="p">{</span>
            <span class="n">ret_val</span> <span class="o">=</span> <span class="n">e1000_config_mac_to_phy</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
            <span class="k">if</span><span class="p">(</span><span class="n">ret_val</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
                <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Error configuring MAC to PHY settings</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
                <span class="k">return</span> <span class="n">ret_val</span><span class="p">;</span>
            <span class="p">}</span>
        <span class="p">}</span>

        <span class="cm">/* Configure Flow Control now that Auto-Neg has completed. First, we </span>
<span class="cm">         * need to restore the desired flow control settings because we may</span>
<span class="cm">         * have had to re-autoneg with a different link partner.</span>
<span class="cm">         */</span>
        <span class="n">ret_val</span> <span class="o">=</span> <span class="n">e1000_config_fc_after_link_up</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
        <span class="k">if</span><span class="p">(</span><span class="n">ret_val</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Error configuring flow control</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
            <span class="k">return</span> <span class="n">ret_val</span><span class="p">;</span>
        <span class="p">}</span>

        <span class="cm">/* At this point we know that we are on copper and we have</span>
<span class="cm">         * auto-negotiated link.  These are conditions for checking the link</span>
<span class="cm">         * parter capability register.  We use the link partner capability to</span>
<span class="cm">         * determine if TBI Compatibility needs to be turned on or off.  If</span>
<span class="cm">         * the link partner advertises any speed in addition to Gigabit, then</span>
<span class="cm">         * we assume that they are GMII-based, and TBI compatibility is not</span>
<span class="cm">         * needed. If no other speeds are advertised, we assume the link</span>
<span class="cm">         * partner is TBI-based, and we turn on TBI Compatibility.</span>
<span class="cm">         */</span>
        <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">tbi_compatibility_en</span><span class="p">)</span> <span class="p">{</span>
            <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_LP_ABILITY</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">lp_capability</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
                <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Read Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
                <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
            <span class="p">}</span>
            <span class="k">if</span><span class="p">(</span><span class="n">lp_capability</span> <span class="o">&amp;</span> <span class="p">(</span><span class="n">NWAY_LPAR_10T_HD_CAPS</span> <span class="o">|</span>
                                <span class="n">NWAY_LPAR_10T_FD_CAPS</span> <span class="o">|</span>
                                <span class="n">NWAY_LPAR_100TX_HD_CAPS</span> <span class="o">|</span>
                                <span class="n">NWAY_LPAR_100TX_FD_CAPS</span> <span class="o">|</span>
                                <span class="n">NWAY_LPAR_100T4_CAPS</span><span class="p">))</span> <span class="p">{</span>
                <span class="cm">/* If our link partner advertises anything in addition to </span>
<span class="cm">                 * gigabit, we do not need to enable TBI compatibility.</span>
<span class="cm">                 */</span>
                <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">tbi_compatibility_on</span><span class="p">)</span> <span class="p">{</span>
                    <span class="cm">/* If we previously were in the mode, turn it off. */</span>
                    <span class="n">rctl</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">RCTL</span><span class="p">);</span>
                    <span class="n">rctl</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="n">E1000_RCTL_SBP</span><span class="p">;</span>
                    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">RCTL</span><span class="p">,</span> <span class="n">rctl</span><span class="p">);</span>
                    <span class="n">hw</span><span class="o">-&gt;</span><span class="n">tbi_compatibility_on</span> <span class="o">=</span> <span class="n">FALSE</span><span class="p">;</span>
                <span class="p">}</span>
            <span class="p">}</span> <span class="k">else</span> <span class="p">{</span>
                <span class="cm">/* If TBI compatibility is was previously off, turn it on. For</span>
<span class="cm">                 * compatibility with a TBI link partner, we will store bad</span>
<span class="cm">                 * packets. Some frames have an additional byte on the end and</span>
<span class="cm">                 * will look like CRC errors to to the hardware.</span>
<span class="cm">                 */</span>
                <span class="k">if</span><span class="p">(</span><span class="o">!</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">tbi_compatibility_on</span><span class="p">)</span> <span class="p">{</span>
                    <span class="n">hw</span><span class="o">-&gt;</span><span class="n">tbi_compatibility_on</span> <span class="o">=</span> <span class="n">TRUE</span><span class="p">;</span>
                    <span class="n">rctl</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">RCTL</span><span class="p">);</span>
                    <span class="n">rctl</span> <span class="o">|=</span> <span class="n">E1000_RCTL_SBP</span><span class="p">;</span>
                    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">RCTL</span><span class="p">,</span> <span class="n">rctl</span><span class="p">);</span>
                <span class="p">}</span>
            <span class="p">}</span>
        <span class="p">}</span>
    <span class="p">}</span>
    <span class="cm">/* If we don&#39;t have link (auto-negotiation failed or link partner cannot</span>
<span class="cm">     * auto-negotiate), the cable is plugged in (we have signal), and our</span>
<span class="cm">     * link partner is not trying to auto-negotiate with us (we are receiving</span>
<span class="cm">     * idles or data), we need to force link up. We also need to give</span>
<span class="cm">     * auto-negotiation time to complete, in case the cable was just plugged</span>
<span class="cm">     * in. The autoneg_failed flag does this.</span>
<span class="cm">     */</span>
    <span class="k">else</span> <span class="k">if</span><span class="p">((</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">media_type</span> <span class="o">==</span> <span class="n">e1000_media_type_fiber</span><span class="p">)</span> <span class="o">&amp;&amp;</span>
            <span class="p">(</span><span class="o">!</span><span class="p">(</span><span class="n">status</span> <span class="o">&amp;</span> <span class="n">E1000_STATUS_LU</span><span class="p">))</span> <span class="o">&amp;&amp;</span>
            <span class="p">((</span><span class="n">ctrl</span> <span class="o">&amp;</span> <span class="n">E1000_CTRL_SWDPIN1</span><span class="p">)</span> <span class="o">==</span> <span class="n">signal</span><span class="p">)</span> <span class="o">&amp;&amp;</span>
            <span class="p">(</span><span class="o">!</span><span class="p">(</span><span class="n">rxcw</span> <span class="o">&amp;</span> <span class="n">E1000_RXCW_C</span><span class="p">)))</span> <span class="p">{</span>
        <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">autoneg_failed</span> <span class="o">==</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
            <span class="n">hw</span><span class="o">-&gt;</span><span class="n">autoneg_failed</span> <span class="o">=</span> <span class="mi">1</span><span class="p">;</span>
            <span class="k">return</span> <span class="mi">0</span><span class="p">;</span>
        <span class="p">}</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;NOT RXing /C/, disable AutoNeg and force link.</span><span class="se">\r\n</span><span class="s">&quot;</span><span class="p">);</span>

        <span class="cm">/* Disable auto-negotiation in the TXCW register */</span>
        <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">TXCW</span><span class="p">,</span> <span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">txcw</span> <span class="o">&amp;</span> <span class="o">~</span><span class="n">E1000_TXCW_ANE</span><span class="p">));</span>

        <span class="cm">/* Force link-up and also force full-duplex. */</span>
        <span class="n">ctrl</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL</span><span class="p">);</span>
        <span class="n">ctrl</span> <span class="o">|=</span> <span class="p">(</span><span class="n">E1000_CTRL_SLU</span> <span class="o">|</span> <span class="n">E1000_CTRL_FD</span><span class="p">);</span>
        <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL</span><span class="p">,</span> <span class="n">ctrl</span><span class="p">);</span>

        <span class="cm">/* Configure Flow Control after forcing link up. */</span>
        <span class="n">ret_val</span> <span class="o">=</span> <span class="n">e1000_config_fc_after_link_up</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
        <span class="k">if</span><span class="p">(</span><span class="n">ret_val</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Error configuring flow control</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
            <span class="k">return</span> <span class="n">ret_val</span><span class="p">;</span>
        <span class="p">}</span>
    <span class="p">}</span>
    <span class="cm">/* If we are forcing link and we are receiving /C/ ordered sets, re-enable</span>
<span class="cm">     * auto-negotiation in the TXCW register and disable forced link in the</span>
<span class="cm">     * Device Control register in an attempt to auto-negotiate with our link</span>
<span class="cm">     * partner.</span>
<span class="cm">     */</span>
    <span class="k">else</span> <span class="k">if</span><span class="p">((</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">media_type</span> <span class="o">==</span> <span class="n">e1000_media_type_fiber</span><span class="p">)</span> <span class="o">&amp;&amp;</span>
              <span class="p">(</span><span class="n">ctrl</span> <span class="o">&amp;</span> <span class="n">E1000_CTRL_SLU</span><span class="p">)</span> <span class="o">&amp;&amp;</span>
              <span class="p">(</span><span class="n">rxcw</span> <span class="o">&amp;</span> <span class="n">E1000_RXCW_C</span><span class="p">))</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;RXing /C/, enable AutoNeg and stop forcing link.</span><span class="se">\r\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">TXCW</span><span class="p">,</span> <span class="n">hw</span><span class="o">-&gt;</span><span class="n">txcw</span><span class="p">);</span>
        <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL</span><span class="p">,</span> <span class="p">(</span><span class="n">ctrl</span> <span class="o">&amp;</span> <span class="o">~</span><span class="n">E1000_CTRL_SLU</span><span class="p">));</span>
    <span class="p">}</span>
    <span class="k">return</span> <span class="mi">0</span><span class="p">;</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm"> * Detects the current speed and duplex settings of the hardware.</span>
<span class="cm"> *</span>
<span class="cm"> * hw - Struct containing variables accessed by shared code</span>
<span class="cm"> * speed - Speed of the connection</span>
<span class="cm"> * duplex - Duplex setting of the connection</span>
<span class="cm"> *****************************************************************************/</span>
<span class="kt">void</span>
<span class="n">e1000_get_speed_and_duplex</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">,</span>
                           <span class="kt">uint16_t</span> <span class="o">*</span><span class="n">speed</span><span class="p">,</span>
                           <span class="kt">uint16_t</span> <span class="o">*</span><span class="n">duplex</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">uint32_t</span> <span class="n">status</span><span class="p">;</span>

    <span class="n">DEBUGFUNC</span><span class="p">(</span><span class="s">&quot;e1000_get_speed_and_duplex&quot;</span><span class="p">);</span>

    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">&gt;=</span> <span class="n">e1000_82543</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">status</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">STATUS</span><span class="p">);</span>
        <span class="k">if</span><span class="p">(</span><span class="n">status</span> <span class="o">&amp;</span> <span class="n">E1000_STATUS_SPEED_1000</span><span class="p">)</span> <span class="p">{</span>
            <span class="o">*</span><span class="n">speed</span> <span class="o">=</span> <span class="n">SPEED_1000</span><span class="p">;</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;1000 Mbs, &quot;</span><span class="p">);</span>
        <span class="p">}</span> <span class="k">else</span> <span class="k">if</span><span class="p">(</span><span class="n">status</span> <span class="o">&amp;</span> <span class="n">E1000_STATUS_SPEED_100</span><span class="p">)</span> <span class="p">{</span>
            <span class="o">*</span><span class="n">speed</span> <span class="o">=</span> <span class="n">SPEED_100</span><span class="p">;</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;100 Mbs, &quot;</span><span class="p">);</span>
        <span class="p">}</span> <span class="k">else</span> <span class="p">{</span>
            <span class="o">*</span><span class="n">speed</span> <span class="o">=</span> <span class="n">SPEED_10</span><span class="p">;</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;10 Mbs, &quot;</span><span class="p">);</span>
        <span class="p">}</span>

        <span class="k">if</span><span class="p">(</span><span class="n">status</span> <span class="o">&amp;</span> <span class="n">E1000_STATUS_FD</span><span class="p">)</span> <span class="p">{</span>
            <span class="o">*</span><span class="n">duplex</span> <span class="o">=</span> <span class="n">FULL_DUPLEX</span><span class="p">;</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Full Duplex</span><span class="se">\r\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="p">}</span> <span class="k">else</span> <span class="p">{</span>
            <span class="o">*</span><span class="n">duplex</span> <span class="o">=</span> <span class="n">HALF_DUPLEX</span><span class="p">;</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot; Half Duplex</span><span class="se">\r\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="p">}</span>
    <span class="p">}</span> <span class="k">else</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;1000 Mbs, Full Duplex</span><span class="se">\r\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="o">*</span><span class="n">speed</span> <span class="o">=</span> <span class="n">SPEED_1000</span><span class="p">;</span>
        <span class="o">*</span><span class="n">duplex</span> <span class="o">=</span> <span class="n">FULL_DUPLEX</span><span class="p">;</span>
    <span class="p">}</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm">* Blocks until autoneg completes or times out (~4.5 seconds)</span>
<span class="cm">*</span>
<span class="cm">* hw - Struct containing variables accessed by shared code</span>
<span class="cm">******************************************************************************/</span>
<span class="kt">int32_t</span>
<span class="n">e1000_wait_autoneg</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">uint16_t</span> <span class="n">i</span><span class="p">;</span>
    <span class="kt">uint16_t</span> <span class="n">phy_data</span><span class="p">;</span>

    <span class="n">DEBUGFUNC</span><span class="p">(</span><span class="s">&quot;e1000_wait_autoneg&quot;</span><span class="p">);</span>
    <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Waiting for Auto-Neg to complete.</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>

    <span class="cm">/* We will wait for autoneg to complete or 4.5 seconds to expire. */</span>
    <span class="k">for</span><span class="p">(</span><span class="n">i</span> <span class="o">=</span> <span class="n">PHY_AUTO_NEG_TIME</span><span class="p">;</span> <span class="n">i</span> <span class="o">&gt;</span> <span class="mi">0</span><span class="p">;</span> <span class="n">i</span><span class="o">--</span><span class="p">)</span> <span class="p">{</span>
        <span class="cm">/* Read the MII Status Register and wait for Auto-Neg</span>
<span class="cm">         * Complete bit to be set.</span>
<span class="cm">         */</span>
        <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_STATUS</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">phy_data</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Read Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
            <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
        <span class="p">}</span>
        <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_STATUS</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">phy_data</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Read Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
            <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
        <span class="p">}</span>
        <span class="k">if</span><span class="p">(</span><span class="n">phy_data</span> <span class="o">&amp;</span> <span class="n">MII_SR_AUTONEG_COMPLETE</span><span class="p">)</span> <span class="p">{</span>
            <span class="k">return</span> <span class="mi">0</span><span class="p">;</span>
        <span class="p">}</span>
        <span class="n">msec_delay</span><span class="p">(</span><span class="mi">100</span><span class="p">);</span>
    <span class="p">}</span>
    <span class="k">return</span> <span class="mi">0</span><span class="p">;</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm">* Raises the Management Data Clock</span>
<span class="cm">*</span>
<span class="cm">* hw - Struct containing variables accessed by shared code</span>
<span class="cm">* ctrl - Device control register&#39;s current value</span>
<span class="cm">******************************************************************************/</span>
<span class="k">static</span> <span class="kt">void</span>
<span class="n">e1000_raise_mdi_clk</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">,</span>
                    <span class="kt">uint32_t</span> <span class="o">*</span><span class="n">ctrl</span><span class="p">)</span>
<span class="p">{</span>
    <span class="cm">/* Raise the clock input to the Management Data Clock (by setting the MDC</span>
<span class="cm">     * bit), and then delay 2 microseconds.</span>
<span class="cm">     */</span>
    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL</span><span class="p">,</span> <span class="p">(</span><span class="o">*</span><span class="n">ctrl</span> <span class="o">|</span> <span class="n">E1000_CTRL_MDC</span><span class="p">));</span>
    <span class="n">E1000_WRITE_FLUSH</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
    <span class="n">udelay</span><span class="p">(</span><span class="mi">2</span><span class="p">);</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm">* Lowers the Management Data Clock</span>
<span class="cm">*</span>
<span class="cm">* hw - Struct containing variables accessed by shared code</span>
<span class="cm">* ctrl - Device control register&#39;s current value</span>
<span class="cm">******************************************************************************/</span>
<span class="k">static</span> <span class="kt">void</span>
<span class="n">e1000_lower_mdi_clk</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">,</span>
                    <span class="kt">uint32_t</span> <span class="o">*</span><span class="n">ctrl</span><span class="p">)</span>
<span class="p">{</span>
    <span class="cm">/* Lower the clock input to the Management Data Clock (by clearing the MDC</span>
<span class="cm">     * bit), and then delay 2 microseconds.</span>
<span class="cm">     */</span>
    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL</span><span class="p">,</span> <span class="p">(</span><span class="o">*</span><span class="n">ctrl</span> <span class="o">&amp;</span> <span class="o">~</span><span class="n">E1000_CTRL_MDC</span><span class="p">));</span>
    <span class="n">E1000_WRITE_FLUSH</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
    <span class="n">udelay</span><span class="p">(</span><span class="mi">2</span><span class="p">);</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm">* Shifts data bits out to the PHY</span>
<span class="cm">*</span>
<span class="cm">* hw - Struct containing variables accessed by shared code</span>
<span class="cm">* data - Data to send out to the PHY</span>
<span class="cm">* count - Number of bits to shift out</span>
<span class="cm">*</span>
<span class="cm">* Bits are shifted out in MSB to LSB order.</span>
<span class="cm">******************************************************************************/</span>
<span class="k">static</span> <span class="kt">void</span>
<span class="n">e1000_shift_out_mdi_bits</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">,</span>
                         <span class="kt">uint32_t</span> <span class="n">data</span><span class="p">,</span>
                         <span class="kt">uint16_t</span> <span class="n">count</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">uint32_t</span> <span class="n">ctrl</span><span class="p">;</span>
    <span class="kt">uint32_t</span> <span class="n">mask</span><span class="p">;</span>

    <span class="cm">/* We need to shift &quot;count&quot; number of bits out to the PHY. So, the value</span>
<span class="cm">     * in the &quot;data&quot; parameter will be shifted out to the PHY one bit at a </span>
<span class="cm">     * time. In order to do this, &quot;data&quot; must be broken down into bits.</span>
<span class="cm">     */</span>
    <span class="n">mask</span> <span class="o">=</span> <span class="mh">0x01</span><span class="p">;</span>
    <span class="n">mask</span> <span class="o">&lt;&lt;=</span> <span class="p">(</span><span class="n">count</span> <span class="o">-</span> <span class="mi">1</span><span class="p">);</span>

    <span class="n">ctrl</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL</span><span class="p">);</span>

    <span class="cm">/* Set MDIO_DIR and MDC_DIR direction bits to be used as output pins. */</span>
    <span class="n">ctrl</span> <span class="o">|=</span> <span class="p">(</span><span class="n">E1000_CTRL_MDIO_DIR</span> <span class="o">|</span> <span class="n">E1000_CTRL_MDC_DIR</span><span class="p">);</span>

    <span class="k">while</span><span class="p">(</span><span class="n">mask</span><span class="p">)</span> <span class="p">{</span>
        <span class="cm">/* A &quot;1&quot; is shifted out to the PHY by setting the MDIO bit to &quot;1&quot; and</span>
<span class="cm">         * then raising and lowering the Management Data Clock. A &quot;0&quot; is</span>
<span class="cm">         * shifted out to the PHY by setting the MDIO bit to &quot;0&quot; and then</span>
<span class="cm">         * raising and lowering the clock.</span>
<span class="cm">         */</span>
        <span class="k">if</span><span class="p">(</span><span class="n">data</span> <span class="o">&amp;</span> <span class="n">mask</span><span class="p">)</span> <span class="n">ctrl</span> <span class="o">|=</span> <span class="n">E1000_CTRL_MDIO</span><span class="p">;</span>
        <span class="k">else</span> <span class="n">ctrl</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="n">E1000_CTRL_MDIO</span><span class="p">;</span>

        <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL</span><span class="p">,</span> <span class="n">ctrl</span><span class="p">);</span>
        <span class="n">E1000_WRITE_FLUSH</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>

        <span class="n">udelay</span><span class="p">(</span><span class="mi">2</span><span class="p">);</span>

        <span class="n">e1000_raise_mdi_clk</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">ctrl</span><span class="p">);</span>
        <span class="n">e1000_lower_mdi_clk</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">ctrl</span><span class="p">);</span>

        <span class="n">mask</span> <span class="o">=</span> <span class="n">mask</span> <span class="o">&gt;&gt;</span> <span class="mi">1</span><span class="p">;</span>
    <span class="p">}</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm">* Shifts data bits in from the PHY</span>
<span class="cm">*</span>
<span class="cm">* hw - Struct containing variables accessed by shared code</span>
<span class="cm">*</span>
<span class="cm">* Bits are shifted in in MSB to LSB order. </span>
<span class="cm">******************************************************************************/</span>
<span class="k">static</span> <span class="kt">uint16_t</span>
<span class="n">e1000_shift_in_mdi_bits</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">uint32_t</span> <span class="n">ctrl</span><span class="p">;</span>
    <span class="kt">uint16_t</span> <span class="n">data</span> <span class="o">=</span> <span class="mi">0</span><span class="p">;</span>
    <span class="kt">uint8_t</span> <span class="n">i</span><span class="p">;</span>

    <span class="cm">/* In order to read a register from the PHY, we need to shift in a total</span>
<span class="cm">     * of 18 bits from the PHY. The first two bit (turnaround) times are used</span>
<span class="cm">     * to avoid contention on the MDIO pin when a read operation is performed.</span>
<span class="cm">     * These two bits are ignored by us and thrown away. Bits are &quot;shifted in&quot;</span>
<span class="cm">     * by raising the input to the Management Data Clock (setting the MDC bit),</span>
<span class="cm">     * and then reading the value of the MDIO bit.</span>
<span class="cm">     */</span> 
    <span class="n">ctrl</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL</span><span class="p">);</span>

    <span class="cm">/* Clear MDIO_DIR (SWDPIO1) to indicate this bit is to be used as input. */</span>
    <span class="n">ctrl</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="n">E1000_CTRL_MDIO_DIR</span><span class="p">;</span>
    <span class="n">ctrl</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="n">E1000_CTRL_MDIO</span><span class="p">;</span>

    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL</span><span class="p">,</span> <span class="n">ctrl</span><span class="p">);</span>
    <span class="n">E1000_WRITE_FLUSH</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>

    <span class="cm">/* Raise and Lower the clock before reading in the data. This accounts for</span>
<span class="cm">     * the turnaround bits. The first clock occurred when we clocked out the</span>
<span class="cm">     * last bit of the Register Address.</span>
<span class="cm">     */</span>
    <span class="n">e1000_raise_mdi_clk</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">ctrl</span><span class="p">);</span>
    <span class="n">e1000_lower_mdi_clk</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">ctrl</span><span class="p">);</span>

    <span class="k">for</span><span class="p">(</span><span class="n">data</span> <span class="o">=</span> <span class="mi">0</span><span class="p">,</span> <span class="n">i</span> <span class="o">=</span> <span class="mi">0</span><span class="p">;</span> <span class="n">i</span> <span class="o">&lt;</span> <span class="mi">16</span><span class="p">;</span> <span class="n">i</span><span class="o">++</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">data</span> <span class="o">=</span> <span class="n">data</span> <span class="o">&lt;&lt;</span> <span class="mi">1</span><span class="p">;</span>
        <span class="n">e1000_raise_mdi_clk</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">ctrl</span><span class="p">);</span>
        <span class="n">ctrl</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL</span><span class="p">);</span>
        <span class="cm">/* Check to see if we shifted in a &quot;1&quot;. */</span>
        <span class="k">if</span><span class="p">(</span><span class="n">ctrl</span> <span class="o">&amp;</span> <span class="n">E1000_CTRL_MDIO</span><span class="p">)</span> <span class="n">data</span> <span class="o">|=</span> <span class="mi">1</span><span class="p">;</span>
        <span class="n">e1000_lower_mdi_clk</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">ctrl</span><span class="p">);</span>
    <span class="p">}</span>

    <span class="n">e1000_raise_mdi_clk</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">ctrl</span><span class="p">);</span>
    <span class="n">e1000_lower_mdi_clk</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">ctrl</span><span class="p">);</span>

    <span class="k">return</span> <span class="n">data</span><span class="p">;</span>
<span class="p">}</span>

<span class="cm">/*****************************************************************************</span>
<span class="cm">* Reads the value from a PHY register</span>
<span class="cm">*</span>
<span class="cm">* hw - Struct containing variables accessed by shared code</span>
<span class="cm">* reg_addr - address of the PHY register to read</span>
<span class="cm">******************************************************************************/</span>
<span class="kt">int32_t</span>
<span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">,</span>
                   <span class="kt">uint32_t</span> <span class="n">reg_addr</span><span class="p">,</span>
                   <span class="kt">uint16_t</span> <span class="o">*</span><span class="n">phy_data</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">uint32_t</span> <span class="n">i</span><span class="p">;</span>
    <span class="kt">uint32_t</span> <span class="n">mdic</span> <span class="o">=</span> <span class="mi">0</span><span class="p">;</span>
    <span class="k">const</span> <span class="kt">uint32_t</span> <span class="n">phy_addr</span> <span class="o">=</span> <span class="mi">1</span><span class="p">;</span>

    <span class="n">DEBUGFUNC</span><span class="p">(</span><span class="s">&quot;XXXXe1000_read_phy_reg&quot;</span><span class="p">);</span>

    <span class="k">if</span><span class="p">(</span><span class="n">reg_addr</span> <span class="o">&gt;</span> <span class="n">MAX_PHY_REG_ADDRESS</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT1</span><span class="p">(</span><span class="s">&quot;PHY Address %d is out of range</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">,</span> <span class="n">reg_addr</span><span class="p">);</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PARAM</span><span class="p">;</span>
    <span class="p">}</span>

    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">&gt;</span> <span class="n">e1000_82543</span><span class="p">)</span> <span class="p">{</span>
        <span class="cm">/* Set up Op-code, Phy Address, and register address in the MDI</span>
<span class="cm">         * Control register.  The MAC will take care of interfacing with the</span>
<span class="cm">         * PHY to retrieve the desired data.</span>
<span class="cm">         */</span>
        <span class="n">mdic</span> <span class="o">=</span> <span class="p">((</span><span class="n">reg_addr</span> <span class="o">&lt;&lt;</span> <span class="n">E1000_MDIC_REG_SHIFT</span><span class="p">)</span> <span class="o">|</span>
                <span class="p">(</span><span class="n">phy_addr</span> <span class="o">&lt;&lt;</span> <span class="n">E1000_MDIC_PHY_SHIFT</span><span class="p">)</span> <span class="o">|</span> 
                <span class="p">(</span><span class="n">E1000_MDIC_OP_READ</span><span class="p">));</span>

        <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">MDIC</span><span class="p">,</span> <span class="n">mdic</span><span class="p">);</span>

        <span class="cm">/* Poll the ready bit to see if the MDI read completed */</span>
        <span class="k">for</span><span class="p">(</span><span class="n">i</span> <span class="o">=</span> <span class="mi">0</span><span class="p">;</span> <span class="n">i</span> <span class="o">&lt;</span> <span class="mi">64</span><span class="p">;</span> <span class="n">i</span><span class="o">++</span><span class="p">)</span> <span class="p">{</span>
            <span class="n">udelay</span><span class="p">(</span><span class="mi">10</span><span class="p">);</span>
            <span class="n">mdic</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">MDIC</span><span class="p">);</span>
            <span class="k">if</span><span class="p">(</span><span class="n">mdic</span> <span class="o">&amp;</span> <span class="n">E1000_MDIC_READY</span><span class="p">)</span> <span class="k">break</span><span class="p">;</span>
        <span class="p">}</span>
        <span class="k">if</span><span class="p">(</span><span class="o">!</span><span class="p">(</span><span class="n">mdic</span> <span class="o">&amp;</span> <span class="n">E1000_MDIC_READY</span><span class="p">))</span> <span class="p">{</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;MDI Read did not complete</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
            <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
        <span class="p">}</span>
        <span class="k">if</span><span class="p">(</span><span class="n">mdic</span> <span class="o">&amp;</span> <span class="n">E1000_MDIC_ERROR</span><span class="p">)</span> <span class="p">{</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;MDI Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
            <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
        <span class="p">}</span>
        <span class="o">*</span><span class="n">phy_data</span> <span class="o">=</span> <span class="p">(</span><span class="kt">uint16_t</span><span class="p">)</span> <span class="n">mdic</span><span class="p">;</span>
    <span class="p">}</span> <span class="k">else</span> <span class="p">{</span>
        <span class="cm">/* We must first send a preamble through the MDIO pin to signal the</span>
<span class="cm">         * beginning of an MII instruction.  This is done by sending 32</span>
<span class="cm">         * consecutive &quot;1&quot; bits.</span>
<span class="cm">         */</span>
        <span class="n">e1000_shift_out_mdi_bits</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_PREAMBLE</span><span class="p">,</span> <span class="n">PHY_PREAMBLE_SIZE</span><span class="p">);</span>

        <span class="cm">/* Now combine the next few fields that are required for a read</span>
<span class="cm">         * operation.  We use this method instead of calling the</span>
<span class="cm">         * e1000_shift_out_mdi_bits routine five different times. The format of</span>
<span class="cm">         * a MII read instruction consists of a shift out of 14 bits and is</span>
<span class="cm">         * defined as follows:</span>
<span class="cm">         *    &lt;Preamble&gt;&lt;SOF&gt;&lt;Op Code&gt;&lt;Phy Addr&gt;&lt;Reg Addr&gt;</span>
<span class="cm">         * followed by a shift in of 18 bits.  This first two bits shifted in</span>
<span class="cm">         * are TurnAround bits used to avoid contention on the MDIO pin when a</span>
<span class="cm">         * READ operation is performed.  These two bits are thrown away</span>
<span class="cm">         * followed by a shift in of 16 bits which contains the desired data.</span>
<span class="cm">         */</span>
        <span class="n">mdic</span> <span class="o">=</span> <span class="p">((</span><span class="n">reg_addr</span><span class="p">)</span> <span class="o">|</span> <span class="p">(</span><span class="n">phy_addr</span> <span class="o">&lt;&lt;</span> <span class="mi">5</span><span class="p">)</span> <span class="o">|</span> 
                <span class="p">(</span><span class="n">PHY_OP_READ</span> <span class="o">&lt;&lt;</span> <span class="mi">10</span><span class="p">)</span> <span class="o">|</span> <span class="p">(</span><span class="n">PHY_SOF</span> <span class="o">&lt;&lt;</span> <span class="mi">12</span><span class="p">));</span>

        <span class="n">e1000_shift_out_mdi_bits</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">mdic</span><span class="p">,</span> <span class="mi">14</span><span class="p">);</span>

        <span class="cm">/* Now that we&#39;ve shifted out the read command to the MII, we need to</span>
<span class="cm">         * &quot;shift in&quot; the 16-bit value (18 total bits) of the requested PHY</span>
<span class="cm">         * register address.</span>
<span class="cm">         */</span>
        <span class="o">*</span><span class="n">phy_data</span> <span class="o">=</span> <span class="n">e1000_shift_in_mdi_bits</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
    <span class="p">}</span>
    <span class="k">return</span> <span class="mi">0</span><span class="p">;</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm">* Writes a value to a PHY register</span>
<span class="cm">*</span>
<span class="cm">* hw - Struct containing variables accessed by shared code</span>
<span class="cm">* reg_addr - address of the PHY register to write</span>
<span class="cm">* data - data to write to the PHY</span>
<span class="cm">******************************************************************************/</span>
<span class="kt">int32_t</span>
<span class="n">e1000_write_phy_reg</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">,</span>
                    <span class="kt">uint32_t</span> <span class="n">reg_addr</span><span class="p">,</span>
                    <span class="kt">uint16_t</span> <span class="n">phy_data</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">uint32_t</span> <span class="n">i</span><span class="p">;</span>
    <span class="kt">uint32_t</span> <span class="n">mdic</span> <span class="o">=</span> <span class="mi">0</span><span class="p">;</span>
    <span class="k">const</span> <span class="kt">uint32_t</span> <span class="n">phy_addr</span> <span class="o">=</span> <span class="mi">1</span><span class="p">;</span>

    <span class="n">DEBUGFUNC</span><span class="p">(</span><span class="s">&quot;e1000_write_phy_reg&quot;</span><span class="p">);</span>

    <span class="k">if</span><span class="p">(</span><span class="n">reg_addr</span> <span class="o">&gt;</span> <span class="n">MAX_PHY_REG_ADDRESS</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT1</span><span class="p">(</span><span class="s">&quot;PHY Address %d is out of range</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">,</span> <span class="n">reg_addr</span><span class="p">);</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PARAM</span><span class="p">;</span>
    <span class="p">}</span>

    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">&gt;</span> <span class="n">e1000_82543</span><span class="p">)</span> <span class="p">{</span>
        <span class="cm">/* Set up Op-code, Phy Address, register address, and data intended</span>
<span class="cm">         * for the PHY register in the MDI Control register.  The MAC will take</span>
<span class="cm">         * care of interfacing with the PHY to send the desired data.</span>
<span class="cm">         */</span>
        <span class="n">mdic</span> <span class="o">=</span> <span class="p">(((</span><span class="kt">uint32_t</span><span class="p">)</span> <span class="n">phy_data</span><span class="p">)</span> <span class="o">|</span>
                <span class="p">(</span><span class="n">reg_addr</span> <span class="o">&lt;&lt;</span> <span class="n">E1000_MDIC_REG_SHIFT</span><span class="p">)</span> <span class="o">|</span>
                <span class="p">(</span><span class="n">phy_addr</span> <span class="o">&lt;&lt;</span> <span class="n">E1000_MDIC_PHY_SHIFT</span><span class="p">)</span> <span class="o">|</span> 
                <span class="p">(</span><span class="n">E1000_MDIC_OP_WRITE</span><span class="p">));</span>

        <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">MDIC</span><span class="p">,</span> <span class="n">mdic</span><span class="p">);</span>

        <span class="cm">/* Poll the ready bit to see if the MDI read completed */</span>
        <span class="k">for</span><span class="p">(</span><span class="n">i</span> <span class="o">=</span> <span class="mi">0</span><span class="p">;</span> <span class="n">i</span> <span class="o">&lt;</span> <span class="mi">64</span><span class="p">;</span> <span class="n">i</span><span class="o">++</span><span class="p">)</span> <span class="p">{</span>
            <span class="n">udelay</span><span class="p">(</span><span class="mi">10</span><span class="p">);</span>
            <span class="n">mdic</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">MDIC</span><span class="p">);</span>
            <span class="k">if</span><span class="p">(</span><span class="n">mdic</span> <span class="o">&amp;</span> <span class="n">E1000_MDIC_READY</span><span class="p">)</span> <span class="k">break</span><span class="p">;</span>
        <span class="p">}</span>
        <span class="k">if</span><span class="p">(</span><span class="o">!</span><span class="p">(</span><span class="n">mdic</span> <span class="o">&amp;</span> <span class="n">E1000_MDIC_READY</span><span class="p">))</span> <span class="p">{</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;MDI Write did not complete</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
            <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
        <span class="p">}</span>
    <span class="p">}</span> <span class="k">else</span> <span class="p">{</span>
        <span class="cm">/* We&#39;ll need to use the SW defined pins to shift the write command</span>
<span class="cm">         * out to the PHY. We first send a preamble to the PHY to signal the</span>
<span class="cm">         * beginning of the MII instruction.  This is done by sending 32 </span>
<span class="cm">         * consecutive &quot;1&quot; bits.</span>
<span class="cm">         */</span>
        <span class="n">e1000_shift_out_mdi_bits</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_PREAMBLE</span><span class="p">,</span> <span class="n">PHY_PREAMBLE_SIZE</span><span class="p">);</span>

        <span class="cm">/* Now combine the remaining required fields that will indicate a </span>
<span class="cm">         * write operation. We use this method instead of calling the</span>
<span class="cm">         * e1000_shift_out_mdi_bits routine for each field in the command. The</span>
<span class="cm">         * format of a MII write instruction is as follows:</span>
<span class="cm">         * &lt;Preamble&gt;&lt;SOF&gt;&lt;Op Code&gt;&lt;Phy Addr&gt;&lt;Reg Addr&gt;&lt;Turnaround&gt;&lt;Data&gt;.</span>
<span class="cm">         */</span>
        <span class="n">mdic</span> <span class="o">=</span> <span class="p">((</span><span class="n">PHY_TURNAROUND</span><span class="p">)</span> <span class="o">|</span> <span class="p">(</span><span class="n">reg_addr</span> <span class="o">&lt;&lt;</span> <span class="mi">2</span><span class="p">)</span> <span class="o">|</span> <span class="p">(</span><span class="n">phy_addr</span> <span class="o">&lt;&lt;</span> <span class="mi">7</span><span class="p">)</span> <span class="o">|</span>
                <span class="p">(</span><span class="n">PHY_OP_WRITE</span> <span class="o">&lt;&lt;</span> <span class="mi">12</span><span class="p">)</span> <span class="o">|</span> <span class="p">(</span><span class="n">PHY_SOF</span> <span class="o">&lt;&lt;</span> <span class="mi">14</span><span class="p">));</span>
        <span class="n">mdic</span> <span class="o">&lt;&lt;=</span> <span class="mi">16</span><span class="p">;</span>
        <span class="n">mdic</span> <span class="o">|=</span> <span class="p">(</span><span class="kt">uint32_t</span><span class="p">)</span> <span class="n">phy_data</span><span class="p">;</span>

        <span class="n">e1000_shift_out_mdi_bits</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">mdic</span><span class="p">,</span> <span class="mi">32</span><span class="p">);</span>
    <span class="p">}</span>
    <span class="k">return</span> <span class="mi">0</span><span class="p">;</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm">* Returns the PHY to the power-on reset state</span>
<span class="cm">*</span>
<span class="cm">* hw - Struct containing variables accessed by shared code</span>
<span class="cm">******************************************************************************/</span>
<span class="kt">void</span>
<span class="n">e1000_phy_hw_reset</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">uint32_t</span> <span class="n">ctrl</span><span class="p">;</span>
    <span class="kt">uint32_t</span> <span class="n">ctrl_ext</span><span class="p">;</span>

    <span class="n">DEBUGFUNC</span><span class="p">(</span><span class="s">&quot;e1000_phy_hw_reset&quot;</span><span class="p">);</span>

    <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Resetting Phy...</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>

    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">&gt;</span> <span class="n">e1000_82543</span><span class="p">)</span> <span class="p">{</span>
        <span class="cm">/* Read the device control register and assert the E1000_CTRL_PHY_RST</span>
<span class="cm">         * bit. Then, take it out of reset.</span>
<span class="cm">         */</span>
        <span class="n">ctrl</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL</span><span class="p">);</span>
        <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL</span><span class="p">,</span> <span class="n">ctrl</span> <span class="o">|</span> <span class="n">E1000_CTRL_PHY_RST</span><span class="p">);</span>
        <span class="n">E1000_WRITE_FLUSH</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
        <span class="n">msec_delay</span><span class="p">(</span><span class="mi">10</span><span class="p">);</span>
        <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL</span><span class="p">,</span> <span class="n">ctrl</span><span class="p">);</span>
        <span class="n">E1000_WRITE_FLUSH</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
    <span class="p">}</span> <span class="k">else</span> <span class="p">{</span>
        <span class="cm">/* Read the Extended Device Control Register, assert the PHY_RESET_DIR</span>
<span class="cm">         * bit to put the PHY into reset. Then, take it out of reset.</span>
<span class="cm">         */</span>
        <span class="n">ctrl_ext</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL_EXT</span><span class="p">);</span>
        <span class="n">ctrl_ext</span> <span class="o">|=</span> <span class="n">E1000_CTRL_EXT_SDP4_DIR</span><span class="p">;</span>
        <span class="n">ctrl_ext</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="n">E1000_CTRL_EXT_SDP4_DATA</span><span class="p">;</span>
        <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL_EXT</span><span class="p">,</span> <span class="n">ctrl_ext</span><span class="p">);</span>
        <span class="n">E1000_WRITE_FLUSH</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
        <span class="n">msec_delay</span><span class="p">(</span><span class="mi">10</span><span class="p">);</span>
        <span class="n">ctrl_ext</span> <span class="o">|=</span> <span class="n">E1000_CTRL_EXT_SDP4_DATA</span><span class="p">;</span>
        <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">CTRL_EXT</span><span class="p">,</span> <span class="n">ctrl_ext</span><span class="p">);</span>
        <span class="n">E1000_WRITE_FLUSH</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
    <span class="p">}</span>
    <span class="n">udelay</span><span class="p">(</span><span class="mi">150</span><span class="p">);</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm">* Resets the PHY</span>
<span class="cm">*</span>
<span class="cm">* hw - Struct containing variables accessed by shared code</span>
<span class="cm">*</span>
<span class="cm">* Sets bit 15 of the MII Control regiser</span>
<span class="cm">******************************************************************************/</span>
<span class="kt">int32_t</span>
<span class="n">e1000_phy_reset</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">uint16_t</span> <span class="n">phy_data</span><span class="p">;</span>

    <span class="n">DEBUGFUNC</span><span class="p">(</span><span class="s">&quot;e1000_phy_reset&quot;</span><span class="p">);</span>

    <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_CTRL</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">phy_data</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Read Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
    <span class="p">}</span>
    <span class="n">phy_data</span> <span class="o">|=</span> <span class="n">MII_CR_RESET</span><span class="p">;</span>
    <span class="k">if</span><span class="p">(</span><span class="n">e1000_write_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_CTRL</span><span class="p">,</span> <span class="n">phy_data</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Write Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
    <span class="p">}</span>
    <span class="n">udelay</span><span class="p">(</span><span class="mi">1</span><span class="p">);</span>
    <span class="k">return</span> <span class="mi">0</span><span class="p">;</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm">* Probes the expected PHY address for known PHY IDs</span>
<span class="cm">*</span>
<span class="cm">* hw - Struct containing variables accessed by shared code</span>
<span class="cm">******************************************************************************/</span>
<span class="kt">int32_t</span>
<span class="n">e1000_detect_gig_phy</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">uint16_t</span> <span class="n">phy_id_high</span><span class="p">,</span> <span class="n">phy_id_low</span><span class="p">;</span>
    <span class="n">boolean_t</span> <span class="n">match</span> <span class="o">=</span> <span class="n">FALSE</span><span class="p">;</span>

    <span class="n">DEBUGFUNC</span><span class="p">(</span><span class="s">&quot;e1000_detect_gig_phy&quot;</span><span class="p">);</span>

    <span class="cm">/* Read the PHY ID Registers to identify which PHY is onboard. */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_ID1</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">phy_id_high</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Read Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
    <span class="p">}</span>
    <span class="n">hw</span><span class="o">-&gt;</span><span class="n">phy_id</span> <span class="o">=</span> <span class="p">(</span><span class="kt">uint32_t</span><span class="p">)</span> <span class="p">(</span><span class="n">phy_id_high</span> <span class="o">&lt;&lt;</span> <span class="mi">16</span><span class="p">);</span>
    <span class="n">udelay</span><span class="p">(</span><span class="mi">2</span><span class="p">);</span>
    <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_ID2</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">phy_id_low</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Read Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
    <span class="p">}</span>
    <span class="n">hw</span><span class="o">-&gt;</span><span class="n">phy_id</span> <span class="o">|=</span> <span class="p">(</span><span class="kt">uint32_t</span><span class="p">)</span> <span class="p">(</span><span class="n">phy_id_low</span> <span class="o">&amp;</span> <span class="n">PHY_REVISION_MASK</span><span class="p">);</span>
    <span class="n">hw</span><span class="o">-&gt;</span><span class="n">phy_revision</span> <span class="o">=</span> <span class="p">(</span><span class="kt">uint32_t</span><span class="p">)</span> <span class="n">phy_id_low</span> <span class="o">&amp;</span> <span class="o">~</span><span class="n">PHY_REVISION_MASK</span><span class="p">;</span>

    <span class="k">switch</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span><span class="p">)</span> <span class="p">{</span>
    <span class="k">case</span> <span class="nl">e1000_82543</span><span class="p">:</span>
        <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">phy_id</span> <span class="o">==</span> <span class="n">M88E1000_E_PHY_ID</span><span class="p">)</span> <span class="n">match</span> <span class="o">=</span> <span class="n">TRUE</span><span class="p">;</span>
        <span class="k">break</span><span class="p">;</span>
    <span class="k">case</span> <span class="nl">e1000_82544</span><span class="p">:</span>
        <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">phy_id</span> <span class="o">==</span> <span class="n">M88E1000_I_PHY_ID</span><span class="p">)</span> <span class="n">match</span> <span class="o">=</span> <span class="n">TRUE</span><span class="p">;</span>
        <span class="k">break</span><span class="p">;</span>
    <span class="k">case</span> <span class="nl">e1000_82540</span><span class="p">:</span>
    <span class="k">case</span> <span class="nl">e1000_82545</span><span class="p">:</span>
    <span class="k">case</span> <span class="nl">e1000_82546</span><span class="p">:</span>
        <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">phy_id</span> <span class="o">==</span> <span class="n">M88E1011_I_PHY_ID</span><span class="p">)</span> <span class="n">match</span> <span class="o">=</span> <span class="n">TRUE</span><span class="p">;</span>
        <span class="k">break</span><span class="p">;</span>
    <span class="k">default</span><span class="o">:</span>
        <span class="n">DEBUGOUT1</span><span class="p">(</span><span class="s">&quot;Invalid MAC type %d</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">,</span> <span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span><span class="p">);</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_CONFIG</span><span class="p">;</span>
    <span class="p">}</span>
    <span class="k">if</span><span class="p">(</span><span class="n">match</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT1</span><span class="p">(</span><span class="s">&quot;PHY ID 0x%X detected</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">,</span> <span class="n">hw</span><span class="o">-&gt;</span><span class="n">phy_id</span><span class="p">);</span>
        <span class="k">return</span> <span class="mi">0</span><span class="p">;</span>
    <span class="p">}</span>
    <span class="n">DEBUGOUT1</span><span class="p">(</span><span class="s">&quot;Invalid PHY ID 0x%X</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">,</span> <span class="n">hw</span><span class="o">-&gt;</span><span class="n">phy_id</span><span class="p">);</span>
    <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm">* Resets the PHY&#39;s DSP</span>
<span class="cm">*</span>
<span class="cm">* hw - Struct containing variables accessed by shared code</span>
<span class="cm">******************************************************************************/</span>
<span class="k">static</span> <span class="kt">int32_t</span>
<span class="n">e1000_phy_reset_dsp</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">int32_t</span> <span class="n">ret_val</span> <span class="o">=</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
    <span class="n">DEBUGFUNC</span><span class="p">(</span><span class="s">&quot;e1000_phy_reset_dsp&quot;</span><span class="p">);</span>
    
    <span class="k">do</span> <span class="p">{</span>
        <span class="k">if</span><span class="p">(</span><span class="n">e1000_write_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="mi">29</span><span class="p">,</span> <span class="mh">0x001d</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="k">break</span><span class="p">;</span>
        <span class="k">if</span><span class="p">(</span><span class="n">e1000_write_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="mi">30</span><span class="p">,</span> <span class="mh">0x00c1</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="k">break</span><span class="p">;</span>
        <span class="k">if</span><span class="p">(</span><span class="n">e1000_write_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="mi">30</span><span class="p">,</span> <span class="mh">0x0000</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="k">break</span><span class="p">;</span>
        <span class="n">ret_val</span> <span class="o">=</span> <span class="mi">0</span><span class="p">;</span>
    <span class="p">}</span> <span class="k">while</span><span class="p">(</span><span class="mi">0</span><span class="p">);</span>

    <span class="k">if</span><span class="p">(</span><span class="n">ret_val</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Write Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
    <span class="k">return</span> <span class="n">ret_val</span><span class="p">;</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm">* Get PHY information from various PHY registers</span>
<span class="cm">*</span>
<span class="cm">* hw - Struct containing variables accessed by shared code</span>
<span class="cm">* phy_info - PHY information structure</span>
<span class="cm">******************************************************************************/</span>
<span class="kt">int32_t</span>
<span class="n">e1000_phy_get_info</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">,</span>
                   <span class="k">struct</span> <span class="nc">e1000_phy_info</span> <span class="o">*</span><span class="n">phy_info</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">int32_t</span> <span class="n">ret_val</span> <span class="o">=</span> <span class="o">-</span><span class="n">E1000_ERR_PHY</span><span class="p">;</span>
    <span class="kt">uint16_t</span> <span class="n">phy_data</span><span class="p">;</span>

    <span class="n">DEBUGFUNC</span><span class="p">(</span><span class="s">&quot;e1000_phy_get_info&quot;</span><span class="p">);</span>

    <span class="n">phy_info</span><span class="o">-&gt;</span><span class="n">cable_length</span> <span class="o">=</span> <span class="n">e1000_cable_length_undefined</span><span class="p">;</span>
    <span class="n">phy_info</span><span class="o">-&gt;</span><span class="n">extended_10bt_distance</span> <span class="o">=</span> <span class="n">e1000_10bt_ext_dist_enable_undefined</span><span class="p">;</span>
    <span class="n">phy_info</span><span class="o">-&gt;</span><span class="n">cable_polarity</span> <span class="o">=</span> <span class="n">e1000_rev_polarity_undefined</span><span class="p">;</span>
    <span class="n">phy_info</span><span class="o">-&gt;</span><span class="n">polarity_correction</span> <span class="o">=</span> <span class="n">e1000_polarity_reversal_undefined</span><span class="p">;</span>
    <span class="n">phy_info</span><span class="o">-&gt;</span><span class="n">mdix_mode</span> <span class="o">=</span> <span class="n">e1000_auto_x_mode_undefined</span><span class="p">;</span>
    <span class="n">phy_info</span><span class="o">-&gt;</span><span class="n">local_rx</span> <span class="o">=</span> <span class="n">e1000_1000t_rx_status_undefined</span><span class="p">;</span>
    <span class="n">phy_info</span><span class="o">-&gt;</span><span class="n">remote_rx</span> <span class="o">=</span> <span class="n">e1000_1000t_rx_status_undefined</span><span class="p">;</span>

    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">media_type</span> <span class="o">!=</span> <span class="n">e1000_media_type_copper</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY info is only valid for copper media</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_CONFIG</span><span class="p">;</span>
    <span class="p">}</span>

    <span class="k">do</span> <span class="p">{</span>
        <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_STATUS</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">phy_data</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="k">break</span><span class="p">;</span>
        <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_STATUS</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">phy_data</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="k">break</span><span class="p">;</span>
        <span class="k">if</span><span class="p">((</span><span class="n">phy_data</span> <span class="o">&amp;</span> <span class="n">MII_SR_LINK_STATUS</span><span class="p">)</span> <span class="o">!=</span> <span class="n">MII_SR_LINK_STATUS</span><span class="p">)</span> <span class="p">{</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY info is only valid if link is up</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
            <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_CONFIG</span><span class="p">;</span>
        <span class="p">}</span>

        <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">M88E1000_PHY_SPEC_CTRL</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">phy_data</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span>
            <span class="k">break</span><span class="p">;</span>
        <span class="n">phy_info</span><span class="o">-&gt;</span><span class="n">extended_10bt_distance</span> <span class="o">=</span>
            <span class="p">(</span><span class="n">phy_data</span> <span class="o">&amp;</span> <span class="n">M88E1000_PSCR_10BT_EXT_DIST_ENABLE</span><span class="p">)</span> <span class="o">&gt;&gt;</span>
            <span class="n">M88E1000_PSCR_10BT_EXT_DIST_ENABLE_SHIFT</span><span class="p">;</span>
        <span class="n">phy_info</span><span class="o">-&gt;</span><span class="n">polarity_correction</span> <span class="o">=</span>
            <span class="p">(</span><span class="n">phy_data</span> <span class="o">&amp;</span> <span class="n">M88E1000_PSCR_POLARITY_REVERSAL</span><span class="p">)</span> <span class="o">&gt;&gt;</span>
            <span class="n">M88E1000_PSCR_POLARITY_REVERSAL_SHIFT</span><span class="p">;</span>

        <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">M88E1000_PHY_SPEC_STATUS</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">phy_data</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span>
            <span class="k">break</span><span class="p">;</span>
        <span class="n">phy_info</span><span class="o">-&gt;</span><span class="n">cable_polarity</span> <span class="o">=</span> <span class="p">(</span><span class="n">phy_data</span> <span class="o">&amp;</span> <span class="n">M88E1000_PSSR_REV_POLARITY</span><span class="p">)</span> <span class="o">&gt;&gt;</span>
            <span class="n">M88E1000_PSSR_REV_POLARITY_SHIFT</span><span class="p">;</span>
        <span class="n">phy_info</span><span class="o">-&gt;</span><span class="n">mdix_mode</span> <span class="o">=</span> <span class="p">(</span><span class="n">phy_data</span> <span class="o">&amp;</span> <span class="n">M88E1000_PSSR_MDIX</span><span class="p">)</span> <span class="o">&gt;&gt;</span>
            <span class="n">M88E1000_PSSR_MDIX_SHIFT</span><span class="p">;</span>
        <span class="k">if</span><span class="p">(</span><span class="n">phy_data</span> <span class="o">&amp;</span> <span class="n">M88E1000_PSSR_1000MBS</span><span class="p">)</span> <span class="p">{</span>
            <span class="cm">/* Cable Length Estimation and Local/Remote Receiver Informatoion</span>
<span class="cm">             * are only valid at 1000 Mbps</span>
<span class="cm">             */</span>
            <span class="n">phy_info</span><span class="o">-&gt;</span><span class="n">cable_length</span> <span class="o">=</span> <span class="p">((</span><span class="n">phy_data</span> <span class="o">&amp;</span> <span class="n">M88E1000_PSSR_CABLE_LENGTH</span><span class="p">)</span> <span class="o">&gt;&gt;</span>
                                      <span class="n">M88E1000_PSSR_CABLE_LENGTH_SHIFT</span><span class="p">);</span>
            <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_phy_reg</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">PHY_1000T_STATUS</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">phy_data</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> 
                <span class="k">break</span><span class="p">;</span>
            <span class="n">phy_info</span><span class="o">-&gt;</span><span class="n">local_rx</span> <span class="o">=</span> <span class="p">(</span><span class="n">phy_data</span> <span class="o">&amp;</span> <span class="n">SR_1000T_LOCAL_RX_STATUS</span><span class="p">)</span> <span class="o">&gt;&gt;</span>
                <span class="n">SR_1000T_LOCAL_RX_STATUS_SHIFT</span><span class="p">;</span>
            <span class="n">phy_info</span><span class="o">-&gt;</span><span class="n">remote_rx</span> <span class="o">=</span> <span class="p">(</span><span class="n">phy_data</span> <span class="o">&amp;</span> <span class="n">SR_1000T_REMOTE_RX_STATUS</span><span class="p">)</span> <span class="o">&gt;&gt;</span>
                <span class="n">SR_1000T_REMOTE_RX_STATUS_SHIFT</span><span class="p">;</span>
        <span class="p">}</span>
        <span class="n">ret_val</span> <span class="o">=</span> <span class="mi">0</span><span class="p">;</span>
    <span class="p">}</span> <span class="k">while</span><span class="p">(</span><span class="mi">0</span><span class="p">);</span>

    <span class="k">if</span><span class="p">(</span><span class="n">ret_val</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;PHY Read Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
    <span class="k">return</span> <span class="n">ret_val</span><span class="p">;</span>
<span class="p">}</span>

<span class="kt">int32_t</span>
<span class="n">e1000_validate_mdi_setting</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">)</span>
<span class="p">{</span>
    <span class="n">DEBUGFUNC</span><span class="p">(</span><span class="s">&quot;e1000_validate_mdi_settings&quot;</span><span class="p">);</span>

    <span class="k">if</span><span class="p">(</span><span class="o">!</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">autoneg</span> <span class="o">&amp;&amp;</span> <span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">mdix</span> <span class="o">==</span> <span class="mi">0</span> <span class="o">||</span> <span class="n">hw</span><span class="o">-&gt;</span><span class="n">mdix</span> <span class="o">==</span> <span class="mi">3</span><span class="p">))</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Invalid MDI setting detected</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="n">hw</span><span class="o">-&gt;</span><span class="n">mdix</span> <span class="o">=</span> <span class="mi">1</span><span class="p">;</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_CONFIG</span><span class="p">;</span>
    <span class="p">}</span>
    <span class="k">return</span> <span class="mi">0</span><span class="p">;</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm"> * Raises the EEPROM&#39;s clock input.</span>
<span class="cm"> *</span>
<span class="cm"> * hw - Struct containing variables accessed by shared code</span>
<span class="cm"> * eecd - EECD&#39;s current value</span>
<span class="cm"> *****************************************************************************/</span>
<span class="k">static</span> <span class="kt">void</span>
<span class="n">e1000_raise_ee_clk</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">,</span>
                   <span class="kt">uint32_t</span> <span class="o">*</span><span class="n">eecd</span><span class="p">)</span>
<span class="p">{</span>
    <span class="cm">/* Raise the clock input to the EEPROM (by setting the SK bit), and then</span>
<span class="cm">     * wait &lt;delay&gt; microseconds.</span>
<span class="cm">     */</span>
    <span class="o">*</span><span class="n">eecd</span> <span class="o">=</span> <span class="o">*</span><span class="n">eecd</span> <span class="o">|</span> <span class="n">E1000_EECD_SK</span><span class="p">;</span>
    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">,</span> <span class="o">*</span><span class="n">eecd</span><span class="p">);</span>
    <span class="n">E1000_WRITE_FLUSH</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
    <span class="n">udelay</span><span class="p">(</span><span class="mi">50</span><span class="p">);</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm"> * Lowers the EEPROM&#39;s clock input.</span>
<span class="cm"> *</span>
<span class="cm"> * hw - Struct containing variables accessed by shared code </span>
<span class="cm"> * eecd - EECD&#39;s current value</span>
<span class="cm"> *****************************************************************************/</span>
<span class="k">static</span> <span class="kt">void</span>
<span class="n">e1000_lower_ee_clk</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">,</span>
                   <span class="kt">uint32_t</span> <span class="o">*</span><span class="n">eecd</span><span class="p">)</span>
<span class="p">{</span>
    <span class="cm">/* Lower the clock input to the EEPROM (by clearing the SK bit), and then </span>
<span class="cm">     * wait 50 microseconds. </span>
<span class="cm">     */</span>
    <span class="o">*</span><span class="n">eecd</span> <span class="o">=</span> <span class="o">*</span><span class="n">eecd</span> <span class="o">&amp;</span> <span class="o">~</span><span class="n">E1000_EECD_SK</span><span class="p">;</span>
    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">,</span> <span class="o">*</span><span class="n">eecd</span><span class="p">);</span>
    <span class="n">E1000_WRITE_FLUSH</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
    <span class="n">udelay</span><span class="p">(</span><span class="mi">50</span><span class="p">);</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm"> * Shift data bits out to the EEPROM.</span>
<span class="cm"> *</span>
<span class="cm"> * hw - Struct containing variables accessed by shared code</span>
<span class="cm"> * data - data to send to the EEPROM</span>
<span class="cm"> * count - number of bits to shift out</span>
<span class="cm"> *****************************************************************************/</span>
<span class="k">static</span> <span class="kt">void</span>
<span class="n">e1000_shift_out_ee_bits</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">,</span>
                        <span class="kt">uint16_t</span> <span class="n">data</span><span class="p">,</span>
                        <span class="kt">uint16_t</span> <span class="n">count</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">uint32_t</span> <span class="n">eecd</span><span class="p">;</span>
    <span class="kt">uint32_t</span> <span class="n">mask</span><span class="p">;</span>

    <span class="cm">/* We need to shift &quot;count&quot; bits out to the EEPROM. So, value in the</span>
<span class="cm">     * &quot;data&quot; parameter will be shifted out to the EEPROM one bit at a time.</span>
<span class="cm">     * In order to do this, &quot;data&quot; must be broken down into bits. </span>
<span class="cm">     */</span>
    <span class="n">mask</span> <span class="o">=</span> <span class="mh">0x01</span> <span class="o">&lt;&lt;</span> <span class="p">(</span><span class="n">count</span> <span class="o">-</span> <span class="mi">1</span><span class="p">);</span>
    <span class="n">eecd</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">);</span>
    <span class="n">eecd</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="p">(</span><span class="n">E1000_EECD_DO</span> <span class="o">|</span> <span class="n">E1000_EECD_DI</span><span class="p">);</span>
    <span class="k">do</span> <span class="p">{</span>
        <span class="cm">/* A &quot;1&quot; is shifted out to the EEPROM by setting bit &quot;DI&quot; to a &quot;1&quot;,</span>
<span class="cm">         * and then raising and then lowering the clock (the SK bit controls</span>
<span class="cm">         * the clock input to the EEPROM).  A &quot;0&quot; is shifted out to the EEPROM</span>
<span class="cm">         * by setting &quot;DI&quot; to &quot;0&quot; and then raising and then lowering the clock.</span>
<span class="cm">         */</span>
        <span class="n">eecd</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="n">E1000_EECD_DI</span><span class="p">;</span>

        <span class="k">if</span><span class="p">(</span><span class="n">data</span> <span class="o">&amp;</span> <span class="n">mask</span><span class="p">)</span>
            <span class="n">eecd</span> <span class="o">|=</span> <span class="n">E1000_EECD_DI</span><span class="p">;</span>

        <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">,</span> <span class="n">eecd</span><span class="p">);</span>
        <span class="n">E1000_WRITE_FLUSH</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>

        <span class="n">udelay</span><span class="p">(</span><span class="mi">50</span><span class="p">);</span>

        <span class="n">e1000_raise_ee_clk</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">eecd</span><span class="p">);</span>
        <span class="n">e1000_lower_ee_clk</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">eecd</span><span class="p">);</span>

        <span class="n">mask</span> <span class="o">=</span> <span class="n">mask</span> <span class="o">&gt;&gt;</span> <span class="mi">1</span><span class="p">;</span>

    <span class="p">}</span> <span class="k">while</span><span class="p">(</span><span class="n">mask</span><span class="p">);</span>

    <span class="cm">/* We leave the &quot;DI&quot; bit set to &quot;0&quot; when we leave this routine. */</span>
    <span class="n">eecd</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="n">E1000_EECD_DI</span><span class="p">;</span>
    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">,</span> <span class="n">eecd</span><span class="p">);</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm"> * Shift data bits in from the EEPROM</span>
<span class="cm"> *</span>
<span class="cm"> * hw - Struct containing variables accessed by shared code</span>
<span class="cm"> *****************************************************************************/</span>
<span class="k">static</span> <span class="kt">uint16_t</span>
<span class="n">e1000_shift_in_ee_bits</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">uint32_t</span> <span class="n">eecd</span><span class="p">;</span>
    <span class="kt">uint32_t</span> <span class="n">i</span><span class="p">;</span>
    <span class="kt">uint16_t</span> <span class="n">data</span><span class="p">;</span>

    <span class="cm">/* In order to read a register from the EEPROM, we need to shift &#39;count&#39;</span>
<span class="cm">     * bits in from the EEPROM. Bits are &quot;shifted in&quot; by raising the clock</span>
<span class="cm">     * input to the EEPROM (setting the SK bit), and then reading the value of</span>
<span class="cm">     * the &quot;DO&quot; bit.  During this &quot;shifting in&quot; process the &quot;DI&quot; bit should</span>
<span class="cm">     * always be clear.</span>
<span class="cm">     */</span>

    <span class="n">eecd</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">);</span>

    <span class="n">eecd</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="p">(</span><span class="n">E1000_EECD_DO</span> <span class="o">|</span> <span class="n">E1000_EECD_DI</span><span class="p">);</span>
    <span class="n">data</span> <span class="o">=</span> <span class="mi">0</span><span class="p">;</span>

    <span class="k">for</span><span class="p">(</span><span class="n">i</span> <span class="o">=</span> <span class="mi">0</span><span class="p">;</span> <span class="n">i</span> <span class="o">&lt;</span> <span class="mi">16</span><span class="p">;</span> <span class="n">i</span><span class="o">++</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">data</span> <span class="o">=</span> <span class="n">data</span> <span class="o">&lt;&lt;</span> <span class="mi">1</span><span class="p">;</span>
        <span class="n">e1000_raise_ee_clk</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">eecd</span><span class="p">);</span>

        <span class="n">eecd</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">);</span>

        <span class="n">eecd</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="p">(</span><span class="n">E1000_EECD_DI</span><span class="p">);</span>
        <span class="k">if</span><span class="p">(</span><span class="n">eecd</span> <span class="o">&amp;</span> <span class="n">E1000_EECD_DO</span><span class="p">)</span>
            <span class="n">data</span> <span class="o">|=</span> <span class="mi">1</span><span class="p">;</span>

        <span class="n">e1000_lower_ee_clk</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">eecd</span><span class="p">);</span>
    <span class="p">}</span>

    <span class="k">return</span> <span class="n">data</span><span class="p">;</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm"> * Prepares EEPROM for access</span>
<span class="cm"> *</span>
<span class="cm"> * hw - Struct containing variables accessed by shared code</span>
<span class="cm"> *</span>
<span class="cm"> * Lowers EEPROM clock. Clears input pin. Sets the chip select pin. This </span>
<span class="cm"> * function should be called before issuing a command to the EEPROM.</span>
<span class="cm"> *****************************************************************************/</span>
<span class="k">static</span> <span class="kt">void</span>
<span class="n">e1000_setup_eeprom</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">uint32_t</span> <span class="n">eecd</span><span class="p">;</span>

    <span class="n">eecd</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">);</span>

    <span class="cm">/* Clear SK and DI */</span>
    <span class="n">eecd</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="p">(</span><span class="n">E1000_EECD_SK</span> <span class="o">|</span> <span class="n">E1000_EECD_DI</span><span class="p">);</span>
    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">,</span> <span class="n">eecd</span><span class="p">);</span>

    <span class="cm">/* Set CS */</span>
    <span class="n">eecd</span> <span class="o">|=</span> <span class="n">E1000_EECD_CS</span><span class="p">;</span>
    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">,</span> <span class="n">eecd</span><span class="p">);</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm"> * Returns EEPROM to a &quot;standby&quot; state</span>
<span class="cm"> * </span>
<span class="cm"> * hw - Struct containing variables accessed by shared code</span>
<span class="cm"> *****************************************************************************/</span>
<span class="k">static</span> <span class="kt">void</span>
<span class="n">e1000_standby_eeprom</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">uint32_t</span> <span class="n">eecd</span><span class="p">;</span>

    <span class="n">eecd</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">);</span>

    <span class="cm">/* Deselct EEPROM */</span>
    <span class="n">eecd</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="p">(</span><span class="n">E1000_EECD_CS</span> <span class="o">|</span> <span class="n">E1000_EECD_SK</span><span class="p">);</span>
    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">,</span> <span class="n">eecd</span><span class="p">);</span>
    <span class="n">E1000_WRITE_FLUSH</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
    <span class="n">udelay</span><span class="p">(</span><span class="mi">50</span><span class="p">);</span>

    <span class="cm">/* Clock high */</span>
    <span class="n">eecd</span> <span class="o">|=</span> <span class="n">E1000_EECD_SK</span><span class="p">;</span>
    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">,</span> <span class="n">eecd</span><span class="p">);</span>
    <span class="n">E1000_WRITE_FLUSH</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
    <span class="n">udelay</span><span class="p">(</span><span class="mi">50</span><span class="p">);</span>

    <span class="cm">/* Select EEPROM */</span>
    <span class="n">eecd</span> <span class="o">|=</span> <span class="n">E1000_EECD_CS</span><span class="p">;</span>
    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">,</span> <span class="n">eecd</span><span class="p">);</span>
    <span class="n">E1000_WRITE_FLUSH</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
    <span class="n">udelay</span><span class="p">(</span><span class="mi">50</span><span class="p">);</span>

    <span class="cm">/* Clock low */</span>
    <span class="n">eecd</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="n">E1000_EECD_SK</span><span class="p">;</span>
    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">,</span> <span class="n">eecd</span><span class="p">);</span>
    <span class="n">E1000_WRITE_FLUSH</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
    <span class="n">udelay</span><span class="p">(</span><span class="mi">50</span><span class="p">);</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm"> * Raises then lowers the EEPROM&#39;s clock pin</span>
<span class="cm"> *</span>
<span class="cm"> * hw - Struct containing variables accessed by shared code</span>
<span class="cm"> *****************************************************************************/</span>
<span class="k">static</span> <span class="kt">void</span>
<span class="n">e1000_clock_eeprom</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">uint32_t</span> <span class="n">eecd</span><span class="p">;</span>

    <span class="n">eecd</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">);</span>

    <span class="cm">/* Rising edge of clock */</span>
    <span class="n">eecd</span> <span class="o">|=</span> <span class="n">E1000_EECD_SK</span><span class="p">;</span>
    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">,</span> <span class="n">eecd</span><span class="p">);</span>
    <span class="n">E1000_WRITE_FLUSH</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
    <span class="n">udelay</span><span class="p">(</span><span class="mi">50</span><span class="p">);</span>

    <span class="cm">/* Falling edge of clock */</span>
    <span class="n">eecd</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="n">E1000_EECD_SK</span><span class="p">;</span>
    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">,</span> <span class="n">eecd</span><span class="p">);</span>
    <span class="n">E1000_WRITE_FLUSH</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
    <span class="n">udelay</span><span class="p">(</span><span class="mi">50</span><span class="p">);</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm"> * Terminates a command by lowering the EEPROM&#39;s chip select pin</span>
<span class="cm"> *</span>
<span class="cm"> * hw - Struct containing variables accessed by shared code</span>
<span class="cm"> *****************************************************************************/</span>
<span class="k">static</span> <span class="kt">void</span>
<span class="n">e1000_cleanup_eeprom</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">uint32_t</span> <span class="n">eecd</span><span class="p">;</span>

    <span class="n">eecd</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">);</span>

    <span class="n">eecd</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="p">(</span><span class="n">E1000_EECD_CS</span> <span class="o">|</span> <span class="n">E1000_EECD_DI</span><span class="p">);</span>

    <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">,</span> <span class="n">eecd</span><span class="p">);</span>

    <span class="n">e1000_clock_eeprom</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm"> * Reads a 16 bit word from the EEPROM.</span>
<span class="cm"> *</span>
<span class="cm"> * hw - Struct containing variables accessed by shared code</span>
<span class="cm"> * offset - offset of  word in the EEPROM to read</span>
<span class="cm"> * data - word read from the EEPROM </span>
<span class="cm"> *****************************************************************************/</span>
<span class="kt">int32_t</span>
<span class="n">e1000_read_eeprom</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">,</span>
                  <span class="kt">uint16_t</span> <span class="n">offset</span><span class="p">,</span>
                  <span class="kt">uint16_t</span> <span class="o">*</span><span class="n">data</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">uint32_t</span> <span class="n">eecd</span><span class="p">;</span>
    <span class="kt">uint32_t</span> <span class="n">i</span> <span class="o">=</span> <span class="mi">0</span><span class="p">;</span>
    <span class="n">boolean_t</span> <span class="n">large_eeprom</span> <span class="o">=</span> <span class="n">FALSE</span><span class="p">;</span>

    <span class="n">DEBUGFUNC</span><span class="p">(</span><span class="s">&quot;e1000_read_eeprom&quot;</span><span class="p">);</span>

    <span class="cm">/* Request EEPROM Access */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">&gt;</span> <span class="n">e1000_82544</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">eecd</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">);</span>
        <span class="k">if</span><span class="p">(</span><span class="n">eecd</span> <span class="o">&amp;</span> <span class="n">E1000_EECD_SIZE</span><span class="p">)</span> <span class="n">large_eeprom</span> <span class="o">=</span> <span class="n">TRUE</span><span class="p">;</span>
        <span class="n">eecd</span> <span class="o">|=</span> <span class="n">E1000_EECD_REQ</span><span class="p">;</span>
        <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">,</span> <span class="n">eecd</span><span class="p">);</span>
        <span class="n">eecd</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">);</span>
        <span class="k">while</span><span class="p">((</span><span class="o">!</span><span class="p">(</span><span class="n">eecd</span> <span class="o">&amp;</span> <span class="n">E1000_EECD_GNT</span><span class="p">))</span> <span class="o">&amp;&amp;</span> <span class="p">(</span><span class="n">i</span> <span class="o">&lt;</span> <span class="mi">100</span><span class="p">))</span> <span class="p">{</span>
            <span class="n">i</span><span class="o">++</span><span class="p">;</span>
            <span class="n">udelay</span><span class="p">(</span><span class="mi">5</span><span class="p">);</span>
            <span class="n">eecd</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">);</span>
        <span class="p">}</span>
        <span class="k">if</span><span class="p">(</span><span class="o">!</span><span class="p">(</span><span class="n">eecd</span> <span class="o">&amp;</span> <span class="n">E1000_EECD_GNT</span><span class="p">))</span> <span class="p">{</span>
            <span class="n">eecd</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="n">E1000_EECD_REQ</span><span class="p">;</span>
            <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">,</span> <span class="n">eecd</span><span class="p">);</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Could not acquire EEPROM grant</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
            <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_EEPROM</span><span class="p">;</span>
        <span class="p">}</span>
    <span class="p">}</span>

    <span class="cm">/*  Prepare the EEPROM for reading  */</span>
    <span class="n">e1000_setup_eeprom</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>

    <span class="cm">/*  Send the READ command (opcode + addr)  */</span>
    <span class="n">e1000_shift_out_ee_bits</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EEPROM_READ_OPCODE</span><span class="p">,</span> <span class="mi">3</span><span class="p">);</span>
    <span class="k">if</span><span class="p">(</span><span class="n">large_eeprom</span><span class="p">)</span> <span class="p">{</span>
        <span class="cm">/* If we have a 256 word EEPROM, there are 8 address bits */</span>
        <span class="n">e1000_shift_out_ee_bits</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">offset</span><span class="p">,</span> <span class="mi">8</span><span class="p">);</span>
    <span class="p">}</span> <span class="k">else</span> <span class="p">{</span>
        <span class="cm">/* If we have a 64 word EEPROM, there are 6 address bits */</span>
        <span class="n">e1000_shift_out_ee_bits</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">offset</span><span class="p">,</span> <span class="mi">6</span><span class="p">);</span>
    <span class="p">}</span>

    <span class="cm">/* Read the data */</span>
    <span class="o">*</span><span class="n">data</span> <span class="o">=</span> <span class="n">e1000_shift_in_ee_bits</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>

    <span class="cm">/* End this read operation */</span>
    <span class="n">e1000_standby_eeprom</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>

    <span class="cm">/* Stop requesting EEPROM access */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">&gt;</span> <span class="n">e1000_82544</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">eecd</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">);</span>
        <span class="n">eecd</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="n">E1000_EECD_REQ</span><span class="p">;</span>
        <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">,</span> <span class="n">eecd</span><span class="p">);</span>
    <span class="p">}</span>

    <span class="k">return</span> <span class="mi">0</span><span class="p">;</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm"> * Verifies that the EEPROM has a valid checksum</span>
<span class="cm"> * </span>
<span class="cm"> * hw - Struct containing variables accessed by shared code</span>
<span class="cm"> *</span>
<span class="cm"> * Reads the first 64 16 bit words of the EEPROM and sums the values read.</span>
<span class="cm"> * If the the sum of the 64 16 bit words is 0xBABA, the EEPROM&#39;s checksum is</span>
<span class="cm"> * valid.</span>
<span class="cm"> *****************************************************************************/</span>
<span class="kt">int32_t</span>
<span class="n">e1000_validate_eeprom_checksum</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">uint16_t</span> <span class="n">checksum</span> <span class="o">=</span> <span class="mi">0</span><span class="p">;</span>
    <span class="kt">uint16_t</span> <span class="n">i</span><span class="p">,</span> <span class="n">eeprom_data</span><span class="p">;</span>

    <span class="n">DEBUGFUNC</span><span class="p">(</span><span class="s">&quot;e1000_validate_eeprom_checksum&quot;</span><span class="p">);</span>

    <span class="k">for</span><span class="p">(</span><span class="n">i</span> <span class="o">=</span> <span class="mi">0</span><span class="p">;</span> <span class="n">i</span> <span class="o">&lt;</span> <span class="p">(</span><span class="n">EEPROM_CHECKSUM_REG</span> <span class="o">+</span> <span class="mi">1</span><span class="p">);</span> <span class="n">i</span><span class="o">++</span><span class="p">)</span> <span class="p">{</span>
        <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_eeprom</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">i</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">eeprom_data</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;EEPROM Read Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
            <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_EEPROM</span><span class="p">;</span>
        <span class="p">}</span>
        <span class="n">checksum</span> <span class="o">+=</span> <span class="n">eeprom_data</span><span class="p">;</span>
    <span class="p">}</span>

    <span class="k">if</span><span class="p">(</span><span class="n">checksum</span> <span class="o">==</span> <span class="p">(</span><span class="kt">uint16_t</span><span class="p">)</span> <span class="n">EEPROM_SUM</span><span class="p">)</span> <span class="p">{</span>
        <span class="k">return</span> <span class="mi">0</span><span class="p">;</span>
    <span class="p">}</span> <span class="k">else</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;EEPROM Checksum Invalid</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>    
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_EEPROM</span><span class="p">;</span>
    <span class="p">}</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm"> * Calculates the EEPROM checksum and writes it to the EEPROM</span>
<span class="cm"> *</span>
<span class="cm"> * hw - Struct containing variables accessed by shared code</span>
<span class="cm"> *</span>
<span class="cm"> * Sums the first 63 16 bit words of the EEPROM. Subtracts the sum from 0xBABA.</span>
<span class="cm"> * Writes the difference to word offset 63 of the EEPROM.</span>
<span class="cm"> *****************************************************************************/</span>
<span class="kt">int32_t</span>
<span class="n">e1000_update_eeprom_checksum</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">uint16_t</span> <span class="n">checksum</span> <span class="o">=</span> <span class="mi">0</span><span class="p">;</span>
    <span class="kt">uint16_t</span> <span class="n">i</span><span class="p">,</span> <span class="n">eeprom_data</span><span class="p">;</span>

    <span class="n">DEBUGFUNC</span><span class="p">(</span><span class="s">&quot;e1000_update_eeprom_checksum&quot;</span><span class="p">);</span>

    <span class="k">for</span><span class="p">(</span><span class="n">i</span> <span class="o">=</span> <span class="mi">0</span><span class="p">;</span> <span class="n">i</span> <span class="o">&lt;</span> <span class="n">EEPROM_CHECKSUM_REG</span><span class="p">;</span> <span class="n">i</span><span class="o">++</span><span class="p">)</span> <span class="p">{</span>
        <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_eeprom</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">i</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">eeprom_data</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;EEPROM Read Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
            <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_EEPROM</span><span class="p">;</span>
        <span class="p">}</span>
        <span class="n">checksum</span> <span class="o">+=</span> <span class="n">eeprom_data</span><span class="p">;</span>
    <span class="p">}</span>
    <span class="n">checksum</span> <span class="o">=</span> <span class="p">(</span><span class="kt">uint16_t</span><span class="p">)</span> <span class="n">EEPROM_SUM</span> <span class="o">-</span> <span class="n">checksum</span><span class="p">;</span>
    <span class="k">if</span><span class="p">(</span><span class="n">e1000_write_eeprom</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EEPROM_CHECKSUM_REG</span><span class="p">,</span> <span class="n">checksum</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;EEPROM Write Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_EEPROM</span><span class="p">;</span>
    <span class="p">}</span>
    <span class="k">return</span> <span class="mi">0</span><span class="p">;</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm"> * Writes a 16 bit word to a given offset in the EEPROM.</span>
<span class="cm"> *</span>
<span class="cm"> * hw - Struct containing variables accessed by shared code</span>
<span class="cm"> * offset - offset within the EEPROM to be written to</span>
<span class="cm"> * data - 16 bit word to be writen to the EEPROM</span>
<span class="cm"> *</span>
<span class="cm"> * If e1000_update_eeprom_checksum is not called after this function, the </span>
<span class="cm"> * EEPROM will most likely contain an invalid checksum.</span>
<span class="cm"> *****************************************************************************/</span>
<span class="kt">int32_t</span>
<span class="n">e1000_write_eeprom</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">,</span>
                   <span class="kt">uint16_t</span> <span class="n">offset</span><span class="p">,</span>
                   <span class="kt">uint16_t</span> <span class="n">data</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">uint32_t</span> <span class="n">eecd</span><span class="p">;</span>
    <span class="kt">uint32_t</span> <span class="n">i</span> <span class="o">=</span> <span class="mi">0</span><span class="p">;</span>
    <span class="kt">int32_t</span> <span class="n">status</span> <span class="o">=</span> <span class="mi">0</span><span class="p">;</span>
    <span class="n">boolean_t</span> <span class="n">large_eeprom</span> <span class="o">=</span> <span class="n">FALSE</span><span class="p">;</span>

    <span class="n">DEBUGFUNC</span><span class="p">(</span><span class="s">&quot;e1000_write_eeprom&quot;</span><span class="p">);</span>

    <span class="cm">/* Request EEPROM Access */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">&gt;</span> <span class="n">e1000_82544</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">eecd</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">);</span>
        <span class="k">if</span><span class="p">(</span><span class="n">eecd</span> <span class="o">&amp;</span> <span class="n">E1000_EECD_SIZE</span><span class="p">)</span> <span class="n">large_eeprom</span> <span class="o">=</span> <span class="n">TRUE</span><span class="p">;</span>
        <span class="n">eecd</span> <span class="o">|=</span> <span class="n">E1000_EECD_REQ</span><span class="p">;</span>
        <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">,</span> <span class="n">eecd</span><span class="p">);</span>
        <span class="n">eecd</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">);</span>
        <span class="k">while</span><span class="p">((</span><span class="o">!</span><span class="p">(</span><span class="n">eecd</span> <span class="o">&amp;</span> <span class="n">E1000_EECD_GNT</span><span class="p">))</span> <span class="o">&amp;&amp;</span> <span class="p">(</span><span class="n">i</span> <span class="o">&lt;</span> <span class="mi">100</span><span class="p">))</span> <span class="p">{</span>
            <span class="n">i</span><span class="o">++</span><span class="p">;</span>
            <span class="n">udelay</span><span class="p">(</span><span class="mi">5</span><span class="p">);</span>
            <span class="n">eecd</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">);</span>
        <span class="p">}</span>
        <span class="k">if</span><span class="p">(</span><span class="o">!</span><span class="p">(</span><span class="n">eecd</span> <span class="o">&amp;</span> <span class="n">E1000_EECD_GNT</span><span class="p">))</span> <span class="p">{</span>
            <span class="n">eecd</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="n">E1000_EECD_REQ</span><span class="p">;</span>
            <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">,</span> <span class="n">eecd</span><span class="p">);</span>
            <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;Could not acquire EEPROM grant</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
            <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_EEPROM</span><span class="p">;</span>
        <span class="p">}</span>
    <span class="p">}</span>

    <span class="cm">/* Prepare the EEPROM for writing  */</span>
    <span class="n">e1000_setup_eeprom</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>

    <span class="cm">/* Send the 9-bit (or 11-bit on large EEPROM) EWEN (write enable) command</span>
<span class="cm">     * to the EEPROM (5-bit opcode plus 4/6-bit dummy). This puts the EEPROM</span>
<span class="cm">     * into write/erase mode. </span>
<span class="cm">     */</span>
    <span class="n">e1000_shift_out_ee_bits</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EEPROM_EWEN_OPCODE</span><span class="p">,</span> <span class="mi">5</span><span class="p">);</span>
    <span class="k">if</span><span class="p">(</span><span class="n">large_eeprom</span><span class="p">)</span> 
        <span class="n">e1000_shift_out_ee_bits</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="mi">0</span><span class="p">,</span> <span class="mi">6</span><span class="p">);</span>
    <span class="k">else</span>
        <span class="nf">e1000_shift_out_ee_bits</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="mi">0</span><span class="p">,</span> <span class="mi">4</span><span class="p">);</span>

    <span class="cm">/* Prepare the EEPROM */</span>
    <span class="n">e1000_standby_eeprom</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>

    <span class="cm">/* Send the Write command (3-bit opcode + addr) */</span>
    <span class="n">e1000_shift_out_ee_bits</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EEPROM_WRITE_OPCODE</span><span class="p">,</span> <span class="mi">3</span><span class="p">);</span>
    <span class="k">if</span><span class="p">(</span><span class="n">large_eeprom</span><span class="p">)</span> 
        <span class="cm">/* If we have a 256 word EEPROM, there are 8 address bits */</span>
        <span class="n">e1000_shift_out_ee_bits</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">offset</span><span class="p">,</span> <span class="mi">8</span><span class="p">);</span>
    <span class="k">else</span>
        <span class="cm">/* If we have a 64 word EEPROM, there are 6 address bits */</span>
        <span class="n">e1000_shift_out_ee_bits</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">offset</span><span class="p">,</span> <span class="mi">6</span><span class="p">);</span>

    <span class="cm">/* Send the data */</span>
    <span class="n">e1000_shift_out_ee_bits</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">data</span><span class="p">,</span> <span class="mi">16</span><span class="p">);</span>

    <span class="cm">/* Toggle the CS line.  This in effect tells to EEPROM to actually execute </span>
<span class="cm">     * the command in question.</span>
<span class="cm">     */</span>
    <span class="n">e1000_standby_eeprom</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>

    <span class="cm">/* Now read DO repeatedly until is high (equal to &#39;1&#39;).  The EEEPROM will</span>
<span class="cm">     * signal that the command has been completed by raising the DO signal.</span>
<span class="cm">     * If DO does not go high in 10 milliseconds, then error out.</span>
<span class="cm">     */</span>
    <span class="k">for</span><span class="p">(</span><span class="n">i</span> <span class="o">=</span> <span class="mi">0</span><span class="p">;</span> <span class="n">i</span> <span class="o">&lt;</span> <span class="mi">200</span><span class="p">;</span> <span class="n">i</span><span class="o">++</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">eecd</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">);</span>
        <span class="k">if</span><span class="p">(</span><span class="n">eecd</span> <span class="o">&amp;</span> <span class="n">E1000_EECD_DO</span><span class="p">)</span> <span class="k">break</span><span class="p">;</span>
        <span class="n">udelay</span><span class="p">(</span><span class="mi">50</span><span class="p">);</span>
    <span class="p">}</span>
    <span class="k">if</span><span class="p">(</span><span class="n">i</span> <span class="o">==</span> <span class="mi">200</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;EEPROM Write did not complete</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="n">status</span> <span class="o">=</span> <span class="o">-</span><span class="n">E1000_ERR_EEPROM</span><span class="p">;</span>
    <span class="p">}</span>

    <span class="cm">/* Recover from write */</span>
    <span class="n">e1000_standby_eeprom</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>

    <span class="cm">/* Send the 9-bit (or 11-bit on large EEPROM) EWDS (write disable) command</span>
<span class="cm">     * to the EEPROM (5-bit opcode plus 4/6-bit dummy). This takes the EEPROM</span>
<span class="cm">     * out of write/erase mode.</span>
<span class="cm">     */</span>
    <span class="n">e1000_shift_out_ee_bits</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EEPROM_EWDS_OPCODE</span><span class="p">,</span> <span class="mi">5</span><span class="p">);</span>
    <span class="k">if</span><span class="p">(</span><span class="n">large_eeprom</span><span class="p">)</span> 
        <span class="n">e1000_shift_out_ee_bits</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="mi">0</span><span class="p">,</span> <span class="mi">6</span><span class="p">);</span>
    <span class="k">else</span>
        <span class="nf">e1000_shift_out_ee_bits</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="mi">0</span><span class="p">,</span> <span class="mi">4</span><span class="p">);</span>

    <span class="cm">/* Done with writing */</span>
    <span class="n">e1000_cleanup_eeprom</span><span class="p">(</span><span class="n">hw</span><span class="p">);</span>

    <span class="cm">/* Stop requesting EEPROM access */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">hw</span><span class="o">-&gt;</span><span class="n">mac_type</span> <span class="o">&gt;</span> <span class="n">e1000_82544</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">eecd</span> <span class="o">=</span> <span class="n">E1000_READ_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">);</span>
        <span class="n">eecd</span> <span class="o">&amp;=</span> <span class="o">~</span><span class="n">E1000_EECD_REQ</span><span class="p">;</span>
        <span class="n">E1000_WRITE_REG</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">EECD</span><span class="p">,</span> <span class="n">eecd</span><span class="p">);</span>
    <span class="p">}</span>

    <span class="k">return</span> <span class="n">status</span><span class="p">;</span>
<span class="p">}</span>

<span class="cm">/******************************************************************************</span>
<span class="cm"> * Reads the adapter&#39;s part number from the EEPROM</span>
<span class="cm"> *</span>
<span class="cm"> * hw - Struct containing variables accessed by shared code</span>
<span class="cm"> * part_num - Adapter&#39;s part number</span>
<span class="cm"> *****************************************************************************/</span>
<span class="kt">int32_t</span>
<span class="n">e1000_read_part_num</span><span class="p">(</span><span class="k">struct</span> <span class="nc">e1000_hw</span> <span class="o">*</span><span class="n">hw</span><span class="p">,</span>
                    <span class="kt">uint32_t</span> <span class="o">*</span><span class="n">part_num</span><span class="p">)</span>
<span class="p">{</span>
    <span class="kt">uint16_t</span> <span class="n">offset</span> <span class="o">=</span> <span class="n">EEPROM_PBA_BYTE_1</span><span class="p">;</span>
    <span class="kt">uint16_t</span> <span class="n">eeprom_data</span><span class="p">;</span>

    <span class="n">DEBUGFUNC</span><span class="p">(</span><span class="s">&quot;e1000_read_part_num&quot;</span><span class="p">);</span>

    <span class="cm">/* Get word 0 from EEPROM */</span>
    <span class="k">if</span><span class="p">(</span><span class="n">e1000_read_eeprom</span><span class="p">(</span><span class="n">hw</span><span class="p">,</span> <span class="n">offset</span><span class="p">,</span> <span class="o">&amp;</span><span class="n">eeprom_data</span><span class="p">)</span> <span class="o">&lt;</span> <span class="mi">0</span><span class="p">)</span> <span class="p">{</span>
        <span class="n">DEBUGOUT</span><span class="p">(</span><span class="s">&quot;EEPROM Read Error</span><span class="se">\n</span><span class="s">&quot;</span><span class="p">);</span>
        <span class="k">return</span> <span class="o">-</span><span class="n">E1000_ERR_EEPROM</span><span class="p">;</span>
    <span class="p">}</span>
    <span class="cm">/* Save word 0 in upper half of part_num */</span>
