From 07e3a510638930e3a4540c42482d24f5249a2b50 Mon Sep 17 00:00:00 2001
From: Luka Perkov <luka@openwrt.org>
Date: Fri, 12 Oct 2012 12:13:55 +0000
Subject: [docs] update VLAN tag example

git-svn-id: svn://svn.openwrt.org/openwrt/trunk@33732 3c298f89-4303-0410-b956-a3cf2f4a3e73
---
 docs/network.tex | 6 ++++--
 1 file changed, 4 insertions(+), 2 deletions(-)

(limited to 'docs/network.tex')

diff --git a/docs/network.tex b/docs/network.tex
index c14c4db9ed..5516bd9a30 100644
--- a/docs/network.tex
+++ b/docs/network.tex
@@ -22,11 +22,13 @@ of interfaces and add:
 \end{Verbatim}
 
 It is possible to use VLAN tagging on an interface simply by adding the VLAN IDs
-to it, e.g. \texttt{eth0.1}. These can be nested as well. See the switch section for
+to it, e.g. \texttt{eth0.15}. These can be nested as well. See the switch section for
 this.
 
 \begin{Verbatim}
-config inter
+config interface
+    option ifname    "eth0.15"
+    option proto     "none"
 \end{Verbatim}
 
 This sets up a simple static configuration for \texttt{eth0}. \texttt{proto} specifies the
-- 
cgit v1.2.3

