From 716ca530e1c4515d8683c9d5be3d56b301758b66 Mon Sep 17 00:00:00 2001
From: James <>
Date: Wed, 4 Nov 2015 11:49:21 +0000
Subject: trunk-47381

---
 docs/network-scripts.tex | 55 ++++++++++++++++++++++++++++++++++++++++++++++++
 1 file changed, 55 insertions(+)
 create mode 100644 docs/network-scripts.tex

(limited to 'docs/network-scripts.tex')

diff --git a/docs/network-scripts.tex b/docs/network-scripts.tex
new file mode 100644
index 0000000..7ace975
--- /dev/null
+++ b/docs/network-scripts.tex
@@ -0,0 +1,55 @@
+\subsubsection{Using the network scripts}
+
+To be able to access the network functions, you need to include
+the necessary shell scripts by running:
+
+\begin{Verbatim}
+. /lib/functions.sh      # common functions
+include /lib/network     # include /lib/network/*.sh
+scan_interfaces          # read and parse the network config
+\end{Verbatim}
+
+Some protocols, such as PPP might change the configured interface names
+at run time (e.g. \texttt{eth0} => \texttt{ppp0} for PPPoE). That's why you have to run
+\texttt{scan\_interfaces} instead of reading the values from the config directly.
+After running \texttt{scan\_interfaces}, the \texttt{'ifname'} option will always contain
+the effective interface name (which is used for IP traffic) and if the
+physical device name differs from it, it will be stored in the \texttt{'device'}
+option.
+That means that running \texttt{config\_get lan ifname}
+after \texttt{scan\_interfaces} might not return the same result as running it before.
+
+After running \texttt{scan\_interfaces}, the following functions are available:
+
+\begin{itemize}
+    \item{\texttt{find\_config \textit{interface}}} \\
+        looks for a network configuration that includes
+        the specified network interface.
+
+    \item{\texttt{setup\_interface \textit{interface [config] [protocol]}}} \\
+      will set up the specified interface, optionally overriding the network configuration
+      name or the protocol that it uses.
+\end{itemize}
+
+\subsubsection{Writing protocol handlers}
+
+You can add custom protocol handlers (e.g: PPPoE, PPPoA, ATM, PPTP ...)
+by adding shell scripts to \texttt{/lib/network}. They provide the following
+two shell functions:
+
+\begin{Verbatim}
+scan_<protocolname>() {
+    local config="$1"
+    # change the interface names if necessary
+}
+
+setup_interface_<protocolname>() {
+    local interface="$1"
+    local config="$2"
+    # set up the interface
+}
+\end{Verbatim}
+
+\texttt{scan\_\textit{protocolname}} is optional and only necessary if your protocol
+uses a custom device, e.g. a tunnel or a PPP device.
+
-- 
cgit v1.2.3

