From d70e805217edcff9bba4dd2e472325c5006c91df Mon Sep 17 00:00:00 2001
From: Florian Fainelli <florian@openwrt.org>
Date: Sun, 5 Jul 2009 11:17:49 +0000
Subject: [package] configure the IPv6 from /etc/config/network and remove
 6scripts's prefix option to set an IPv6 address on the LAN (#5450)

git-svn-id: svn://svn.openwrt.org/openwrt/trunk@16683 3c298f89-4303-0410-b956-a3cf2f4a3e73
---
 docs/network.tex | 3 ---
 1 file changed, 3 deletions(-)

(limited to 'docs/network.tex')

diff --git a/docs/network.tex b/docs/network.tex
index c7e80c68f1..793a398228 100644
--- a/docs/network.tex
+++ b/docs/network.tex
@@ -169,7 +169,6 @@ config 6tunnel
         option remoteip4        '1.0.0.1'
         option localip4         '1.0.0.2'
         option localip6         '2001::DEAD::BEEF::1'
-        option prefix           '/64'
 \end{Verbatim}
 
 \begin{itemize}
@@ -184,8 +183,6 @@ config 6tunnel
     \item{\texttt{'localip6'}:}
 	IPv6 address to setup on your tunnel side
 	This address is given by the tunnel broker
-    \item{\texttt{'prefix'}:}
-	IPv6 prefix to setup on the LAN.
 \end{itemize}
 
 Using the same package you can also setup an IPv6 bridged connection :
-- 
cgit v1.2.3

